| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
spi_master_BusConfig_struct Struct Reference

`#include <isf_spi_master_types.h>`

Collaboration diagram for spi_master_BusConfig_struct:

## Data Fields
isf_duration_t | timeout
dspi_device_t | device
dspi_master_user_config_t | userConfig

## Detailed Description

Definition at line 20 of file isf_spi_master_types.h.

## Field Documentation

dspi_device_t device

The configuration information.

Definition at line 22 of file isf_spi_master_types.h.

Referenced by spi_master_adapter_configure().

isf_duration_t timeout

The bus timeout value to use.

Definition at line 21 of file isf_spi_master_types.h.

Referenced by spi_master_adapter_acquire_lock(), spi_master_adapter_get_endpoint(), spi_master_adapter_start(), and spi_master_adapter_stop().

dspi_master_user_config_t userConfig

The user configuration information.

Definition at line 23 of file isf_spi_master_types.h.

The documentation for this struct was generated from the following file:

- ISF/ProtocolAdapter/Include/isf_spi_master_types.h

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.