| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

- All
- Variables

- a
- b
- c
- d
- e
- f
- g
- h
- i
- l
- m
- n
- o
- p
- q
- r
- s
- t
- u
- v
- w
- x
- y
- z

Here is a list of all struct and union fields with links to the structures/unions they belong to:

### - d -

- data : Analog_1_DataBuffer_t , App1AppInstance_t , Custom_1_DataBuffer_t
- dataBlockSize : DeviceDescriptor_struct
- dataPoints : fLfiTable_t
- dataReadyEventFlag : SensorInfo_t
- dataTypeSize : SensorInfo_t
- defaultSpeed : i2c_Master_BusConfig_struct
- destBufferSize : ci_protocol_t
- device : i2c_deviceEndpoint_struct , rliAppStatus_t , spi_master_BusConfig_struct
- deviceAddress : rliConfigRegister_t
- deviceHandle : DeviceDescriptor_struct , fxlc95000_DeviceDescriptor_t , mma955x_DeviceDescriptor_t
- deviceSemaphore : DeviceDescriptor_struct , fsl_fusion_DeviceDescriptor_t , fxlc95000_DeviceDescriptor_t , mma955x_DeviceDescriptor_t
- devInfo : isf_dsa_Adapter_st
- distance : mma955x_PedometerData_t
- dummy : Analog_1_device_t

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.