| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
ci_rx_packet_t Struct Reference

This structure holds information to receive a packet of data to the host. CI will fill the structure with the information as it receives it from the ISR and will notify the CI task when a packet has been fully received. More...

`#include <task_ci.h>`

Collaboration diagram for ci_rx_packet_t:

## Data Fields
volatile ci_recv_state_t | rxState
volatile uint8 | mbIndex
| Internal receive state. More...
volatile uint8 | packetSize
| Mailbox index. More...
volatile uint8 * | pRxbuf
| Expected packet size. More...

## Detailed Description

This structure holds information to receive a packet of data to the host. CI will fill the structure with the information as it receives it from the ISR and will notify the CI task when a packet has been fully received.

Definition at line 76 of file task_ci.h.

## Field Documentation

volatile uint8 mbIndex

Internal receive state.

Definition at line 79 of file task_ci.h.

Referenced by process_recv_byte(), and task_ci().

volatile uint8 packetSize

Mailbox index.

Definition at line 80 of file task_ci.h.

Referenced by process_recv_byte().

volatile uint8* pRxbuf

Expected packet size.

Definition at line 81 of file task_ci.h.

Referenced by ci_init(), process_recv_byte(), and task_ci().

volatile ci_recv_state_t rxState

Definition at line 78 of file task_ci.h.

Referenced by process_recv_byte().

The documentation for this struct was generated from the following file:

- ISF/Command_Interpreter/Include/task_ci.h

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.