| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
fxlc95000_SensorSetting_t Struct Reference

`#include <fxlc95000.h>`

Collaboration diagram for fxlc95000_SensorSetting_t:

## Data Fields
uint8 | nSettingsToUse
| 1 = current; 2=given; 3=best possible More...
uint8 | nFifoDepth
| 1 = no FIFO, or another value < SM_MAX_FIFO_DEPTH More...
uint32 | nCurrentReportRate
| Sample period in microseconds. More...
uint8 | nCurrentResolution
| Expected sensor resolution. More...
uint8 | nRange
| Expected sensor dynamic range. More...
uint8 | nMode
| sensor specific mode More...

## Detailed Description

Definition at line 20 of file fxlc95000.h.

## Field Documentation

uint32 nCurrentReportRate

Sample period in microseconds.

Definition at line 24 of file fxlc95000.h.

Referenced by fsl_fxlc95000_Configure().

uint8 nCurrentResolution

Expected sensor resolution.

Definition at line 25 of file fxlc95000.h.

Referenced by fsl_fxlc95000_Configure().

uint8 nFifoDepth

1 = no FIFO, or another value < SM_MAX_FIFO_DEPTH

Definition at line 23 of file fxlc95000.h.

uint8 nMode

sensor specific mode

Definition at line 27 of file fxlc95000.h.

Referenced by fsl_fxlc95000_Configure().

uint8 nRange

Expected sensor dynamic range.

Definition at line 26 of file fxlc95000.h.

Referenced by fsl_fxlc95000_Configure().

uint8 nSettingsToUse

1 = current; 2=given; 3=best possible

Definition at line 22 of file fxlc95000.h.

The documentation for this struct was generated from the following file:

- SensorSpecific/fxlc95000.h

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.