| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- _
- a
- b
- c
- d
- e
- f
- g
- h
- i
- j
- k
- l
- m
- n
- o
- p
- q
- r
- s
- t
- u
- v
- w
- x
- y
- z

Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - m -

- isf_mem_copy() : isf_util.h , isf_util.c
- isf_microTeslas_fixed_32s1i16_t : isf_magnetometer_types.h
- isf_microTeslas_raw_16count_t : isf_magnetometer_types.h
- MAG3100_READ_BUF_SIZE : fxas21002.h , mag3110.h
- MAG3110_1_Adapter : MAG3110_1.h , MAG3110_1.c
- MAG3110_1_DATA_TYPE : MAG3110_1.h
- MAG3110_1_DeviceInfo : MAG3110_1.c , MAG3110_1.h
- MAG3110_1_Sensor_Specific_Config : MAG3110_1.c , MAG3110_1.h
- MAG3110_AC_MASK : mag3110.h
- MAG3110_AC_SHIFT : mag3110.h
- MAG3110_AUTO_MRST_EN_MASK : mag3110.h
- MAG3110_AUTO_MRST_EN_SHIFT : mag3110.h
- mag3110_CheckId() : fsl_mag3110_i2c_3D_mag.c
- MAG3110_CTRL_REG1 : mag3110.h
- MAG3110_CTRL_REG2 : mag3110.h
- MAG3110_DEVICE_ID : mag3110.h
- MAG3110_DIE_TEMP : mag3110.h
- MAG3110_DR_MASK : mag3110.h
- MAG3110_DR_SHIFT : mag3110.h
- MAG3110_DR_STATUS : mag3110.h
- MAG3110_FR_MASK : mag3110.h
- MAG3110_FR_SHIFT : mag3110.h
- MAG3110_GET_FIELD : mag3110.h
- mag3110_GetData() : fsl_mag3110_i2c_3D_mag.c
- MAG3110_IIC_ADDRESS : mag3110.h
- MAG3110_MAG_FIXED_CONVERSION_FACTOR : fsl_mag3110_i2c_3D_mag.c
- MAG3110_MAG_FIXED_CONVERSION_OFFSET : fsl_mag3110_i2c_3D_mag.c
- MAG3110_MAG_FLOAT_CONVERSION_FACTOR : fsl_mag3110_i2c_3D_mag.c
- MAG3110_MAG_FLOAT_CONVERSION_OFFSET : fsl_mag3110_i2c_3D_mag.c
- MAG3110_MAG_RST_MASK : mag3110.h
- MAG3110_MAG_RST_SHIFT : mag3110.h
- MAG3110_NUMBER_AXIS : mag3110.h
- MAG3110_NUMBER_BYTES_AXIS : mag3110.h
- MAG3110_OFF_X_LSB : mag3110.h
- MAG3110_OFF_X_MSB : mag3110.h
- MAG3110_OFF_Y_LSB : mag3110.h
- MAG3110_OFF_Y_MSB : mag3110.h
- MAG3110_OFF_Z_LSB : mag3110.h
- MAG3110_OFF_Z_MSB : mag3110.h
- MAG3110_OS_MASK : mag3110.h
- MAG3110_OS_SHIFT : mag3110.h
- MAG3110_OUT_X_LSB : mag3110.h
- MAG3110_OUT_X_MSB : mag3110.h
- MAG3110_OUT_Y_LSB : mag3110.h
- MAG3110_OUT_Y_MSB : mag3110.h
- MAG3110_OUT_Z_LSB : mag3110.h
- MAG3110_OUT_Z_MSB : mag3110.h
- MAG3110_RAW_MASK : mag3110.h
- MAG3110_RAW_SHIFT : mag3110.h
- mag3110_Reset() : fsl_mag3110_i2c_3D_mag.c
- MAG3110_SET_FIELD : mag3110.h
- mag3110_SetConfig() : fsl_mag3110_i2c_3D_mag.c
- mag3110_SetMode() : fsl_mag3110_i2c_3D_mag.c
- MAG3110_STANDBY_TO_ACTIVE_SAMPLE_WAIT : mag3110.h
- mag3110_status_t : mag3110.h
- mag3110_SupportedDataTypes : fsl_mag3110_i2c_3D_mag.c , fsl_mag3110_i2c_3D_mag.h
- mag3110_SupportedSensorTypes : fsl_mag3110_i2c_3D_mag.c , fsl_mag3110_i2c_3D_mag.h
- MAG3110_SYS_MOD : mag3110.h
- MAG3110_SYSMOD0_MASK : mag3110.h
- MAG3110_SYSMOD0_SHIFT : mag3110.h
- MAG3110_SYSMOD1_MASK : mag3110.h
- MAG3110_SYSMOD1_SHIFT : mag3110.h
- MAG3110_TM_MASK : mag3110.h
- MAG3110_TM_SHIFT : mag3110.h
- mag3110_ValidateConfig() : fsl_mag3110_i2c_3D_mag.c
- MAG3110_WHO_AM_I : mag3110.h
- MAG3110_WHOAMI_VALUE : mag3110.h
- MAG3110_XDR_MASK : mag3110.h
- MAG3110_XDR_SHIFT : mag3110.h
- MAG3110_XOW_MASK : mag3110.h
- MAG3110_XOW_SHIFT : mag3110.h
- MAG3110_YDR_MASK : mag3110.h
- MAG3110_YDR_SHIFT : mag3110.h
- MAG3110_YOW_MASK : mag3110.h
- MAG3110_YOW_SHIFT : mag3110.h
- MAG3110_ZDR_MASK : mag3110.h
- MAG3110_ZDR_SHIFT : mag3110.h
- MAG3110_ZOW_MASK : mag3110.h
- MAG3110_ZOW_SHIFT : mag3110.h
- MAG3110_ZYXDR_MASK : mag3110.h
- MAG3110_ZYXDR_SHIFT : mag3110.h
- MAG3110_ZYXOW_MASK : mag3110.h
- MAG3110_ZYXOW_SHIFT : mag3110.h
- MAG_DATA_READY_EVENT : fsl_fusion_virt_3D_orient.c
- MAG_GET_HAL_X_VALUE : fusion_config.h
- MAG_GET_HAL_Y_VALUE : fusion_config.h
- MAG_HAL_X_INDEX : fusion_config.h
- MAG_HAL_Y_INDEX : fusion_config.h
- MAG_HAL_Z_INDEX : fusion_config.h
- MAG_OVERSAMPLE_RATIO : fusion_config.h
- MAGBUFFSIZEX : magnetic_config.h
- MAGBUFFSIZEY : magnetic_config.h
- MAGCAL_EVENT_FLAG : fsl_fusion_virt_3D_orient.c
- MagCal_Run() : fusion_exec.c , fusion_exec.h
- main() : main.c
- MainTask_Init() : MainTask.c
- MainTask_PEX_RTOS_COMPONENTS_INIT : MainTask.h
- MAINTASK_TASK : mqx_ksdk.h
- MAINTASK_TASK_NAME : MainTask.h
- MAINTASK_TASK_PRIORITY : MainTask.h
- MAINTASK_TASK_STACK_SIZE : MainTask.h
- MAX_ACCEL_FULL_SCALE_RANGE : fsl_fxls8952_i2c_3D_accel.c , fsl_fxos8700_i2cspi_6D_AccMag.c
- MAX_ADC_CHANNELS : fsl_Sensor_Analog_1_Functions.h
- MAX_BM_CALLBACKS : isf_bm.h
- MAX_BM_PERIOD_USEC : isf_bm.h
- MAX_BUF_SIZE : fsl_fxas21002_i2cspi_3D_gyro.c
- MAX_DATA_READ_SIZE : fsl_fxas21002_i2cspi_3D_gyro.c , fsl_fxos8700_i2cspi_6D_AccMag.c
- MAX_EVENTS : isf_eventhandler.h
- MAX_FXAS21002_DM_BYTES : fsl_fxas21002_i2cspi_3D_gyro.c
- MAX_FXLS8952_DM_BYTES : fsl_fxls8952_i2c_3D_accel.c
- MAX_FXOS8700_DM_BYTES : fsl_fxos8700_i2cspi_6D_AccMag.c
- MAX_GYRO_FULL_SCALE_RANGE : fsl_fxas21002_i2cspi_3D_gyro.c
- MAX_ISF_APPLICATIONS : isf.h
- MAX_ISF_COMMIT_ID_SIZE : isf.h
- MAX_NUM_AXES : fsl_fxls8952_i2c_3D_accel.c , fsl_fxos8700_i2cspi_6D_AccMag.c
- MAX_NUM_MAILBOXES : ci_protocol_mbox.h
- MAX_NUM_OUT_BUFFER : ci_protocol_mbox.h
- MAX_SUPPORTED : Analog_1.h
- MAXBFITUT : magnetic_config.h
- MAXMEASUREMENTS : magnetic_config.h
- MB_APP_RESP_DATA_START : ci_protocol_mbox.h
- MB_APP_RESP_SIZE : ci_protocol_mbox.h
- MB_HOST_APP_ID : ci_protocol_mbox.h
- MB_HOST_CMD : ci_protocol_mbox.h
- MB_HOST_CMD_SIZE : ci_protocol_mbox.h
- MB_HOST_COUNT : ci_protocol_mbox.h
- MB_HOST_COUNT_EXT : ci_protocol_mbox.h
- MB_HOST_OFFSET : ci_protocol_mbox.h
- MB_HOST_OFFSET_EXT : ci_protocol_mbox.h
- MB_HOST_WR_DATA_START : ci_protocol_mbox.h
- MB_RESP_APP_ID : ci_protocol_mbox.h
- MB_RESP_BYTES_XFER : ci_protocol_mbox.h
- MB_RESP_COUNT : ci_protocol_mbox.h
- MB_RESP_INDEX_APP_ID : ci_protocol_mbox.h
- MB_RESP_INDEX_BYTES_XFER : ci_protocol_mbox.h
- MB_RESP_INDEX_COUNT : ci_protocol_mbox.h
- MB_RESP_INDEX_STATUS_CC : ci_protocol_mbox.h
- MB_RESP_STATUS_CC : ci_protocol_mbox.h
- MBOX_APP_DATA : ci_protocol_mbox.c
- MBOX_CRC_BYTE_SIZE : ci_protocol_mbox.h
- MBoxQRDataXYZ : MMA955x_1.c , MMA955x_2.c
- MESHDELTACOUNTS : magnetic_config.h
- MIN_BM_PERIOD_USEC : isf_bm.h
- MINBFITUT : magnetic_config.h
- MINMEASUREMENTS10CAL : magnetic_config.h
- MINMEASUREMENTS4CAL : magnetic_config.h
- MINMEASUREMENTS7CAL : magnetic_config.h
- MK64F : build.h
- MMA7330L : Analog_1.h
- MMA7340L : Analog_1.h
- MMA7360L : Analog_1.h
- MMA8491Q_1_Adapter : MMA8491Q_1.c , MMA8491Q_1.h
- MMA8491Q_1_DATA_TYPE : MMA8491Q_1.h
- MMA8491Q_1_DeviceInfo : MMA8491Q_1.c , MMA8491Q_1.h
- MMA8491Q_1_Sensor_Specific_Config : MMA8491Q_1.c , MMA8491Q_1.h
- MMA8491Q_ACCEL_FIXED_CONVERSION_FACTOR : fsl_mma8491q_i2c_3D_accel.c
- MMA8491Q_ACCEL_FLOAT_CONVERSION_FACTOR : fsl_mma8491q_i2c_3D_accel.c
- MMA8491Q_ACTIVE : mma8491q.h
- mma8491q_CheckId() : fsl_mma8491q_i2c_3D_accel.c
- MMA8491Q_DATA_FAIL : mma8491q.h
- MMA8491Q_DATA_SUCCESS : mma8491q.h
- mma8491q_getAccelData() : fsl_mma8491q_i2c_3D_accel.c
- mma8491q_mode : fsl_mma8491q_i2c_3D_accel.c
- mma8491q_mode_t : mma8491q.h
- MMA8491Q_OUT_X_LSB : mma8491q.h
- MMA8491Q_OUT_X_MSB : mma8491q.h
- MMA8491Q_OUT_Y_lSB : mma8491q.h
- MMA8491Q_OUT_Y_MSB : mma8491q.h
- MMA8491Q_OUT_Z_LSB : mma8491q.h
- MMA8491Q_OUT_Z_MSB : mma8491q.h
- MMA8491Q_SHUTDOWN : mma8491q.h
- MMA8491Q_STANDBY : mma8491q.h
- MMA8491Q_STATUS_00 : mma8491q.h
- mma8491q_SupportedDataTypes : fsl_mma8491q_i2c_3D_accel.c , fsl_mma8491q_i2c_3D_accel.h
- mma8491q_SupportedSensorTypes : fsl_mma8491q_i2c_3D_accel.c , fsl_mma8491q_i2c_3D_accel.h
- MMA8491Q_WHOAMI_VALUE : mma8491q.h
- mma8491q_xyz_format : fsl_mma8491q_i2c_3D_accel.c
- MMA865x_1_Adapter : MMA865x_1.c , MMA865x_1.h
- MMA865x_1_DATA_TYPE : MMA865x_1.h
- MMA865x_1_DeviceInfo : MMA865x_1.c , MMA865x_1.h
- MMA865x_1_Sensor_Specific_Config : MMA865x_1.c , MMA865x_1.h
- MMA865x_ACTIVE : mma865x.h
- MMA865x_ACTIVE_MASK : mma865x.h
- MMA865x_ASLP_COUNT : mma865x.h
- MMA865x_ASLP_RATE0_MASK : mma865x.h
- MMA865x_ASLP_RATE1_MASK : mma865x.h
- MMA865x_ASLP_RATE_12_5HZ : mma865x.h
- MMA865x_ASLP_RATE_160MS : mma865x.h
- MMA865x_ASLP_RATE_1_56HZ : mma865x.h
- MMA865x_ASLP_RATE_20MS : mma865x.h
- MMA865x_ASLP_RATE_50HZ : mma865x.h
- MMA865x_ASLP_RATE_640MS : mma865x.h
- MMA865x_ASLP_RATE_6_25HZ : mma865x.h
- MMA865x_ASLP_RATE_80MS : mma865x.h
- MMA865x_ASLP_RATE_MASK : mma865x.h
- MMA865x_ASLP_RATE_SHIFT : mma865x.h
- MMA865x_AXX_MASK : mma865x.h
- MMA865x_AXY_MASK : mma865x.h
- MMA865x_AXZ_MASK : mma865x.h
- MMA865x_BAFRO_MASK : mma865x.h
- MMA865x_BAFRO_SHIFT : mma865x.h
- MMA865x_BKFR0_MASK : mma865x.h
- MMA865x_BKFR1_MASK : mma865x.h
- MMA865x_BKFR_MASK : mma865x.h
- MMA865x_BKFR_SHIFT : mma865x.h
- mma865x_CheckId() : fsl_mma865x_i2c_3D_accel.c
- MMA865x_CTRL_REG1 : mma865x.h
- MMA865x_CTRL_REG2 : mma865x.h
- MMA865x_CTRL_REG3 : mma865x.h
- MMA865x_CTRL_REG4 : mma865x.h
- MMA865x_CTRL_REG5 : mma865x.h
- MMA865x_DATA_OVERWRITE : mma865x.h
- MMA865x_DATA_RATE_100HZ : mma865x.h
- MMA865x_DATA_RATE_10MS : mma865x.h
- MMA865x_DATA_RATE_1250US : mma865x.h
- MMA865x_DATA_RATE_12_5HZ : mma865x.h
- MMA865x_DATA_RATE_160MS : mma865x.h
- MMA865x_DATA_RATE_1_56HZ : mma865x.h
- MMA865x_DATA_RATE_200HZ : mma865x.h
- MMA865x_DATA_RATE_20MS : mma865x.h
- MMA865x_DATA_RATE_2500US : mma865x.h
- MMA865x_DATA_RATE_400HZ : mma865x.h
- MMA865x_DATA_RATE_50HZ : mma865x.h
- MMA865x_DATA_RATE_5MS : mma865x.h
- MMA865x_DATA_RATE_640MS : mma865x.h
- MMA865x_DATA_RATE_6_25HZ : mma865x.h
- MMA865x_DATA_RATE_800HZ : mma865x.h
- MMA865x_DATA_RATE_80MS : mma865x.h
- MMA865x_DBCNTM_MASK : mma865x.h
- MMA865x_DBCNTM_SHIFT : mma865x.h
- MMA865x_DPA_MASK : mma865x.h
- MMA865x_DPA_SHIFT : mma865x.h
- MMA865x_DPE_MASK : mma865x.h
- MMA865x_DR0_MASK : mma865x.h
- MMA865x_DR1_MASK : mma865x.h
- MMA865x_DR2_MASK : mma865x.h
- MMA865x_DR_MASK : mma865x.h
- MMA865x_DR_SHIFT : mma865x.h
- MMA865x_EA_MASK : mma865x.h
- MMA865x_ELE_MASK : mma865x.h
- MMA865x_ELE_SHIFT : mma865x.h
- MMA865x_ERROR : mma865x.h
- MMA865x_F_CNT0_MASK : mma865x.h
- MMA865x_F_CNT1_MASK : mma865x.h
- MMA865x_F_CNT2_MASK : mma865x.h
- MMA865x_F_CNT3_MASK : mma865x.h
- MMA865x_F_CNT4_MASK : mma865x.h
- MMA865x_F_CNT5_MASK : mma865x.h
- MMA865x_F_CNT_MASK : mma865x.h
- MMA865x_F_MODE0_MASK : mma865x.h
- MMA865x_F_MODE1_MASK : mma865x.h
- MMA865x_F_MODE_CIRCULAR : mma865x.h
- MMA865x_F_MODE_DISABLED : mma865x.h
- MMA865x_F_MODE_FILL : mma865x.h
- MMA865x_F_MODE_MASK : mma865x.h
- MMA865x_F_MODE_TRIGGER : mma865x.h
- MMA865x_F_OVF_MASK : mma865x.h
- MMA865x_F_SETUP : mma865x.h
- MMA865x_F_WMRK0_MASK : mma865x.h
- MMA865x_F_WMRK1_MASK : mma865x.h
- MMA865x_F_WMRK2_MASK : mma865x.h
- MMA865x_F_WMRK3_MASK : mma865x.h
- MMA865x_F_WMRK4_MASK : mma865x.h
- MMA865x_F_WMRK5_MASK : mma865x.h
- MMA865x_F_WMRK_FLAG_MASK : mma865x.h
- MMA865x_F_WMRK_MASK : mma865x.h
- MMA865x_FF_MT_CFG : mma865x.h
- MMA865x_FF_MT_COUNT : mma865x.h
- MMA865x_FF_MT_SRC : mma865x.h
- MMA865x_FF_MT_THS : mma865x.h
- MMA865x_FFMT_OUTPUT_EN : mma865x.h
- MMA865x_FGERR_MASK : mma865x.h
- MMA865x_FGT_0_MASK : mma865x.h
- MMA865x_FGT_1_MASK : mma865x.h
- MMA865x_FGT_2_MASK : mma865x.h
- MMA865x_FGT_3_MASK : mma865x.h
- MMA865x_FGT_4_MASK : mma865x.h
- MMA865x_FGT_MASK : mma865x.h
- MMA865x_FIFO_GATE_MASK : mma865x.h
- MMA865x_FIFO_GATE_SHIFT : mma865x.h
- MMA865x_FREAD_MASK : mma865x.h
- MMA865x_FREAD_SHIFT : mma865x.h
- MMA865x_FS0_MASK : mma865x.h
- MMA865x_FS1_MASK : mma865x.h
- MMA865x_FS_MASK : mma865x.h
- MMA865x_FS_SHIFT : mma865x.h
- MMA865x_FULL_SCALE_2G : mma865x.h
- MMA865x_FULL_SCALE_4G : mma865x.h
- MMA865x_FULL_SCALE_8G : mma865x.h
- MMA865x_GET_FIELD : mma865x.h
- mma865x_GetConfig() : fsl_mma865x_i2c_3D_accel.c
- mma865x_GetData() : fsl_mma865x_i2c_3D_accel.c
- MMA865x_HP_FILTER_CUTOFF : mma865x.h
- MMA865x_HPF_BYP_MASK : mma865x.h
- MMA865x_HPF_BYP_SHIFT : mma865x.h
- MMA865x_HPF_OUT_MASK : mma865x.h
- MMA865x_HPF_OUT_SHIFT : mma865x.h
- MMA865x_HYS0_MASK : mma865x.h
- MMA865x_HYS1_MASK : mma865x.h
- MMA865x_HYS2_MASK : mma865x.h
- MMA865x_HYS_MASK : mma865x.h
- MMA865x_HYS_SHIFT : mma865x.h
- MMA865x_INT_CFG_ASLP_MASK : mma865x.h
- MMA865x_INT_CFG_ASLP_SHIFT : mma865x.h
- MMA865x_INT_CFG_DRDY_MASK : mma865x.h
- MMA865x_INT_CFG_DRDY_SHIFT : mma865x.h
- MMA865x_INT_CFG_FF_MT_MASK : mma865x.h
- MMA865x_INT_CFG_FF_MT_SHIFT : mma865x.h
- MMA865x_INT_CFG_FIFO_MASK : mma865x.h
- MMA865x_INT_CFG_FIFO_SHIFT : mma865x.h
- MMA865x_INT_CFG_LNDPRT_MASK : mma865x.h
- MMA865x_INT_CFG_LNDPRT_SHIFT : mma865x.h
- MMA865x_INT_CFG_PULSE_MASK : mma865x.h
- MMA865x_INT_CFG_PULSE_SHIFT : mma865x.h
- MMA865x_INT_CFG_TRANS_MASK : mma865x.h
- MMA865x_INT_CFG_TRANS_SHIFT : mma865x.h
- MMA865x_INT_EN_ASLP_MASK : mma865x.h
- MMA865x_INT_EN_ASLP_SHIFT : mma865x.h
- MMA865x_INT_EN_DRDY_MASK : mma865x.h
- MMA865x_INT_EN_DRDY_SHIFT : mma865x.h
- MMA865x_INT_EN_FF_MT_MASK : mma865x.h
- MMA865x_INT_EN_FF_MT_SHIFT : mma865x.h
- MMA865x_INT_EN_FIFO_MASK : mma865x.h
- MMA865x_INT_EN_FIFO_SHIFT : mma865x.h
- MMA865x_INT_EN_LNDPRT_MASK : mma865x.h
- MMA865x_INT_EN_LNDPRT_SHIFT : mma865x.h
- MMA865x_INT_EN_PULSE_MASK : mma865x.h
- MMA865x_INT_EN_PULSE_SHIFT : mma865x.h
- MMA865x_INT_EN_TRANS_MASK : mma865x.h
- MMA865x_INT_EN_TRANS_SHIFT : mma865x.h
- MMA865x_INT_SOURCE : mma865x.h
- MMA865x_IPOL_MASK : mma865x.h
- MMA865x_IPOL_SHIFT : mma865x.h
- MMA865x_LAPO0_MASK : mma865x.h
- MMA865x_LAPO1_MASK : mma865x.h
- MMA865x_LAPO_MASK : mma865x.h
- MMA865x_LAPO_SHIFT : mma865x.h
- MMA865x_LNOISE_MASK : mma865x.h
- MMA865x_LO_MASK : mma865x.h
- MMA865x_LO_SHIFT : mma865x.h
- MMA865x_MMA865xQ : mma865x.h
- MMA865x_MOD_HIGH_RES : mma865x.h
- MMA865x_MOD_LOW_NOISE : mma865x.h
- MMA865x_MOD_LOW_POWER : mma865x.h
- MMA865x_MOD_NORMAL : mma865x.h
- MMA865x_MODS0_MASK : mma865x.h
- MMA865x_MODS1_MASK : mma865x.h
- MMA865x_MODS_MASK : mma865x.h
- MMA865x_MODS_SHIFT : mma865x.h
- MMA865x_NEWLP_MASK : mma865x.h
- MMA865x_OAE_MASK : mma865x.h
- MMA865x_OAE_SHIFT : mma865x.h
- MMA865x_OFF_X : mma865x.h
- MMA865x_OFF_Y : mma865x.h
- MMA865x_OFF_Z : mma865x.h
- MMA865x_OUT_X_LSB : mma865x.h
- MMA865x_OUT_X_MSB : mma865x.h
- MMA865x_OUT_Y_lSB : mma865x.h
- MMA865x_OUT_Y_MSB : mma865x.h
- MMA865x_OUT_Z_LSB : mma865x.h
- MMA865x_OUT_Z_MSB : mma865x.h
- MMA865x_P_L_THS0_MASK : mma865x.h
- MMA865x_P_L_THS1_MASK : mma865x.h
- MMA865x_P_L_THS2_MASK : mma865x.h
- MMA865x_P_L_THS3_MASK : mma865x.h
- MMA865x_P_L_THS4_MASK : mma865x.h
- MMA865x_P_L_THS_MASK : mma865x.h
- MMA865x_P_L_THS_SHIFT : mma865x.h
- MMA865x_PEA_MASK : mma865x.h
- MMA865x_PELE_MASK : mma865x.h
- MMA865x_PELE_SHIFT : mma865x.h
- MMA865x_PL_BF_ZCOMP : mma865x.h
- MMA865x_PL_CFG : mma865x.h
- MMA865x_PL_COUNT : mma865x.h
- MMA865x_PL_EN_MASK : mma865x.h
- MMA865x_PL_EN_SHIFT : mma865x.h
- MMA865x_PL_OUTPUT_EN : mma865x.h
- MMA865x_PL_P_L_THS : mma865x.h
- MMA865x_PL_STATUS : mma865x.h
- MMA865x_POLX_MASK : mma865x.h
- MMA865x_POLY_MASK : mma865x.h
- MMA865x_POLZ_MASK : mma865x.h
- MMA865x_PP_OD_MASK : mma865x.h
- MMA865x_PP_OD_SHIFT : mma865x.h
- MMA865x_PTHS_MASK : mma865x.h
- MMA865x_PTHS_SHIFT : mma865x.h
- MMA865x_PULSE_CFG : mma865x.h
- MMA865x_PULSE_HPF_BYP_MASK : mma865x.h
- MMA865x_PULSE_HPF_BYP_SHIFT : mma865x.h
- MMA865x_PULSE_LPF_EN_MASK : mma865x.h
- MMA865x_PULSE_LPF_EN_SHIFT : mma865x.h
- MMA865x_PULSE_LTCY : mma865x.h
- MMA865x_PULSE_OUTPUT_EN : mma865x.h
- MMA865x_PULSE_SRC : mma865x.h
- MMA865x_PULSE_THSX : mma865x.h
- MMA865x_PULSE_THSY : mma865x.h
- MMA865x_PULSE_THSZ : mma865x.h
- MMA865x_PULSE_TMLT : mma865x.h
- MMA865x_PULSE_WIND : mma865x.h
- mma865x_Reset() : fsl_mma865x_i2c_3D_accel.c
- MMA865x_RST_MASK : mma865x.h
- MMA865x_RST_SHIFT : mma865x.h
- MMA865x_RSVD_0 : mma865x.h
- MMA865x_RSVD_1 : mma865x.h
- MMA865x_RSVD_2 : mma865x.h
- MMA865x_RSVD_3 : mma865x.h
- MMA865x_RSVD_4 : mma865x.h
- MMA865x_RSVD_5 : mma865x.h
- MMA865x_SEL0_MASK : mma865x.h
- MMA865x_SEL1_MASK : mma865x.h
- MMA865x_SEL_MASK : mma865x.h
- MMA865x_SEL_SHIFT : mma865x.h
- MMA865x_SET_FIELD : mma865x.h
- mma865x_SetConfig() : fsl_mma865x_i2c_3D_accel.c
- mma865x_SetMode() : fsl_mma865x_i2c_3D_accel.c
- MMA865x_SLPE_MASK : mma865x.h
- MMA865x_SLPE_SHIFT : mma865x.h
- MMA865x_SMOD_HIGH_RES : mma865x.h
- MMA865x_SMOD_LOW_NOISE : mma865x.h
- MMA865x_SMOD_LOW_POWER : mma865x.h
- MMA865x_SMOD_NORMAL : mma865x.h
- MMA865x_SMODS0_MASK : mma865x.h
- MMA865x_SMODS1_MASK : mma865x.h
- MMA865x_SMODS_MASK : mma865x.h
- MMA865x_SMODS_SHIFT : mma865x.h
- MMA865x_SRC_ASLP_MASK : mma865x.h
- MMA865x_SRC_DRDY_MASK : mma865x.h
- MMA865x_SRC_FF_MT_MASK : mma865x.h
- MMA865x_SRC_FIFO_MASK : mma865x.h
- MMA865x_SRC_LNDPRT_MASK : mma865x.h
- MMA865x_SRC_PULSE_MASK : mma865x.h
- MMA865x_SRC_TRANS_MASK : mma865x.h
- MMA865x_ST_MASK : mma865x.h
- MMA865x_ST_SHIFT : mma865x.h
- MMA865x_STANDBY : mma865x.h
- MMA865x_STATUS_00 : mma865x.h
- mma865x_status_t : fsl_mma865x_i2c_3D_accel.c
- MMA865x_SUCCESS : mma865x.h
- mma865x_SupportedDataTypes : fsl_mma865x_i2c_3D_accel.c , fsl_mma865x_i2c_3D_accel.h
- mma865x_SupportedSensorTypes : fsl_mma865x_i2c_3D_accel.c , fsl_mma865x_i2c_3D_accel.h
- MMA865x_SYSMOD : mma865x.h
- MMA865x_SYSMOD_MASK : mma865x.h
- MMA865x_SYSMOD_SLEEP : mma865x.h
- MMA865x_SYSMOD_STANDBY : mma865x.h
- MMA865x_SYSMOD_WAKE : mma865x.h
- MMA865x_TEA_MASK : mma865x.h
- MMA865x_TELE_MASK : mma865x.h
- MMA865x_TELE_SHIFT : mma865x.h
- MMA865x_THS0_MASK : mma865x.h
- MMA865x_THS2_MASK : mma865x.h
- MMA865x_THS3_MASK : mma865x.h
- MMA865x_THS4_MASK : mma865x.h
- MMA865x_THS5_MASK : mma865x.h
- MMA865x_THS6_MASK : mma865x.h
- MMA865x_THS_MASK : mma865x.h
- MMA865x_THS_SHIFT : mma865x.h
- MMA865x_TRANS_OUTPUT_EN : mma865x.h
- MMA865x_TRANSIENT_CFG : mma865x.h
- MMA865x_TRANSIENT_COUNT : mma865x.h
- MMA865x_TRANSIENT_SRC : mma865x.h
- MMA865x_TRANSIENT_THS : mma865x.h
- MMA865x_TRIG_CFG : mma865x.h
- MMA865x_TRIG_FF_MT_MASK : mma865x.h
- MMA865x_TRIG_LNDPRT_MASK : mma865x.h
- MMA865x_TRIG_PULSE_MASK : mma865x.h
- MMA865x_TRIG_TRANS_MASK : mma865x.h
- MMA865x_TXS1_MASK : mma865x.h
- mma865x_ValidateConfig() : fsl_mma865x_i2c_3D_accel.c
- MMA865x_WAKE_FF_MT_MASK : mma865x.h
- MMA865x_WAKE_FF_MT_SHIFT : mma865x.h
- MMA865x_WAKE_LNDPRT_MASK : mma865x.h
- MMA865x_WAKE_LNDPRT_SHIFT : mma865x.h
- MMA865x_WAKE_PULSE_MASK : mma865x.h
- MMA865x_WAKE_PULSE_SHIFT : mma865x.h
- MMA865x_WAKE_TRANS_MASK : mma865x.h
- MMA865x_WAKE_TRANS_SHIFT : mma865x.h
- MMA865x_WHO_AM_I : mma865x.h
- MMA865x_WHOAMI_VALUE_8652 : mma865x.h
- MMA865x_WHOAMI_VALUE_8653 : mma865x.h
- MMA865x_X_TRANS_POL_MASK : mma865x.h
- MMA865x_XDPEFE_MASK : mma865x.h
- MMA865x_XDPEFE_SHIFT : mma865x.h
- MMA865x_XDR_MASK : mma865x.h
- MMA865x_XEFE_MASK : mma865x.h
- MMA865x_XEFE_SHIFT : mma865x.h
- MMA865x_XHE_MASK : mma865x.h
- MMA865x_XHP_MASK : mma865x.h
- MMA865x_XOW_MASK : mma865x.h
- MMA865x_XSPEFE_MASK : mma865x.h
- MMA865x_XSPEFE_SHIFT : mma865x.h
- MMA865x_XTEFE_MASK : mma865x.h
- MMA865x_XTEFE_SHIFT : mma865x.h
- MMA865x_XTRANSE_MASK : mma865x.h
- MMA865x_XYZ_DATA_CFG : mma865x.h
- MMA865x_Y_TRANS_POL_MASK : mma865x.h
- MMA865x_YDPEFE_MASK : mma865x.h
- MMA865x_YDPEFE_SHIFT : mma865x.h
- MMA865x_YDR_MASK : mma865x.h
- MMA865x_YEFE_MASK : mma865x.h
- MMA865x_YEFE_SHIFT : mma865x.h
- MMA865x_YHE_MASK : mma865x.h
- MMA865x_YHP_MASK : mma865x.h
- MMA865x_YOW_MASK : mma865x.h
- MMA865x_YSPEFE_MASK : mma865x.h
- MMA865x_YSPEFE_SHIFT : mma865x.h
- MMA865x_YTEFE_MASK : mma865x.h
- MMA865x_YTEFE_SHIFT : mma865x.h
- MMA865x_YTRANSE_MASK : mma865x.h
- MMA865x_Z_TRANS_POL_MASK : mma865x.h
- MMA865x_ZDPEFE_MASK : mma865x.h
- MMA865x_ZDPEFE_SHIFT : mma865x.h
- MMA865x_ZDR_MASK : mma865x.h
- MMA865x_ZEFE_MASK : mma865x.h
- MMA865x_ZEFE_SHIFT : mma865x.h
- MMA865x_ZHE_MASK : mma865x.h
- MMA865x_ZHP_MASK : mma865x.h
- MMA865x_ZLOCK0_MASK : mma865x.h
- MMA865x_ZLOCK1_MASK : mma865x.h
- MMA865x_ZLOCK2_MASK : mma865x.h
- MMA865x_ZLOCK_MASK : mma865x.h
- MMA865x_ZLOCK_SHIFT : mma865x.h
- MMA865x_ZOW_MASK : mma865x.h
- MMA865x_ZSPEFE_MASK : mma865x.h
- MMA865x_ZSPEFE_SHIFT : mma865x.h
- MMA865x_ZTEFE_MASK : mma865x.h
- MMA865x_ZTEFE_SHIFT : mma865x.h
- MMA865x_ZTRANSE_MASK : mma865x.h
- MMA865x_ZYXDR_MASK : mma865x.h
- MMA865x_ZYXDR_SHIFT : mma865x.h
- MMA865x_ZYXOW_MASK : mma865x.h
- MMA865x_ZYXOW_SHIFT : mma865x.h
- mma865xAccelConvTable : fsl_mma865x_i2c_3D_accel.c
- MMA955x_1_ACC_FLOAT_CONVERSION_FACTOR_2g : MMA955x_1.h
- MMA955x_1_ACC_FLOAT_CONVERSION_FACTOR_4g : MMA955x_1.h
- MMA955x_1_ACC_FLOAT_CONVERSION_FACTOR_8g : MMA955x_1.h
- MMA955x_1_Adapter : MMA955x_1.c , MMA955x_1.h
- MMA955x_1_CONFIG_REGISTER_READ_OFFSET : MMA955x_1.h
- MMA955x_1_CONFIG_REGISTER_SIZE : MMA955x_1.h
- MMA955x_1_ConfigRegisterBuffer : MMA955x_1.c
- MMA955x_1_DATA_TYPE : MMA955x_1.h
- MMA955x_1_DeviceInfo : MMA955x_1.h , MMA955x_1.c
- MMA955x_1_SAMPLE_OFFSET : MMA955x_1.h
- MMA955x_1_SAMPLE_SIZE : MMA955x_1.h
- MMA955x_1_Sensor_Specific_Config : MMA955x_1.c , MMA955x_1.h
- MMA955x_2_ACC_FLOAT_CONVERSION_FACTOR_2g : MMA955x_2.h
- MMA955x_2_ACC_FLOAT_CONVERSION_FACTOR_4g : MMA955x_2.h
- MMA955x_2_ACC_FLOAT_CONVERSION_FACTOR_8g : MMA955x_2.h
- MMA955x_2_Adapter : MMA955x_2.h , MMA955x_2.c
- MMA955x_2_CONFIG_REGISTER_READ_OFFSET : MMA955x_2.h
- MMA955x_2_CONFIG_REGISTER_SIZE : MMA955x_2.h
- MMA955x_2_ConfigRegisterBuffer : MMA955x_2.c
- MMA955x_2_DATA_TYPE : MMA955x_2.h
- MMA955x_2_DeviceInfo : MMA955x_2.c , MMA955x_2.h
- MMA955x_2_SAMPLE_OFFSET : MMA955x_2.h
- MMA955x_2_SAMPLE_SIZE : MMA955x_2.h
- MMA955x_2_Sensor_Specific_Config : MMA955x_2.h , MMA955x_2.c
- MMA955x_ConfigureSequence : MMA955x_2.c , MMA955x_1.c
- mma955x_GetConfig() : fsl_mma955x_i2cspi_pedo.c
- mma955x_GetData() : fsl_mma955x_i2cspi_pedo.c
- mma955x_GetPedometerData() : fsl_mma955x_i2cspi_pedo.c
- MMA955x_InitializeSequence : MMA955x_1.c , MMA955x_2.c
- mma955x_read() : fsl_mma955x_i2cspi_pedo.c
- MMA955x_ReadConfigurationSequence : MMA955x_2.c , MMA955x_1.c
- MMA955x_ReadPeadometerDataSequence : MMA955x_2.c , MMA955x_1.c
- mma955x_send() : fsl_mma955x_i2cspi_pedo.c
- MMA955x_ShutdownDataSequence : MMA955x_1.c , MMA955x_2.c
- MMA955x_StartDataSequence : MMA955x_1.c , MMA955x_2.c
- mma955x_status_t : mma955x.h
- MMA955x_StopDataSequence : MMA955x_1.c , MMA955x_2.c
- mma955x_SupportedDataTypes : fsl_mma955x_i2cspi_pedo.h , fsl_mma955x_i2cspi_pedo.c
- mma955x_SupportedSensorTypes : fsl_mma955x_i2cspi_pedo.h , fsl_mma955x_i2cspi_pedo.c
- mma955x_ValidateConfig() : fsl_mma955x_i2cspi_pedo.c
- mma955x_waitForCoCo() : fsl_mma955x_i2cspi_pedo.c
- mma955x_WriteConfig() : fsl_mma955x_i2cspi_pedo.c
- MMA955x_WriteConfigurationSequence : MMA955x_2.c , MMA955x_1.c
- mma955xSetSamplingRate() : MMA955x_1.c , fsl_mma955x_i2cspi_pedo.c , MMA955x_2.c
- MODE_OFFSET : fxlc95000.h
- MPL3115_1_Adapter : MPL3115_1.c , MPL3115_1.h
- MPL3115_1_DATA_TYPE : MPL3115_1.h
- MPL3115_1_DeviceInfo : MPL3115_1.h , MPL3115_1.c
- MPL3115_1_Sensor_Specific_Config : MPL3115_1.c , MPL3115_1.h
- MPL3115_ACTIVE_MASK : mpl3115.h
- MPL3115_ALARM_SEL_MASK : mpl3115.h
- MPL3115_ALARM_SEL_SHIFT : mpl3115.h
- MPL3115_ALT_FIXED_CONVERSION_FACTOR : fsl_mpl3115_i2c_1D_press.c
- MPL3115_ALT_FIXED_CONVERSION_OFFSET : fsl_mpl3115_i2c_1D_press.c
- MPL3115_ALT_FLOAT_CONVERSION_FACTOR : fsl_mpl3115_i2c_1D_press.c
- MPL3115_ALT_FLOAT_CONVERSION_OFFSET : fsl_mpl3115_i2c_1D_press.c
- MPL3115_ALT_MASK : mpl3115.h
- MPL3115_ALT_SHIFT : mpl3115.h
- MPL3115_BAR_IN_LSB : mpl3115.h
- MPL3115_BAR_IN_MSB : mpl3115.h
- mpl3115_CheckId() : fsl_mpl3115_i2c_1D_press.c
- MPL3115_CTRL_REG1 : mpl3115.h
- MPL3115_CTRL_REG2 : mpl3115.h
- MPL3115_CTRL_REG3 : mpl3115.h
- MPL3115_CTRL_REG4 : mpl3115.h
- MPL3115_CTRL_REG5 : mpl3115.h
- mpl3115_DataReady() : fsl_mpl3115_i2c_1D_press.c
- MPL3115_DREM_MASK : mpl3115.h
- MPL3115_DREM_SHIFT : mpl3115.h
- MPL3115_ERROR : mpl3115.h
- MPL3115_F_DATA : mpl3115.h
- MPL3115_F_SETUP : mpl3115.h
- MPL3115_F_STATUS : mpl3115.h
- MPL3115_GET_FIELD : mpl3115.h
- mpl3115_GetData() : fsl_mpl3115_i2c_1D_press.c
- MPL3115_IIC_ADDRESS : mpl3115.h
- MPL3115_INT_CFG_DRDY_MASK : mpl3115.h
- MPL3115_INT_CFG_DRDY_SHIFT : mpl3115.h
- MPL3115_INT_CFG_PCHG_MASK : mpl3115.h
- MPL3115_INT_CFG_PCHG_SHIFT : mpl3115.h
- MPL3115_INT_CFG_PTH_MASK : mpl3115.h
- MPL3115_INT_CFG_PTH_SHIFT : mpl3115.h
- MPL3115_INT_CFG_PW_MASK : mpl3115.h
- MPL3115_INT_CFG_PW_SHIFT : mpl3115.h
- MPL3115_INT_CFG_TCHG_MASK : mpl3115.h
- MPL3115_INT_CFG_TCHG_SHIFT : mpl3115.h
- MPL3115_INT_CFG_TTH_MASK : mpl3115.h
- MPL3115_INT_CFG_TTH_SHIFT : mpl3115.h
- MPL3115_INT_CFG_TW_MASK : mpl3115.h
- MPL3115_INT_CFG_TW_SHIFT : mpl3115.h
- MPL3115_INT_EN_DRDY_MASK : mpl3115.h
- MPL3115_INT_EN_DRDY_SHIFT : mpl3115.h
- MPL3115_INT_EN_PCHG_MASK : mpl3115.h
- MPL3115_INT_EN_PCHG_SHIFT : mpl3115.h
- MPL3115_INT_EN_PTH_MASK : mpl3115.h
- MPL3115_INT_EN_PTH_SHIFT : mpl3115.h
- MPL3115_INT_EN_PW_MASK : mpl3115.h
- MPL3115_INT_EN_PW_SHIFT : mpl3115.h
- MPL3115_INT_EN_TCHG_MASK : mpl3115.h
- MPL3115_INT_EN_TCHG_SHIFT : mpl3115.h
- MPL3115_INT_EN_TTH_MASK : mpl3115.h
- MPL3115_INT_EN_TTH_SHIFT : mpl3115.h
- MPL3115_INT_EN_TW_MASK : mpl3115.h
- MPL3115_INT_EN_TW_SHIFT : mpl3115.h
- MPL3115_INT_SOURCE : mpl3115.h
- MPL3115_IPOL1_MASK : mpl3115.h
- MPL3115_IPOL1_SHIFT : mpl3115.h
- MPL3115_IPOL2_MASK : mpl3115.h
- MPL3115_IPOL2_SHIFT : mpl3115.h
- MPL3115_LOAD_OUT_MASK : mpl3115.h
- MPL3115_LOAD_OUT_SHIFT : mpl3115.h
- MPL3115_OFF_H : mpl3115.h
- MPL3115_OFF_P : mpl3115.h
- MPL3115_OFF_T : mpl3115.h
- MPL3115_OS_MASK : mpl3115.h
- MPL3115_OS_SHIFT : mpl3115.h
- MPL3115_OST_MASK : mpl3115.h
- MPL3115_OST_SHIFT : mpl3115.h
- mpl3115_osTable : fsl_mpl3115_i2c_1D_press.c
- MPL3115_OUT_DR_STATUS : mpl3115.h
- MPL3115_OUT_P_CSB : mpl3115.h
- MPL3115_OUT_P_DELTA_CSB : mpl3115.h
- MPL3115_OUT_P_DELTA_LSB : mpl3115.h
- MPL3115_OUT_P_DELTA_MSB : mpl3115.h
- MPL3115_OUT_P_LSB : mpl3115.h
- MPL3115_OUT_P_MSB : mpl3115.h
- MPL3115_OUT_T_DELTA_LSB : mpl3115.h
- MPL3115_OUT_T_DELTA_MSB : mpl3115.h
- MPL3115_OUT_T_LSB : mpl3115.h
- MPL3115_OUT_T_MSB : mpl3115.h
- MPL3115_P_ARM_LSB : mpl3115.h
- MPL3115_P_ARM_MSB : mpl3115.h
- MPL3115_P_ARM_WND_LSB : mpl3115.h
- MPL3115_P_ARM_WND_MSB : mpl3115.h
- MPL3115_P_MAX_CSB : mpl3115.h
- MPL3115_P_MAX_LSB : mpl3115.h
- MPL3115_P_MAX_MSB : mpl3115.h
- MPL3115_P_MIN_CSB : mpl3115.h
- MPL3115_P_MIN_LSB : mpl3115.h
- MPL3115_P_MIN_MSB : mpl3115.h
- MPL3115_PDEFE_MASK : mpl3115.h
- MPL3115_PDEFE_SHIFT : mpl3115.h
- MPL3115_PDR_MASK : mpl3115.h
- MPL3115_PDR_SHIFT : mpl3115.h
- MPL3115_PP_OD1_MASK : mpl3115.h
- MPL3115_PP_OD1_SHIFT : mpl3115.h
- MPL3115_PP_OD2_MASK : mpl3115.h
- MPL3115_PP_OD2_SHIFT : mpl3115.h
- MPL3115_PRESS_FIXED_CONVERSION_FACTOR : fsl_mpl3115_i2c_1D_press.c
- MPL3115_PRESS_FIXED_CONVERSION_OFFSET : fsl_mpl3115_i2c_1D_press.c
- MPL3115_PRESS_FLOAT_CONVERSION_FACTOR : fsl_mpl3115_i2c_1D_press.c
- MPL3115_PRESS_FLOAT_CONVERSION_OFFSET : fsl_mpl3115_i2c_1D_press.c
- MPL3115_PT_DATA_CFG : mpl3115.h
- MPL3115_PTDR_MASK : mpl3115.h
- MPL3115_PTDR_SHIFT : mpl3115.h
- MPL3115_PTOW_MASK : mpl3115.h
- MPL3115_PTOW_SHIFT : mpl3115.h
- MPL3115_RAW_MASK : mpl3115.h
- MPL3115_RAW_SHIFT : mpl3115.h
- mpl3115_Reset() : fsl_mpl3115_i2c_1D_press.c
- MPL3115_RST_MASK : mpl3115.h
- MPL3115_RST_SHIFT : mpl3115.h
- MPL3115_SBYB_MASK : mpl3115.h
- MPL3115_SBYB_SHIFT : mpl3115.h
- MPL3115_SET_FIELD : mpl3115.h
- mpl3115_SetConfig() : fsl_mpl3115_i2c_1D_press.c
- mpl3115_SetMode() : fsl_mpl3115_i2c_1D_press.c
- MPL3115_SRC_DRDY_MASK : mpl3115.h
- MPL3115_SRC_DRDY_SHIFT : mpl3115.h
- MPL3115_SRC_PCHG_MASK : mpl3115.h
- MPL3115_SRC_PCHG_SHIFT : mpl3115.h
- MPL3115_SRC_PTH_MASK : mpl3115.h
- MPL3115_SRC_PTH_SHIFT : mpl3115.h
- MPL3115_SRC_PW_MASK : mpl3115.h
- MPL3115_SRC_PW_SHIFT : mpl3115.h
- MPL3115_SRC_TCHG_MASK : mpl3115.h
- MPL3115_SRC_TCHG_SHIFT : mpl3115.h
- MPL3115_SRC_TTH_MASK : mpl3115.h
- MPL3115_SRC_TTH_SHIFT : mpl3115.h
- MPL3115_SRC_TW_MASK : mpl3115.h
- MPL3115_SRC_TW_SHIFT : mpl3115.h
- MPL3115_ST_MASK : mpl3115.h
- MPL3115_ST_SHIFT : mpl3115.h
- mpl3115_StartSample() : fsl_mpl3115_i2c_1D_press.c
- MPL3115_STATUS_00 : mpl3115.h
- mpl3115_status_t : mpl3115.h
- MPL3115_SUCCESS : mpl3115.h
- mpl3115_SupportedDataTypes : fsl_mpl3115_i2c_1D_press.h , fsl_mpl3115_i2c_1D_press.c
- mpl3115_SupportedSensorTypes : fsl_mpl3115_i2c_1D_press.h , fsl_mpl3115_i2c_1D_press.c
- MPL3115_SYSMOD : mpl3115.h
- MPL3115_SYSMOD_MASK : mpl3115.h
- MPL3115_SYSMOD_SHIFT : mpl3115.h
- MPL3115_T_ARM : mpl3115.h
- MPL3115_T_ARM_WND : mpl3115.h
- MPL3115_T_MAX_LSB : mpl3115.h
- MPL3115_T_MAX_MSB : mpl3115.h
- MPL3115_T_MIN_LSB : mpl3115.h
- MPL3115_T_MIN_MSB : mpl3115.h
- MPL3115_TDEFE_MASK : mpl3115.h
- MPL3115_TDEFE_SHIFT : mpl3115.h
- MPL3115_TDR_MASK : mpl3115.h
- MPL3115_TDR_SHIFT : mpl3115.h
- MPL3115_TEMP_FIXED_CONVERSION_FACTOR : fsl_mpl3115_i2c_1D_press.c
- MPL3115_TEMP_FIXED_CONVERSION_OFFSET : fsl_mpl3115_i2c_1D_press.c
- MPL3115_TEMP_FLOAT_CONVERSION_FACTOR : fsl_mpl3115_i2c_1D_press.c
- MPL3115_TEMP_FLOAT_CONVERSION_OFFSET : fsl_mpl3115_i2c_1D_press.c
- MPL3115_TIME_DLY : mpl3115.h
- mpl3115_ValidateConfig() : fsl_mpl3115_i2c_1D_press.c
- MPL3115_WHO_AM_I : mpl3115.h
- MPL3115_WHOAMI_VALUE : mpl3115.h
- MPxx5004 : Analog_1.h
- MQX_init_struct : mqx_ksdk.h
- mqx_task_stack_pointers : fsl_fusion_virt_3D_orient.c
- MQX_template_list : mqx_ksdk.c
- MSG_SIZE : fsl_Sensor_Analog_1_Functions.c

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.