| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
dm_DeviceDescriptor_struct Struct Reference

This structure defines a handle for the device. More...

`#include <isf_devmsg.h>`

Collaboration diagram for dm_DeviceDescriptor_struct:

## Data Fields
dm_ChannelDescriptor_t * | pChannelDescriptor
void * | pEndpointHandle

## Detailed Description

This structure defines a handle for the device.

The device handle contains the information required by the device messaging functions to address and communicate with a slave device.

Definition at line 61 of file isf_devmsg.h.

## Field Documentation

dm_ChannelDescriptor_t* pChannelDescriptor

The pointer to the channel descriptor.

Definition at line 62 of file isf_devmsg.h.

Referenced by dm_channel_get_descriptor(), dm_device_close(), dm_device_open(), dm_device_readx(), dm_device_writex(), fxlc95000_read(), fxlc95000_send(), mma955x_read(), and mma955x_send().

void* pEndpointHandle

The protocol-specific endpoint handle.

Definition at line 63 of file isf_devmsg.h.

Referenced by dm_device_close(), dm_device_open(), dm_device_readx(), and dm_device_writex().

The documentation for this struct was generated from the following file:

- ISF/Core/Include/isf_devmsg.h

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.