| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
rliAppStatus_t Struct Reference

rli application configuration buffer format. More...

Collaboration diagram for rliAppStatus_t:

## Data Fields
uint8 | device
uint8 | channel
uint8 | error

## Detailed Description

rli application configuration buffer format.

Definition at line 69 of file rli_project.c.

## Field Documentation

uint8 channel

Definition at line 71 of file rli_project.c.

Referenced by device_connect(), and device_disconnect().

uint8 device

Definition at line 70 of file rli_project.c.

Referenced by device_connect(), device_disconnect(), and rli_ci_app_callback().

uint8 error

Definition at line 72 of file rli_project.c.

Referenced by rli_ci_app_callback(), and rli_PeriodicCallback().

The documentation for this struct was generated from the following file:

- ISF/RLI/Source/rli_project.c

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.