| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

Macros | Variables
MMA955x_1.h File Reference
`#include "I2C1.h"`
`#include "mma955x.h"`
`#include "fsl_mma955x_i2cspi_pedo.h"`
`#include "fsl_i2c_master_driver.h"`
`#include "Cpu.h"`
Include dependency graph for MMA955x_1.h:
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Macros
#define | MMA955x_1_DATA_TYPE mma955x_PedometerNativeData_t
#define | MMA955x_1_SAMPLE_OFFSET (26)
#define | MMA955x_1_SAMPLE_SIZE (6)
#define | MMA955x_1_CONFIG_REGISTER_READ_OFFSET (0)
#define | MMA955x_1_CONFIG_REGISTER_SIZE (sizeof(mma955x_readConfigResponseBuffer_t))
#define | MMA955x_1_ACC_FLOAT_CONVERSION_FACTOR_2g (0.000061035156)
#define | MMA955x_1_ACC_FLOAT_CONVERSION_FACTOR_4g (0.000122070312)
#define | MMA955x_1_ACC_FLOAT_CONVERSION_FACTOR_8g (0.000244140624)

## Variables
mma955x_Sensor_Specific_Settings_t | MMA955x_1_Sensor_Specific_Config
| This allows access to the sensor specific configuration for the target sensor. More...
const isf_dsa_Adapter_t | MMA955x_1_Adapter
| This allows access to the sensor adapter instance for the target sensor. More...
const i2c_device_t | MMA955x_1_DeviceInfo
| This allows access to the sensor communications specific configuration. More...

## Detailed Description

Version
  01.00

Definition in file MMA955x_1.h.

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.