| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
uart_BusHandle_struct Struct Reference

This structure defines the data bus handle. More...

`#include <isf_uart_types.h>`

Collaboration diagram for uart_BusHandle_struct:

## Data Fields
isf_uart_state_t | uartHandle
uint8 | id
uint8 | busState
uart_BusConfig_t | busConfig

## Detailed Description

This structure defines the data bus handle.

Definition at line 28 of file isf_uart_types.h.

## Field Documentation

uart_BusConfig_t busConfig

current bus configuration.

Definition at line 33 of file isf_uart_types.h.

Referenced by uart_adapter_acquire_lock(), uart_adapter_configure(), uart_adapter_get_endpoint(), uart_adapter_read(), uart_adapter_start(), uart_adapter_stop(), and uart_adapter_write().

uint8 busState

The bus sate.

Definition at line 32 of file isf_uart_types.h.

Referenced by uart_adapter_configure(), uart_adapter_get_endpoint(), uart_adapter_get_state(), uart_adapter_init(), uart_adapter_read(), uart_adapter_start(), uart_adapter_stop(), and uart_adapter_write().

uint8 id

The unique ID associated with the bus handle.

Definition at line 31 of file isf_uart_types.h.

isf_uart_state_t uartHandle

The uart current handle.

Definition at line 30 of file isf_uart_types.h.

Referenced by uart_adapter_configure(), uart_adapter_init(), uart_adapter_read(), uart_adapter_start(), uart_adapter_stop(), and uart_adapter_write().

The documentation for this struct was generated from the following file:

- ISF/ProtocolAdapter/Include/isf_uart_types.h

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.