| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

Data Structures | Typedefs
isf_altitude_types.h File Reference

The isf_altitude_types.h file contains the ISF data type definitions for use with the ISF generic altitude fixed and floating point interface. More...

`#include <isf_sensor_base_types.h>`
Include dependency graph for isf_altitude_types.h:
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Data Structures
struct | isf_Meters1D_EngFixed_t
| Standard fixed type for single axis altitude sensor. More...
struct | isf_Meters1D_float_t
| Standard floating point type for single axis altitude sensor. More...

## Typedefs
typedef int32 | isf_alt_meters_fixed_32s1i16_t
| ISF sensors standard fixed point altitude in meters using AC_Fixed(32,16,1) notation This means of 32 total bits, 16 are used to represent the integer portion with the MSB as a sign bit. the LSB is therefore ~1.5259E-05 meters. The type can contain pressures in the +/- 32768 meter range. More...
typedef float | isf_altitude_meters_float_t
| ISF sensors standard floating point altitude in meters. More...

## Detailed Description

The isf_altitude_types.h file contains the ISF data type definitions for use with the ISF generic altitude fixed and floating point interface.

Copyright
  Copyright (c) 2015, Freescale Semiconductor, Inc.

Definition in file isf_altitude_types.h.

## Typedef Documentation

typedef int32 isf_alt_meters_fixed_32s1i16_t

ISF sensors standard fixed point altitude in meters using AC_Fixed(32,16,1) notation This means of 32 total bits, 16 are used to represent the integer portion with the MSB as a sign bit. the LSB is therefore ~1.5259E-05 meters. The type can contain pressures in the +/- 32768 meter range.

Definition at line 22 of file isf_altitude_types.h.

typedef float isf_altitude_meters_float_t

ISF sensors standard floating point altitude in meters.

Definition at line 33 of file isf_altitude_types.h.

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.