| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

Enumerations | Variables
SensorEnable module documentation

## Enumerations
enum | _SensorEnable_pinNames { J199_3 = GPIO_MAKE_PIN(GPIOC_IDX, 14U) }
| Pin names. More...

## Variables
const gpio_output_pin_user_config_t | SensorEnable_OutConfig0 []
| Configuration structure 0 for output pins. More...
const gpio_output_pin_user_config_t | SensorEnable_OutConfig0 []
| Configuration structure 0 for output pins. More...

## Detailed Description

## Enumeration Type Documentation

enum _SensorEnable_pinNames

Pin names.

Enumerator
J199_3 |

Definition at line 81 of file SensorEnable.h.

## Variable Documentation

const gpio_output_pin_user_config_t SensorEnable_OutConfig0[]

Initial value:
= {
{
.pinName = J199_3,
.config.outputLogic = 0,
.config.slewRate = kPortSlowSlewRate,
.config.isOpenDrainEnabled = true,
.config.driveStrength = kPortLowDriveStrength,
},
{
.pinName = GPIO_PINS_OUT_OF_RANGE,
}
}
J199_3
Definition: SensorEnable.h:82

Configuration structure 0 for output pins.

Definition at line 56 of file SensorEnable.c.

Referenced by Components_Init().

const gpio_output_pin_user_config_t SensorEnable_OutConfig0[]

Configuration structure 0 for output pins.

Definition at line 56 of file SensorEnable.c.

Referenced by Components_Init().

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.