| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

hardware_init.c
Go to the documentation of this file.
1 /* ###################################################################
2 ** This component module is generated by Processor Expert. Do not modify it.
3 ** Filename : pin_init.c
4 ** Project : ISF2P2_K64F_MQX_PROJ
5 ** Processor : MK64FN1M0VLL12
6 ** Component : PinSettings
7 ** Version : Component 1.2.0, Driver 1.4, CPU db: 3.00.000
8 ** Repository : KSDK 1.2.0
9 ** Compiler : GNU C Compiler
10 ** Date/Time : 2016-10-06, 13:38, # CodeGen: 0
11 ** Abstract :
12 **
13 ** Settings :
14 ** Component name : pin_init
15 ** PinSettings IP Block : PinSettings
16 ** Processor : MK64FN1M0LL12_4SDK
17 ** Pin settings :
18 ** Routing :
19 ** Peripheral Type ADC :
20 ** Custom name : ADC0
21 ** ADC0 :
22 ** DM0 - Minus channel 0 : ADC0_DM0/ADC1_DM3
23 ** DM1 - Minus channel 1 : ADC0_DM1
24 ** DM2 - Minus channel 2 : <Automatic>
25 ** DM3 - Minus channel 3 : ADC1_DM0/ADC0_DM3
26 ** DP0 - Plus channel 0 : ADC0_DP0/ADC1_DP3
27 ** DP1 - Plus channel 1 : ADC0_DP1
28 ** DP2 - Plus channel 2 : <Automatic>
29 ** DP3 - Plus channel 3 : ADC1_DP0/ADC0_DP3
30 ** SE0 - Single-ended channel 0 : ADC0_DP0/ADC1_DP3
31 ** SE1 - Single-ended channel 1 : ADC0_DP1
32 ** SE2 - Single-ended channel 2 : <Automatic>
33 ** SE3 - Single-ended channel 3 : ADC1_DP0/ADC0_DP3
34 ** SE8 - Single-ended channel 8 : <Automatic>
35 ** SE9 - Single-ended channel 9 : <Automatic>
36 ** SE12 - Single-ended channel 12 : <Automatic>
37 ** SE13 - Single-ended channel 13 : <Automatic>
38 ** SE14 - Single-ended channel 14 : <Automatic>
39 ** SE15 - Single-ended channel 15 : <Automatic>
40 ** SE17 - Single-ended channel 17 : <Automatic>
41 ** SE18 - Single-ended channel 18 : <Automatic>
42 ** SE19 - Single-ended channel 19 : ADC0_DM0/ADC1_DM3
43 ** SE20 - Single-ended channel 20 : ADC0_DM1
44 ** SE23 - Single-ended channel 23 : J26_11
45 ** SE4b - Single-ended channel 4b : <Automatic>
46 ** SE5b - Single-ended channel 5b : <Automatic>
47 ** SE6b - Single-ended channel 6b : <Automatic>
48 ** SE7b - Single-ended channel 7b : <Automatic>
49 ** Trigger A input : <Automatic>
50 ** Trigger B input : <Automatic>
51 ** Voltage reference high : VDDA
52 ** Voltage reference high : VREFH
53 ** Voltage reference low : VREFL
54 ** Voltage reference low : VSSA
55 ** Bool_ADC0 : yes
56 ** Custom name : ADC1
57 ** ADC1 :
58 ** DM0 - Minus channel 0 : ADC1_DM0/ADC0_DM3
59 ** DM1 - Minus channel 1 : ADC1_DM1
60 ** DM3 - Minus channel 3 : ADC0_DM0/ADC1_DM3
61 ** DP0 - Plus channel 0 : ADC1_DP0/ADC0_DP3
62 ** DP1 - Plus channel 1 : ADC1_DP1
63 ** DP3 - Plus channel 3 : ADC0_DP0/ADC1_DP3
64 ** SE0 - Single-ended channel 0 : ADC1_DP0/ADC0_DP3
65 ** SE1 - Single-ended channel 1 : ADC1_DP1
66 ** SE3 - Single-ended channel 3 : ADC0_DP0/ADC1_DP3
67 ** SE8 - Single-ended channel 8 : <Automatic>
68 ** SE9 - Single-ended channel 9 : <Automatic>
69 ** SE14 - Single-ended channel 14 : <Automatic>
70 ** SE15 - Single-ended channel 15 : <Automatic>
71 ** SE17 - Single-ended channel 17 : <Automatic>
72 ** SE18 - Single-ended channel 18 : VREF_OUT/CMP1_IN5/CMP0_IN5/ADC1_SE18
73 ** SE19 - Single-ended channel 19 : ADC1_DM0/ADC0_DM3
74 ** SE20 - Single-ended channel 20 : ADC1_DM1
75 ** SE4a - Single-ended channel 4a : <Automatic>
76 ** SE5a - Single-ended channel 5a : <Automatic>
77 ** SE6a - Single-ended channel 6a : <Automatic>
78 ** SE7a - Single-ended channel 7a : <Automatic>
79 ** SE4b - Single-ended channel 4b : <Automatic>
80 ** SE5b - Single-ended channel 5b : <Automatic>
81 ** SE6b - Single-ended channel 6b : <Automatic>
82 ** SE7b - Single-ended channel 7b : <Automatic>
83 ** Trigger A input : <Automatic>
84 ** Trigger B input : <Automatic>
85 ** Voltage reference high : VDDA
86 ** Voltage reference high : VREFH
87 ** Voltage reference low : VREFL
88 ** Voltage reference low : VSSA
89 ** Bool_ADC1 : yes
90 ** Peripheral Type AIPS :
91 ** Custom name : AIPS0
92 ** Custom name : AIPS1
93 ** Peripheral Type AXBS :
94 ** Custom name : AXBS
95 ** Peripheral Type CAN :
96 ** Custom name : CAN0
97 ** CAN0 :
98 ** RX - receiver input : <Automatic>
99 ** TX - transmitter output : <Automatic>
100 ** Bool_CAN0 : yes
101 ** Peripheral Type CAU :
102 ** Custom name : CAU
103 ** Peripheral Type CMP :
104 ** Custom name : CMP0
105 ** CMP0 :
106 ** IN0 - Input 0 : <Automatic>
107 ** IN1 - Input 1 : <Automatic>
108 ** IN2 - Input 2 : <Automatic>
109 ** IN3 - Input 3 : <Automatic>
110 ** IN5 - Input 5 : VREF_OUT/CMP1_IN5/CMP0_IN5/ADC1_SE18
111 ** OUT - Comparator output : <Automatic>
112 ** Bool_CMP0 : yes
113 ** Custom name : CMP1
114 ** CMP1 :
115 ** IN0 - Input 0 : <Automatic>
116 ** IN1 - Input 1 : <Automatic>
117 ** IN3 - Input 3 : J26_11
118 ** IN5 - Input 5 : VREF_OUT/CMP1_IN5/CMP0_IN5/ADC1_SE18
119 ** OUT - Comparator output : <Automatic>
120 ** Bool_CMP1 : yes
121 ** Custom name : CMP2
122 ** CMP2 :
123 ** IN0 - Input 0 : <Automatic>
124 ** IN1 - Input 1 : <Automatic>
125 ** OUT - Comparator output : <Automatic>
126 ** Bool_CMP2 : yes
127 ** Peripheral Type CMT :
128 ** Custom name : CMT
129 ** CMT :
130 ** Infrared output : <Automatic>
131 ** Bool_CMT : yes
132 ** Peripheral Type CRC :
133 ** Custom name : CRC
134 ** Peripheral Type CoreDebug :
135 ** Peripheral Type DAC :
136 ** Custom name : DAC0
137 ** DAC0 :
138 ** Output pin : J26_11
139 ** Bool_DAC0 : yes
140 ** Peripheral Type DMA :
141 ** Custom name : DMA
142 ** Peripheral Type DMAMUX :
143 ** Custom name : DMAMUX
144 ** Peripheral Type DRY :
145 ** Peripheral Type DWT :
146 ** Peripheral Type ENET :
147 ** Custom name : ENET
148 ** ENET :
149 ** 1588 timer 0 : <Automatic>
150 ** Direction : <Automatic>
151 ** 1588 timer 1 : <Automatic>
152 ** Direction : <Automatic>
153 ** 1588 timer 2 : <Automatic>
154 ** Direction : <Automatic>
155 ** MII MDC - Management data clock : <Automatic>
156 ** MII MDIO - Management data input/output: <Automatic>
157 ** MII RXD0 - Receive data 0 : <Automatic>
158 ** MII RXD1 - Receive data 1 : <Automatic>
159 ** MII RXDV - Receive data valid : <Automatic>
160 ** MII RXER - Receive error : <Automatic>
161 ** MII TXD0 - Transmit data 0 : <Automatic>
162 ** MII TXD1 - Transmit data 1 : <Automatic>
163 ** MII TXNE - Transmit enable : <Automatic>
164 ** RMII EXTAL - External reference clock : <Automatic>
165 ** RMII CRS_DV - Receive data valid : <Automatic>
166 ** RMII MDC - Management data clock : <Automatic>
167 ** RMII MDIO - Management data input/output: <Automatic>
168 ** RMII RXD0 - Receive data 0 : <Automatic>
169 ** RMII RXD1 - Receive data 1 : <Automatic>
170 ** RMII RXER - Receive error : <Automatic>
171 ** RMII TXD0 - Transmit data 0 : <Automatic>
172 ** RMII TXD1 - Transmit data 1 : <Automatic>
173 ** RMII TXEN - Transmit enable : <Automatic>
174 ** Bool_ENET : yes
175 ** Peripheral Type ETB :
176 ** Peripheral Type ETF :
177 ** Peripheral Type ETM :
178 ** Peripheral Type EWM :
179 ** Custom name : EWM
180 ** EWM :
181 ** Input pin : <Automatic>
182 ** Output pin : <Automatic>
183 ** Bool_EWM : yes
184 ** Peripheral Type FB :
185 ** Custom name : FB
186 ** FB :
187 ** AD0 - Address/data bus 0 : <Automatic>
188 ** AD1 - Address/data bus 1 : <Automatic>
189 ** AD2 - Address/data bus 2 : <Automatic>
190 ** AD3 - Address/data bus 3 : <Automatic>
191 ** AD4 - Address/data bus 4 : <Automatic>
192 ** AD5 - Address/data bus 5 : <Automatic>
193 ** AD6 - Address/data bus 6 : <Automatic>
194 ** AD7 - Address/data bus 7 : <Automatic>
195 ** AD8 - Address/data bus 8 : <Automatic>
196 ** AD9 - Address/data bus 9 : <Automatic>
197 ** AD10 - Address/data bus 10 : <Automatic>
198 ** AD11 - Address/data bus 11 : <Automatic>
199 ** AD12 - Address/data bus 12 : <Automatic>
200 ** AD13 - Address/data bus 13 : <Automatic>
201 ** AD14 - Address/data bus 14 : <Automatic>
202 ** AD15 - Address/data bus 15 : <Automatic>
203 ** AD16 - Address/data bus 16 : <Automatic>
204 ** AD17 - Address/data bus 17 : <Automatic>
205 ** AD18 - Address/data bus 18 : <Automatic>
206 ** AD19 - Address/data bus 19 : <Automatic>
207 ** AD20 - Address/data bus 20 : <Automatic>
208 ** AD24 - Address/data bus 24 : <Automatic>
209 ** AD25 - Address/data bus 25 : <Automatic>
210 ** AD26 - Address/data bus 26 : <Automatic>
211 ** AD27 - Address/data bus 27 : <Automatic>
212 ** AD28 - Address/data bus 28 : <Automatic>
213 ** AD29 - Address/data bus 29 : <Automatic>
214 ** AD30 - Address/data bus 30 : <Automatic>
215 ** AD31 - Address/data bus 31 : <Automatic>
216 ** CLKOUT - Clock Output : <Automatic>
217 ** CS0 - Chip select 0 : <Automatic>
218 ** CS1/ALE/TS : <Automatic>
219 ** CS2/TBST/BE15_8 : <Automatic>
220 ** CS4/TSIZ0/BE31_24 : <Automatic>
221 ** CS5/TSIZ1/BE23_16 : <Automatic>
222 ** OE - Output enable : <Automatic>
223 ** RW - Read/write : <Automatic>
224 ** Bool_FB : yes
225 ** Peripheral Type FMC :
226 ** Custom name : FMC
227 ** Peripheral Type FPB :
228 ** Peripheral Type FTFE :
229 ** Custom name : FTFE
230 ** Peripheral Type FTM :
231 ** Custom name : FTM0
232 ** FTM0 :
233 ** CH0 - Channel 0 : <Automatic>
234 ** Direction : <Automatic>
235 ** CH1 - Channel 1 : <Automatic>
236 ** Direction : <Automatic>
237 ** CH2 - Channel 2 : <Automatic>
238 ** Direction : <Automatic>
239 ** CH3 - Channel 3 : <Automatic>
240 ** Direction : <Automatic>
241 ** CH4 - Channel 4 : <Automatic>
242 ** Direction : <Automatic>
243 ** CH5 - Channel 5 : <Automatic>
244 ** Direction : <Automatic>
245 ** CH6 - Channel 6 : <Automatic>
246 ** Direction : <Automatic>
247 ** CH7 - Channel 7 : <Automatic>
248 ** Direction : <Automatic>
249 ** CLKIN0 - External clock input : <Automatic>
250 ** FLT0 - fault input 0 : <Automatic>
251 ** FLT1 - fault input 1 : <Automatic>
252 ** FLT2 - fault input 2 : <Automatic>
253 ** FLT3 - fault input 3 : <Automatic>
254 ** Trigger input 0 : <Automatic>
255 ** Trigger input 1 : <Automatic>
256 ** Trigger input 2 : <Automatic>
257 ** Bool_FTM0 : yes
258 ** Custom name : FTM1
259 ** FTM1 :
260 ** CH0 - Channel 0 : <Automatic>
261 ** Direction : <Automatic>
262 ** CH1 - Channel 1 : <Automatic>
263 ** Direction : <Automatic>
264 ** CLKIN0 - External clock input : <Automatic>
265 ** FLT0 - fault input 0 : <Automatic>
266 ** FLT1 - fault input 1 : <Automatic>
267 ** FLT2 - fault input 2 : <Automatic>
268 ** Quadrature decoder phase A input : <Automatic>
269 ** Quadrature decoder phase B input : <Automatic>
270 ** Trigger input 0 : <Automatic>
271 ** Trigger input 1 : <Automatic>
272 ** Trigger input 2 : <Automatic>
273 ** Bool_FTM1 : yes
274 ** Custom name : FTM2
275 ** FTM2 :
276 ** CH0 - Channel 0 : <Automatic>
277 ** Direction : <Automatic>
278 ** CH1 - Channel 1 : <Automatic>
279 ** Direction : <Automatic>
280 ** CLKIN0 - External clock input : <Automatic>
281 ** FLT0 - fault input 0 : <Automatic>
282 ** FLT1 - fault input 1 : <Automatic>
283 ** FLT2 - fault input 2 : <Automatic>
284 ** Quadrature decoder phase A input : <Automatic>
285 ** Quadrature decoder phase B input : <Automatic>
286 ** Trigger input 0 : <Automatic>
287 ** Trigger input 1 : <Automatic>
288 ** Bool_FTM2 : yes
289 ** Custom name : FTM3
290 ** FTM3 :
291 ** CH0 - Channel 0 : <Automatic>
292 ** Direction : <Automatic>
293 ** CH1 - Channel 1 : <Automatic>
294 ** Direction : <Automatic>
295 ** CH2 - Channel 2 : <Automatic>
296 ** Direction : <Automatic>
297 ** CH3 - Channel 3 : <Automatic>
298 ** Direction : <Automatic>
299 ** CH4 - Channel 4 : <Automatic>
300 ** Direction : <Automatic>
301 ** CH5 - Channel 5 : <Automatic>
302 ** Direction : <Automatic>
303 ** CH6 - Channel 6 : <Automatic>
304 ** Direction : <Automatic>
305 ** CH7 - Channel 7 : <Automatic>
306 ** Direction : <Automatic>
307 ** CLKIN0 - External clock input : <Automatic>
308 ** FLT0 - fault input 0 : <Automatic>
309 ** FLT1 - fault input 1 : <Automatic>
310 ** Trigger input 0 : <Automatic>
311 ** Trigger input 1 : <Automatic>
312 ** Bool_FTM3 : yes
313 ** Peripheral Type GPIO :
314 ** Custom name : PTA
315 ** PTA :
316 ** Pin 0 : <Automatic>
317 ** Direction : <Automatic>
318 ** Pin 1 : <Automatic>
319 ** Direction : <Automatic>
320 ** Pin 2 : <Automatic>
321 ** Direction : <Automatic>
322 ** Pin 3 : <Automatic>
323 ** Direction : <Automatic>
324 ** Pin 4 : <Automatic>
325 ** Direction : <Automatic>
326 ** Pin 5 : <Automatic>
327 ** Direction : <Automatic>
328 ** Pin 12 : <Automatic>
329 ** Direction : <Automatic>
330 ** Pin 13 : <Automatic>
331 ** Direction : <Automatic>
332 ** Pin 14 : <Automatic>
333 ** Direction : <Automatic>
334 ** Pin 15 : <Automatic>
335 ** Direction : <Automatic>
336 ** Pin 16 : <Automatic>
337 ** Direction : <Automatic>
338 ** Pin 17 : <Automatic>
339 ** Direction : <Automatic>
340 ** Pin 18 : <Automatic>
341 ** Direction : <Automatic>
342 ** Pin 19 : <Automatic>
343 ** Direction : <Automatic>
344 ** Bool_PTA : yes
345 ** Custom name : PTB
346 ** PTB :
347 ** Pin 0 : <Automatic>
348 ** Direction : <Automatic>
349 ** Pin 1 : <Automatic>
350 ** Direction : <Automatic>
351 ** Pin 2 : <Automatic>
352 ** Direction : <Automatic>
353 ** Pin 3 : <Automatic>
354 ** Direction : <Automatic>
355 ** Pin 9 : <Automatic>
356 ** Direction : <Automatic>
357 ** Pin 10 : <Automatic>
358 ** Direction : <Automatic>
359 ** Pin 11 : <Automatic>
360 ** Direction : <Automatic>
361 ** Pin 16 : <Automatic>
362 ** Direction : <Automatic>
363 ** Pin 17 : <Automatic>
364 ** Direction : <Automatic>
365 ** Pin 18 : <Automatic>
366 ** Direction : <Automatic>
367 ** Pin 19 : <Automatic>
368 ** Direction : <Automatic>
369 ** Pin 20 : <Automatic>
370 ** Direction : <Automatic>
371 ** Pin 21 : <Automatic>
372 ** Direction : <Automatic>
373 ** Pin 22 : <Automatic>
374 ** Direction : <Automatic>
375 ** Pin 23 : <Automatic>
376 ** Direction : <Automatic>
377 ** Bool_PTB : yes
378 ** Custom name : PTC
379 ** PTC :
380 ** Pin 0 : <Automatic>
381 ** Direction : <Automatic>
382 ** Pin 1 : <Automatic>
383 ** Direction : <Automatic>
384 ** Pin 2 : <Automatic>
385 ** Direction : <Automatic>
386 ** Pin 3 : <Automatic>
387 ** Direction : <Automatic>
388 ** Pin 4 : <Automatic>
389 ** Direction : <Automatic>
390 ** Pin 5 : <Automatic>
391 ** Direction : <Automatic>
392 ** Pin 6 : <Automatic>
393 ** Direction : <Automatic>
394 ** Pin 7 : <Automatic>
395 ** Direction : <Automatic>
396 ** Pin 8 : <Automatic>
397 ** Direction : <Automatic>
398 ** Pin 9 : <Automatic>
399 ** Direction : <Automatic>
400 ** Pin 10 : <Automatic>
401 ** Direction : <Automatic>
402 ** Pin 11 : <Automatic>
403 ** Direction : <Automatic>
404 ** Pin 12 : <Automatic>
405 ** Direction : <Automatic>
406 ** Pin 13 : <Automatic>
407 ** Direction : <Automatic>
408 ** Pin 14 : <Automatic>
409 ** Direction : <Automatic>
410 ** Pin 15 : <Automatic>
411 ** Direction : <Automatic>
412 ** Pin 16 : <Automatic>
413 ** Direction : <Automatic>
414 ** Pin 17 : <Automatic>
415 ** Direction : <Automatic>
416 ** Pin 18 : <Automatic>
417 ** Direction : <Automatic>
418 ** Bool_PTC : yes
419 ** Custom name : PTD
420 ** PTD :
421 ** Pin 0 : <Automatic>
422 ** Direction : <Automatic>
423 ** Pin 1 : <Automatic>
424 ** Direction : <Automatic>
425 ** Pin 2 : <Automatic>
426 ** Direction : <Automatic>
427 ** Pin 3 : <Automatic>
428 ** Direction : <Automatic>
429 ** Pin 4 : <Automatic>
430 ** Direction : <Automatic>
431 ** Pin 5 : <Automatic>
432 ** Direction : <Automatic>
433 ** Pin 6 : <Automatic>
434 ** Direction : <Automatic>
435 ** Pin 7 : <Automatic>
436 ** Direction : <Automatic>
437 ** Bool_PTD : yes
438 ** Custom name : PTE
439 ** PTE :
440 ** Pin 0 : <Automatic>
441 ** Direction : <Automatic>
442 ** Pin 1 : <Automatic>
443 ** Direction : <Automatic>
444 ** Pin 2 : <Automatic>
445 ** Direction : <Automatic>
446 ** Pin 3 : <Automatic>
447 ** Direction : <Automatic>
448 ** Pin 4 : <Automatic>
449 ** Direction : <Automatic>
450 ** Pin 5 : <Automatic>
451 ** Direction : <Automatic>
452 ** Pin 6 : <Automatic>
453 ** Direction : <Automatic>
454 ** Pin 24 : <Automatic>
455 ** Direction : <Automatic>
456 ** Pin 25 : <Automatic>
457 ** Direction : <Automatic>
458 ** Pin 26 : <Automatic>
459 ** Direction : <Automatic>
460 ** Bool_PTE : yes
461 ** Peripheral Type I2C :
462 ** Custom name : I2C0
463 ** I2C0 :
464 ** SCL - Serial clock : <Automatic>
465 ** SDA - Serial data : <Automatic>
466 ** Bool_I2C0 : yes
467 ** Custom name : I2C1
468 ** I2C1 :
469 ** SCL - Serial clock : <Automatic>
470 ** SDA - Serial data : <Automatic>
471 ** Bool_I2C1 : yes
472 ** Custom name : I2C2
473 ** I2C2 :
474 ** SCL - Serial clock : <Automatic>
475 ** SDA - Serial data : <Automatic>
476 ** Bool_I2C2 : yes
477 ** Peripheral Type I2S :
478 ** Custom name : I2S0
479 ** I2S0 :
480 ** MCLK - Master clock : <Automatic>
481 ** Direction : <Automatic>
482 ** RX_BCLK - RX bit clock : <Automatic>
483 ** Direction : <Automatic>
484 ** RX_FS - RX frame sync : <Automatic>
485 ** Direction : <Automatic>
486 ** RXD0 - Receive data 0 : <Automatic>
487 ** RXD1 - Receive data 1 : <Automatic>
488 ** TX_BCLK - TX bit clock : <Automatic>
489 ** Direction : <Automatic>
490 ** TX_FS - TX frame sync : <Automatic>
491 ** Direction : <Automatic>
492 ** TXD0 - Transmit data 0 : <Automatic>
493 ** TXD1 - Transmit data 1 : <Automatic>
494 ** Bool_I2S0 : yes
495 ** Peripheral Type ITM :
496 ** Peripheral Type JTAG :
497 ** JTAG :
498 ** TCLK - Test clock : <Automatic>
499 ** TDI - Test data input : <Automatic>
500 ** TDO - Test data output : <Automatic>
501 ** TMS - Test mode selection : <Automatic>
502 ** TRST - Reset : <Automatic>
503 ** Bool_JTAG : yes
504 ** Peripheral Type LLWU :
505 ** Custom name : LLWU
506 ** LLWU :
507 ** P0 - Wake-up pin 0 : <Automatic>
508 ** P1 - Wake-up pin 1 : <Automatic>
509 ** P2 - Wake-up pin 2 : <Automatic>
510 ** P3 - Wake-up pin 3 : <Automatic>
511 ** P4 - Wake-up pin 4 : <Automatic>
512 ** P5 - Wake-up pin 5 : <Automatic>
513 ** P6 - Wake-up pin 6 : <Automatic>
514 ** P7 - Wake-up pin 7 : <Automatic>
515 ** P8 - Wake-up pin 8 : <Automatic>
516 ** P9 - Wake-up pin 9 : <Automatic>
517 ** P10 - Wake-up pin 10 : <Automatic>
518 ** P11 - Wake-up pin 11 : <Automatic>
519 ** P12 - Wake-up pin 12 : <Automatic>
520 ** P13 - Wake-up pin 13 : <Automatic>
521 ** P14 - Wake-up pin 14 : <Automatic>
522 ** P15 - Wake-up pin 15 : <Automatic>
523 ** Bool_LLWU : yes
524 ** Peripheral Type LPTMR :
525 ** Custom name : LPTMR0
526 ** LPTMR0 :
527 ** Pulse counter input 0 : <Automatic>
528 ** Pulse counter input 1 : <Automatic>
529 ** Pulse counter input 2 : <Automatic>
530 ** Bool_LPTMR0 : yes
531 ** Peripheral Type LPUART :
532 ** Peripheral Type MCG :
533 ** Custom name : MCG
534 ** Peripheral Type MCM :
535 ** Custom name : MCM
536 ** Peripheral Type MPU :
537 ** Custom name : MPU
538 ** Peripheral Type NV :
539 ** Custom name : FTFE_FlashConfig
540 ** Peripheral Type NVIC :
541 ** Custom name : NVIC
542 ** Peripheral Type OSC :
543 ** Custom name : OSC
544 ** OSC :
545 ** External clock/oscillator input : <Automatic>
546 ** Oscillator output : <Automatic>
547 ** Bool_OSC : yes
548 ** Peripheral Type PDB :
549 ** Custom name : PDB0
550 ** PDB0 :
551 ** External trigger input : <Automatic>
552 ** Bool_PDB0 : yes
553 ** Peripheral Type PIT :
554 ** Custom name : PIT
555 ** Peripheral Type PMC :
556 ** Custom name : PMC
557 ** Peripheral Type PORT :
558 ** Custom name : PORTA
559 ** Custom name : PORTB
560 ** Custom name : PORTC
561 ** Custom name : PORTD
562 ** Custom name : PORTE
563 ** Peripheral Type RCM :
564 ** Custom name : RCM
565 ** RCM :
566 ** Reset input : RST_TGTMCU_B/J14_1/J5_1/J9_10/J25_6
567 ** Bool_RCM : yes
568 ** Peripheral Type RFSYS :
569 ** Custom name : RFSYS
570 ** Peripheral Type RFVBAT :
571 ** Custom name : RFVBAT
572 ** Peripheral Type RNG :
573 ** Custom name : RNG
574 ** Peripheral Type RTC :
575 ** Custom name : RTC
576 ** RTC :
577 ** Oscillator output : <Automatic>
578 ** 32.768 kHz oscillator input : EXTAL32
579 ** VBAT power supply : VBAT
580 ** 32.768 kHz oscillator output : XTAL32
581 ** Bool_RTC : yes
582 ** Peripheral Type SCB :
583 ** Custom name : SystemControl
584 ** SystemControl :
585 ** NMI - Non-maskable interrupt : <Automatic>
586 ** Bool_SystemControl : yes
587 ** Peripheral Type SDHC :
588 ** Custom name : SDHC
589 ** SDHC :
590 ** CMD - Command line : <Automatic>
591 ** D0 - Data 0 : <Automatic>
592 ** D1 - Data 1 : <Automatic>
593 ** D2 - Data 2 : <Automatic>
594 ** D3 - Data 3 : <Automatic>
595 ** CLK - Card clock : <Automatic>
596 ** Bool_SDHC : yes
597 ** Peripheral Type SIM :
598 ** Custom name : SIM
599 ** SIM :
600 ** Clock generation SIM output : <Automatic>
601 ** Bool_SIM : yes
602 ** Peripheral Type SMC :
603 ** Custom name : SMC
604 ** Peripheral Type SPI :
605 ** Custom name : SPI0
606 ** SPI0 :
607 ** SPI peripheral chip select(output) 0 or slave select(input): <Automatic>
608 ** Direction : <Automatic>
609 ** PCS1 - Peripheral chip select 1 : <Automatic>
610 ** PCS2 - Peripheral chip select 2 : <Automatic>
611 ** PCS3 - Peripheral chip select 3 : <Automatic>
612 ** PCS4 - Peripheral chip select 4 : <Automatic>
613 ** PCS5 - Peripheral chip select 5 : <Automatic>
614 ** SPI chip select strobe : <Automatic>
615 ** SIN - Serial data in : <Automatic>
616 ** SCK - Serial clock : <Automatic>
617 ** Direction : <Automatic>
618 ** SOUT - serial data out : <Automatic>
619 ** Bool_SPI0 : yes
620 ** Custom name : SPI1
621 ** SPI1 :
622 ** SPI peripheral chip select(output) 0 or slave select(input): <Automatic>
623 ** Direction : <Automatic>
624 ** PCS1 - Peripheral chip select 1 : <Automatic>
625 ** PCS2 - Peripheral chip select 2 : <Automatic>
626 ** PCS3 - Peripheral chip select 3 : <Automatic>
627 ** SIN - Serial data in : <Automatic>
628 ** SCK - Serial clock : <Automatic>
629 ** Direction : <Automatic>
630 ** SOUT - serial data out : <Automatic>
631 ** Bool_SPI1 : yes
632 ** Custom name : SPI2
633 ** SPI2 :
634 ** SPI peripheral chip select(output) 0 or slave select(input): <Automatic>
635 ** Direction : <Automatic>
636 ** SIN - Serial data in : <Automatic>
637 ** SCK - Serial clock : <Automatic>
638 ** Direction : <Automatic>
639 ** SOUT - serial data out : <Automatic>
640 ** Bool_SPI2 : yes
641 ** Peripheral Type SUPPLY :
642 ** SUPPLY :
643 ** Chip power supply : VDD16
644 ** Chip power supply : VDD63
645 ** Chip power supply : VDD78
646 ** Chip power supply : VDD104
647 ** Chip power supply : VDD118
648 ** Chip power supply : VDD132
649 ** Analog power supply : VDDA
650 ** Chip power ground : VSS17
651 ** Chip power ground : VSS64
652 ** Chip power ground : VSS79
653 ** Chip power ground : VSS103
654 ** Chip power ground : VSS117
655 ** Chip power ground : VSS131
656 ** Analog ground : VSSA
657 ** Bool_SUPPLY : yes
658 ** Peripheral Type SysTick :
659 ** Custom name : SysTick
660 ** Peripheral Type TPIU :
661 ** Custom name : TPIU
662 ** TPIU :
663 ** Trace clock output : <Automatic>
664 ** Trace output data 0 : <Automatic>
665 ** Trace output data 1 : <Automatic>
666 ** Trace output data 2 : <Automatic>
667 ** Trace output data 3 : <Automatic>
668 ** Trace data : <Automatic>
669 ** Bool_TPIU : yes
670 ** Peripheral Type TPM :
671 ** Peripheral Type UART :
672 ** Custom name : UART0
673 ** UART0 :
674 ** COL - Collision detect : <Automatic>
675 ** CTS - Clear to send : <Automatic>
676 ** RTS - Request to send : <Automatic>
677 ** RX - Receive data : <Automatic>
678 ** TX - Transmit data : <Automatic>
679 ** UART Tx modulator input : <Automatic>
680 ** Bool_UART0 : yes
681 ** Custom name : UART1
682 ** UART1 :
683 ** CTS - Clear to send : <Automatic>
684 ** RTS - Request to send : <Automatic>
685 ** RX - Receive data : <Automatic>
686 ** TX - Transmit data : <Automatic>
687 ** UART Tx modulator input : <Automatic>
688 ** Bool_UART1 : yes
689 ** Custom name : UART2
690 ** UART2 :
691 ** CTS - Clear to send : <Automatic>
692 ** RTS - Request to send : <Automatic>
693 ** RX - Receive data : <Automatic>
694 ** TX - Transmit data : <Automatic>
695 ** Bool_UART2 : yes
696 ** Custom name : UART3
697 ** UART3 :
698 ** CTS - Clear to send : <Automatic>
699 ** RTS - Request to send : <Automatic>
700 ** RX - Receive data : <Automatic>
701 ** TX - Transmit data : <Automatic>
702 ** Bool_UART3 : yes
703 ** Custom name : UART4
704 ** UART4 :
705 ** CTS - Clear to send : <Automatic>
706 ** RTS - Request to send : <Automatic>
707 ** RX - Receive data : <Automatic>
708 ** TX - Transmit data : <Automatic>
709 ** Bool_UART4 : yes
710 ** Custom name : UART5
711 ** UART5 :
712 ** Bool_UART5 : yes
713 ** Peripheral Type USB :
714 ** Custom name : USB0
715 ** USB0 :
716 ** CLKIN - Alternate Clock : <Automatic>
717 ** DM - Data minus : USB0_DM
718 ** DP - Data plus : USB0_DP
719 ** SOF - Start of frame : <Automatic>
720 ** Regulator output voltage : VOUT33
721 ** Unregulated power supply : VREGIN
722 ** Bool_USB0 : yes
723 ** Peripheral Type USBDCD :
724 ** Custom name : USBDCD
725 ** USBDCD :
726 ** DM - Data minus : USB0_DM
727 ** DP - Data plus : USB0_DP
728 ** Bool_USBDCD : yes
729 ** Peripheral Type VREF :
730 ** Custom name : VREF
731 ** VREF :
732 ** Voltage reference output : VREF_OUT/CMP1_IN5/CMP0_IN5/ADC1_SE18
733 ** Bool_VREF : yes
734 ** Peripheral Type WDOG :
735 ** Custom name : WDOG
736 ** Non-peripheral pins :
737 ** Electrical properties :
738 ** Pin 1: ADC1_SE4a/PTE0/SPI1_PCS1/UART1_TX/SDHC0_D1/TRACE_CLKOUT/I2C1_SDA/RTC_CLKOUT:
739 ** Custom name, Signal name : SD_CARD_DAT1
740 ** Slew rate : <Automatic>
741 ** Open drain : <Automatic>
742 ** Drive strength : <Automatic>
743 ** Passive filter : <Automatic>
744 ** Pull select : <Automatic>
745 ** Pull enable : <Automatic>
746 ** Pin 2: ADC1_SE5a/PTE1/LLWU_P0/SPI1_SOUT/UART1_RX/SDHC0_D0/TRACE_D3/I2C1_SCL/SPI1_SIN:
747 ** Custom name, Signal name : SD_CARD_DAT0
748 ** Slew rate : <Automatic>
749 ** Open drain : <Automatic>
750 ** Drive strength : <Automatic>
751 ** Passive filter : <Automatic>
752 ** Pull select : <Automatic>
753 ** Pull enable : <Automatic>
754 ** Pin 3: ADC0_DP2/ADC1_SE6a/PTE2/LLWU_P1/SPI1_SCK/UART1_CTS_b/SDHC0_DCLK/TRACE_D2:
755 ** Custom name, Signal name : SDHC0_DCLK
756 ** Slew rate : <Automatic>
757 ** Open drain : <Automatic>
758 ** Drive strength : <Automatic>
759 ** Passive filter : <Automatic>
760 ** Pull select : <Automatic>
761 ** Pull enable : <Automatic>
762 ** Pin 4: ADC0_DM2/ADC1_SE7a/PTE3/SPI1_SIN/UART1_RTS_b/SDHC0_CMD/TRACE_D1/SPI1_SOUT:
763 ** Custom name, Signal name : SDHC0_CMD
764 ** Slew rate : <Automatic>
765 ** Open drain : <Automatic>
766 ** Drive strength : <Automatic>
767 ** Passive filter : <Automatic>
768 ** Pull select : <Automatic>
769 ** Pull enable : <Automatic>
770 ** Pin 5: PTE4/LLWU_P2/SPI1_PCS0/UART3_TX/SDHC0_D3/TRACE_D0:
771 ** Custom name, Signal name : SDHC0_D3
772 ** Slew rate : <Automatic>
773 ** Open drain : <Automatic>
774 ** Drive strength : <Automatic>
775 ** Passive filter : <Automatic>
776 ** Pull select : <Automatic>
777 ** Pull enable : <Automatic>
778 ** Pin 6: PTE5/SPI1_PCS2/UART3_RX/SDHC0_D2/FTM3_CH0:
779 ** Custom name, Signal name : SDHC0_D2
780 ** Slew rate : <Automatic>
781 ** Open drain : <Automatic>
782 ** Drive strength : <Automatic>
783 ** Passive filter : <Automatic>
784 ** Pull select : <Automatic>
785 ** Pull enable : <Automatic>
786 ** Pin 7: PTE6/SPI1_PCS3/UART3_CTS_b/I2S0_MCLK/FTM3_CH1/USB_SOF_OUT:
787 ** Custom name, Signal name : SD_CARD_DETECT
788 ** Slew rate : <Automatic>
789 ** Open drain : <Automatic>
790 ** Drive strength : <Automatic>
791 ** Passive filter : <Automatic>
792 ** Pull select : <Automatic>
793 ** Pull enable : <Automatic>
794 ** Pin 8: VDD16 :
795 ** Custom name, Signal name : VDD16
796 ** Pin 9: VSS17 :
797 ** Custom name, Signal name : VSS17
798 ** Pin 10: USB0_DP :
799 ** Custom name, Signal name : USB0_DP
800 ** Pin 11: USB0_DM :
801 ** Custom name, Signal name : USB0_DM
802 ** Pin 12: VOUT33 :
803 ** Custom name, Signal name : VOUT33
804 ** Pin 13: VREGIN :
805 ** Custom name, Signal name : VREGIN
806 ** Pin 14: ADC0_DP1 :
807 ** Custom name, Signal name : ADC0_DP1
808 ** Pin 15: ADC0_DM1 :
809 ** Custom name, Signal name : ADC0_DM1
810 ** Pin 16: ADC1_DP1 :
811 ** Custom name, Signal name : ADC1_DP1
812 ** Pin 17: ADC1_DM1 :
813 ** Custom name, Signal name : ADC1_DM1
814 ** Pin 18: ADC0_DP0/ADC1_DP3 :
815 ** Custom name, Signal name : ADC0_DP0/ADC1_DP3
816 ** Pin 19: ADC0_DM0/ADC1_DM3 :
817 ** Custom name, Signal name : ADC0_DM0/ADC1_DM3
818 ** Pin 20: ADC1_DP0/ADC0_DP3 :
819 ** Custom name, Signal name : ADC1_DP0/ADC0_DP3
820 ** Pin 21: ADC1_DM0/ADC0_DM3 :
821 ** Custom name, Signal name : ADC1_DM0/ADC0_DM3
822 ** Pin 22: VDDA :
823 ** Custom name, Signal name : VDDA
824 ** Pin 23: VREFH :
825 ** Custom name, Signal name : VREFH
826 ** Pin 24: VREFL :
827 ** Custom name, Signal name : VREFL
828 ** Pin 25: VSSA :
829 ** Custom name, Signal name : VSSA
830 ** Pin 26: VREF_OUT/CMP1_IN5/CMP0_IN5/ADC1_SE18:
831 ** Custom name, Signal name : VREF_OUT/CMP1_IN5/CMP0_IN5/ADC1_SE18
832 ** Pin 27: DAC0_OUT/CMP1_IN3/ADC0_SE23 :
833 ** Custom name, Signal name : J26_11
834 ** Pin 28: XTAL32 :
835 ** Custom name, Signal name : XTAL32
836 ** Pin 29: EXTAL32 :
837 ** Custom name, Signal name : EXTAL32
838 ** Pin 30: VBAT :
839 ** Custom name, Signal name : VBAT
840 ** Pin 31: ADC0_SE17/PTE24/UART4_TX/I2C0_SCL/EWM_OUT_b:
841 ** Custom name, Signal name : J2_18/I2C1_SCL
842 ** Slew rate : <Automatic>
843 ** Open drain : <Automatic>
844 ** Drive strength : <Automatic>
845 ** Passive filter : <Automatic>
846 ** Pull select : <Automatic>
847 ** Pull enable : <Automatic>
848 ** Pin 32: ADC0_SE18/PTE25/UART4_RX/I2C0_SDA/EWM_IN:
849 ** Custom name, Signal name : J2_20/I2C1_SDA
850 ** Slew rate : <Automatic>
851 ** Open drain : <Automatic>
852 ** Drive strength : <Automatic>
853 ** Passive filter : <Automatic>
854 ** Pull select : <Automatic>
855 ** Pull enable : <Automatic>
856 ** Pin 33: PTE26/ENET_1588_CLKIN/UART4_CTS_b/RTC_CLKOUT/USB_CLKIN:
857 ** Custom name, Signal name : J2_1/LEDRGB_GREEN
858 ** Slew rate : <Automatic>
859 ** Open drain : <Automatic>
860 ** Drive strength : <Automatic>
861 ** Passive filter : <Automatic>
862 ** Pull select : <Automatic>
863 ** Pull enable : <Automatic>
864 ** Pin 34: PTA0/UART0_CTS_b/UART0_COL_b/FTM0_CH5/JTAG_TCLK/SWD_CLK/EZP_CLK:
865 ** Custom name, Signal name : J2_2/J11_1
866 ** Slew rate : <Automatic>
867 ** Open drain : <Automatic>
868 ** Drive strength : <Automatic>
869 ** Passive filter : <Automatic>
870 ** Pull select : <Automatic>
871 ** Pull enable : <Automatic>
872 ** Pin 35: PTA1/UART0_RX/FTM0_CH6/JTAG_TDI/EZP_DI:
873 ** Custom name, Signal name : J1_8
874 ** Slew rate : <Automatic>
875 ** Open drain : <Automatic>
876 ** Drive strength : <Automatic>
877 ** Passive filter : <Automatic>
878 ** Pull select : <Automatic>
879 ** Pull enable : <Automatic>
880 ** Pin 36: PTA2/UART0_TX/FTM0_CH7/JTAG_TDO/TRACE_SWO/EZP_DO:
881 ** Custom name, Signal name : J1_12
882 ** Slew rate : <Automatic>
883 ** Open drain : <Automatic>
884 ** Drive strength : <Automatic>
885 ** Passive filter : <Automatic>
886 ** Pull select : <Automatic>
887 ** Pull enable : <Automatic>
888 ** Pin 37: PTA3/UART0_RTS_b/FTM0_CH0/JTAG_TMS/SWD_DIO:
889 ** Custom name, Signal name : J9_2/SWD_DIO_TGTMCU/J12_2
890 ** Slew rate : <Automatic>
891 ** Open drain : <Automatic>
892 ** Drive strength : <Automatic>
893 ** Passive filter : <Automatic>
894 ** Pull select : <Automatic>
895 ** Pull enable : <Automatic>
896 ** Pin 38: PTA4/LLWU_P3/FTM0_CH1/NMI_b/EZP_CS_b:
897 ** Custom name, Signal name : BUTTON_SW3/FXOS8700CQ_INT1
898 ** Slew rate : <Automatic>
899 ** Open drain : <Automatic>
900 ** Drive strength : <Automatic>
901 ** Passive filter : <Automatic>
902 ** Pull select : <Automatic>
903 ** Pull enable : <Automatic>
904 ** Pin 39: PTA5/USB_CLKIN/FTM0_CH2/RMII0_RXER/MII0_RXER/CMP2_OUT/I2S0_TX_BCLK/JTAG_TRST_b:
905 ** Custom name, Signal name : RMII0_RXER
906 ** Slew rate : <Automatic>
907 ** Open drain : <Automatic>
908 ** Drive strength : <Automatic>
909 ** Passive filter : <Automatic>
910 ** Pull select : <Automatic>
911 ** Pull enable : <Automatic>
912 ** Pin 40: VDD63 :
913 ** Custom name, Signal name : VDD63
914 ** Pin 41: VSS64 :
915 ** Custom name, Signal name : VSS64
916 ** Pin 42: CMP2_IN0/PTA12/CAN0_TX/FTM1_CH0/RMII0_RXD1/MII0_RXD1/I2C2_SCL/I2S0_TXD0/FTM1_QD_PHA:
917 ** Custom name, Signal name : RMII0_RXD_1
918 ** Slew rate : <Automatic>
919 ** Open drain : <Automatic>
920 ** Drive strength : <Automatic>
921 ** Passive filter : <Automatic>
922 ** Pull select : <Automatic>
923 ** Pull enable : <Automatic>
924 ** Pin 43: CMP2_IN1/PTA13/LLWU_P4/CAN0_RX/FTM1_CH1/RMII0_RXD0/MII0_RXD0/I2C2_SDA/I2S0_TX_FS/FTM1_QD_PHB:
925 ** Custom name, Signal name : RMII0_RXD_0
926 ** Slew rate : <Automatic>
927 ** Open drain : <Automatic>
928 ** Drive strength : <Automatic>
929 ** Passive filter : <Automatic>
930 ** Pull select : <Automatic>
931 ** Pull enable : <Automatic>
932 ** Pin 44: PTA14/SPI0_PCS0/UART0_TX/RMII0_CRS_DV/MII0_RXDV/I2C2_SCL/I2S0_RX_BCLK/I2S0_TXD1:
933 ** Custom name, Signal name : RMII0_CRS_DV
934 ** Slew rate : <Automatic>
935 ** Open drain : <Automatic>
936 ** Drive strength : <Automatic>
937 ** Passive filter : <Automatic>
938 ** Pull select : <Automatic>
939 ** Pull enable : <Automatic>
940 ** Pin 45: PTA15/SPI0_SCK/UART0_RX/RMII0_TXEN/MII0_TXEN/I2S0_RXD0:
941 ** Custom name, Signal name : RMII0_TXEN
942 ** Slew rate : <Automatic>
943 ** Open drain : <Automatic>
944 ** Drive strength : <Automatic>
945 ** Passive filter : <Automatic>
946 ** Pull select : <Automatic>
947 ** Pull enable : <Automatic>
948 ** Pin 46: PTA16/SPI0_SOUT/UART0_CTS_b/UART0_COL_b/RMII0_TXD0/MII0_TXD0/I2S0_RX_FS/I2S0_RXD1:
949 ** Custom name, Signal name : RMII0_TXD_0
950 ** Slew rate : <Automatic>
951 ** Open drain : <Automatic>
952 ** Drive strength : <Automatic>
953 ** Passive filter : <Automatic>
954 ** Pull select : <Automatic>
955 ** Pull enable : <Automatic>
956 ** Pin 47: ADC1_SE17/PTA17/SPI0_SIN/UART0_RTS_b/RMII0_TXD1/MII0_TXD1/I2S0_MCLK:
957 ** Custom name, Signal name : RMII0_TXD_1
958 ** Slew rate : <Automatic>
959 ** Open drain : <Automatic>
960 ** Drive strength : <Automatic>
961 ** Passive filter : <Automatic>
962 ** Pull select : <Automatic>
963 ** Pull enable : <Automatic>
964 ** Pin 48: VDD78 :
965 ** Custom name, Signal name : VDD78
966 ** Pin 49: VSS79 :
967 ** Custom name, Signal name : VSS79
968 ** Pin 50: EXTAL0/PTA18/FTM0_FLT2/FTM_CLKIN0 :
969 ** Custom name, Signal name : RMII_RXCLK
970 ** Slew rate : <Automatic>
971 ** Open drain : <Automatic>
972 ** Drive strength : <Automatic>
973 ** Passive filter : <Automatic>
974 ** Pull select : <Automatic>
975 ** Pull enable : <Automatic>
976 ** Pin 51: XTAL0/PTA19/FTM1_FLT0/FTM_CLKIN1/LPTMR0_ALT1:
977 ** Custom name, Signal name : XTAL_K64_MAIN
978 ** Slew rate : <Automatic>
979 ** Open drain : <Automatic>
980 ** Drive strength : <Automatic>
981 ** Passive filter : <Automatic>
982 ** Pull select : <Automatic>
983 ** Pull enable : <Automatic>
984 ** Pin 52: RESET_b :
985 ** Custom name, Signal name : RST_TGTMCU_B/J14_1/J5_1/J9_10/J25_6
986 ** Pin 53: ADC0_SE8/ADC1_SE8/PTB0/LLWU_P5/I2C0_SCL/FTM1_CH0/RMII0_MDIO/MII0_MDIO/FTM1_QD_PHA:
987 ** Custom name, Signal name : RMII0_MDIO
988 ** Slew rate : <Automatic>
989 ** Open drain : <Automatic>
990 ** Drive strength : <Automatic>
991 ** Passive filter : <Automatic>
992 ** Pull select : <Automatic>
993 ** Pull enable : <Automatic>
994 ** Pin 54: ADC0_SE9/ADC1_SE9/PTB1/I2C0_SDA/FTM1_CH1/RMII0_MDC/MII0_MDC/FTM1_QD_PHB:
995 ** Custom name, Signal name : RMII0_MDC
996 ** Slew rate : <Automatic>
997 ** Open drain : <Automatic>
998 ** Drive strength : <Automatic>
999 ** Passive filter : <Automatic>
1000 ** Pull select : <Automatic>
1001 ** Pull enable : <Automatic>
1002 ** Pin 55: ADC0_SE12/PTB2/I2C0_SCL/UART0_RTS_b/ENET0_1588_TMR0/FTM0_FLT3:
1003 ** Custom name, Signal name : J26_2
1004 ** Slew rate : <Automatic>
1005 ** Open drain : <Automatic>
1006 ** Drive strength : <Automatic>
1007 ** Passive filter : <Automatic>
1008 ** Pull select : <Automatic>
1009 ** Pull enable : <Automatic>
1010 ** Pin 56: ADC0_SE13/PTB3/I2C0_SDA/UART0_CTS_b/UART0_COL_b/ENET0_1588_TMR1/FTM0_FLT0:
1011 ** Custom name, Signal name : J26_4
1012 ** Slew rate : <Automatic>
1013 ** Open drain : <Automatic>
1014 ** Drive strength : <Automatic>
1015 ** Passive filter : <Automatic>
1016 ** Pull select : <Automatic>
1017 ** Pull enable : <Automatic>
1018 ** Pin 57: PTB9/SPI1_PCS1/UART3_CTS_b/FB_AD20 :
1019 ** Custom name, Signal name : J1_6
1020 ** Slew rate : <Automatic>
1021 ** Open drain : <Automatic>
1022 ** Drive strength : <Automatic>
1023 ** Passive filter : <Automatic>
1024 ** Pull select : <Automatic>
1025 ** Pull enable : <Automatic>
1026 ** Pin 58: ADC1_SE14/PTB10/SPI1_PCS0/UART3_RX/FB_AD19/FTM0_FLT1:
1027 ** Custom name, Signal name : J26_6
1028 ** Slew rate : <Automatic>
1029 ** Open drain : <Automatic>
1030 ** Drive strength : <Automatic>
1031 ** Passive filter : <Automatic>
1032 ** Pull select : <Automatic>
1033 ** Pull enable : <Automatic>
1034 ** Pin 59: ADC1_SE15/PTB11/SPI1_SCK/UART3_TX/FB_AD18/FTM0_FLT2:
1035 ** Custom name, Signal name : J26_8
1036 ** Slew rate : <Automatic>
1037 ** Open drain : <Automatic>
1038 ** Drive strength : <Automatic>
1039 ** Passive filter : <Automatic>
1040 ** Pull select : <Automatic>
1041 ** Pull enable : <Automatic>
1042 ** Pin 60: VSS103 :
1043 ** Custom name, Signal name : VSS103
1044 ** Pin 61: VDD104 :
1045 ** Custom name, Signal name : VDD104
1046 ** Pin 62: PTB16/SPI1_SOUT/UART0_RX/FTM_CLKIN0/FB_AD17/EWM_IN:
1047 ** Custom name, Signal name : UART1_RX_TGTMCU
1048 ** Slew rate : <Automatic>
1049 ** Open drain : <Automatic>
1050 ** Drive strength : <Automatic>
1051 ** Passive filter : <Automatic>
1052 ** Pull select : <Automatic>
1053 ** Pull enable : <Automatic>
1054 ** Pin 63: PTB17/SPI1_SIN/UART0_TX/FTM_CLKIN1/FB_AD16/EWM_OUT_b:
1055 ** Custom name, Signal name : UART1_TX_TGTMCU
1056 ** Slew rate : <Automatic>
1057 ** Open drain : <Automatic>
1058 ** Drive strength : <Automatic>
1059 ** Passive filter : <Automatic>
1060 ** Pull select : <Automatic>
1061 ** Pull enable : <Automatic>
1062 ** Pin 64: PTB18/CAN0_TX/FTM2_CH0/I2S0_TX_BCLK/FB_AD15/FTM2_QD_PHA:
1063 ** Custom name, Signal name : J1_1
1064 ** Slew rate : <Automatic>
1065 ** Open drain : <Automatic>
1066 ** Drive strength : <Automatic>
1067 ** Passive filter : <Automatic>
1068 ** Pull select : <Automatic>
1069 ** Pull enable : <Automatic>
1070 ** Pin 65: PTB19/CAN0_RX/FTM2_CH1/I2S0_TX_FS/FB_OE_b/FTM2_QD_PHB:
1071 ** Custom name, Signal name : J1_3
1072 ** Slew rate : <Automatic>
1073 ** Open drain : <Automatic>
1074 ** Drive strength : <Automatic>
1075 ** Passive filter : <Automatic>
1076 ** Pull select : <Automatic>
1077 ** Pull enable : <Automatic>
1078 ** Pin 66: PTB20/SPI2_PCS0/FB_AD31/CMP0_OUT :
1079 ** Custom name, Signal name : J26_9
1080 ** Slew rate : <Automatic>
1081 ** Open drain : <Automatic>
1082 ** Drive strength : <Automatic>
1083 ** Passive filter : <Automatic>
1084 ** Pull select : <Automatic>
1085 ** Pull enable : <Automatic>
1086 ** Pin 67: PTB21/SPI2_SCK/FB_AD30/CMP1_OUT :
1087 ** Custom name, Signal name : LEDRGB_BLUE
1088 ** Slew rate : <Automatic>
1089 ** Open drain : <Automatic>
1090 ** Drive strength : <Automatic>
1091 ** Passive filter : <Automatic>
1092 ** Pull select : <Automatic>
1093 ** Pull enable : <Automatic>
1094 ** Pin 68: PTB22/SPI2_SOUT/FB_AD29/CMP2_OUT :
1095 ** Custom name, Signal name : LEDRGB_RED
1096 ** Slew rate : <Automatic>
1097 ** Open drain : <Automatic>
1098 ** Drive strength : <Automatic>
1099 ** Passive filter : <Automatic>
1100 ** Pull select : <Automatic>
1101 ** Pull enable : <Automatic>
1102 ** Pin 69: PTB23/SPI2_SIN/SPI0_PCS5/FB_AD28 :
1103 ** Custom name, Signal name : J1_10
1104 ** Slew rate : <Automatic>
1105 ** Open drain : <Automatic>
1106 ** Drive strength : <Automatic>
1107 ** Passive filter : <Automatic>
1108 ** Pull select : <Automatic>
1109 ** Pull enable : <Automatic>
1110 ** Pin 70: ADC0_SE14/PTC0/SPI0_PCS4/PDB0_EXTRG/USB_SOF_OUT/FB_AD14/I2S0_TXD1:
1111 ** Custom name, Signal name : J1_11
1112 ** Slew rate : <Automatic>
1113 ** Open drain : <Automatic>
1114 ** Drive strength : <Automatic>
1115 ** Passive filter : <Automatic>
1116 ** Pull select : <Automatic>
1117 ** Pull enable : <Automatic>
1118 ** Pin 71: ADC0_SE15/PTC1/LLWU_P6/SPI0_PCS3/UART1_RTS_b/FTM0_CH0/FB_AD13/I2S0_TXD0:
1119 ** Custom name, Signal name : J1_5
1120 ** Slew rate : <Automatic>
1121 ** Open drain : <Automatic>
1122 ** Drive strength : <Automatic>
1123 ** Passive filter : <Automatic>
1124 ** Pull select : <Automatic>
1125 ** Pull enable : <Automatic>
1126 ** Pin 72: ADC0_SE4b/CMP1_IN0/PTC2/SPI0_PCS2/UART1_CTS_b/FTM0_CH1/FB_AD12/I2S0_TX_FS:
1127 ** Custom name, Signal name : J1_14
1128 ** Slew rate : <Automatic>
1129 ** Open drain : <Automatic>
1130 ** Drive strength : <Automatic>
1131 ** Passive filter : <Automatic>
1132 ** Pull select : <Automatic>
1133 ** Pull enable : <Automatic>
1134 ** Pin 73: CMP1_IN1/PTC3/LLWU_P7/SPI0_PCS1/UART1_RX/FTM0_CH2/CLKOUT/I2S0_TX_BCLK:
1135 ** Custom name, Signal name : J1_16
1136 ** Slew rate : <Automatic>
1137 ** Open drain : <Automatic>
1138 ** Drive strength : <Automatic>
1139 ** Passive filter : <Automatic>
1140 ** Pull select : <Automatic>
1141 ** Pull enable : <Automatic>
1142 ** Pin 74: VSS117 :
1143 ** Custom name, Signal name : VSS117
1144 ** Pin 75: VDD118 :
1145 ** Custom name, Signal name : VDD118
1146 ** Pin 76: PTC4/LLWU_P8/SPI0_PCS0/UART1_TX/FTM0_CH3/FB_AD11/CMP1_OUT:
1147 ** Custom name, Signal name : J2_4
1148 ** Slew rate : <Automatic>
1149 ** Open drain : <Automatic>
1150 ** Drive strength : <Automatic>
1151 ** Passive filter : <Automatic>
1152 ** Pull select : <Automatic>
1153 ** Pull enable : <Automatic>
1154 ** Pin 77: PTC5/LLWU_P9/SPI0_SCK/LPTMR0_ALT2/I2S0_RXD0/FB_AD10/CMP0_OUT/FTM0_CH2:
1155 ** Custom name, Signal name : J1_15
1156 ** Slew rate : <Automatic>
1157 ** Open drain : <Automatic>
1158 ** Drive strength : <Automatic>
1159 ** Passive filter : <Automatic>
1160 ** Pull select : <Automatic>
1161 ** Pull enable : <Automatic>
1162 ** Pin 78: CMP0_IN0/PTC6/LLWU_P10/SPI0_SOUT/PDB0_EXTRG/I2S0_RX_BCLK/FB_AD9/I2S0_MCLK:
1163 ** Custom name, Signal name : BUTTON_SW2
1164 ** Slew rate : <Automatic>
1165 ** Open drain : <Automatic>
1166 ** Drive strength : <Automatic>
1167 ** Passive filter : <Automatic>
1168 ** Pull select : <Automatic>
1169 ** Pull enable : <Automatic>
1170 ** Pin 79: CMP0_IN1/PTC7/SPI0_SIN/USB_SOF_OUT/I2S0_RX_FS/FB_AD8:
1171 ** Custom name, Signal name : J1_13
1172 ** Slew rate : <Automatic>
1173 ** Open drain : <Automatic>
1174 ** Drive strength : <Automatic>
1175 ** Passive filter : <Automatic>
1176 ** Pull select : <Automatic>
1177 ** Pull enable : <Automatic>
1178 ** Pin 80: ADC1_SE4b/CMP0_IN2/PTC8/FTM3_CH4/I2S0_MCLK/FB_AD7:
1179 ** Custom name, Signal name : J1_7
1180 ** Slew rate : <Automatic>
1181 ** Open drain : <Automatic>
1182 ** Drive strength : <Automatic>
1183 ** Passive filter : <Automatic>
1184 ** Pull select : <Automatic>
1185 ** Pull enable : <Automatic>
1186 ** Pin 81: ADC1_SE5b/CMP0_IN3/PTC9/FTM3_CH5/I2S0_RX_BCLK/FB_AD6/FTM2_FLT0:
1187 ** Custom name, Signal name : J1_9
1188 ** Slew rate : <Automatic>
1189 ** Open drain : <Automatic>
1190 ** Drive strength : <Automatic>
1191 ** Passive filter : <Automatic>
1192 ** Pull select : <Automatic>
1193 ** Pull enable : <Automatic>
1194 ** Pin 82: ADC1_SE6b/PTC10/I2C1_SCL/FTM3_CH6/I2S0_RX_FS/FB_AD5:
1195 ** Custom name, Signal name : J26_10
1196 ** Slew rate : <Automatic>
1197 ** Open drain : Enabled
1198 ** Drive strength : <Automatic>
1199 ** Passive filter : <Automatic>
1200 ** Pull select : <Automatic>
1201 ** Pull enable : <Automatic>
1202 ** Pin 83: ADC1_SE7b/PTC11/LLWU_P11/I2C1_SDA/FTM3_CH7/I2S0_RXD1/FB_RW_b:
1203 ** Custom name, Signal name : J26_12
1204 ** Slew rate : <Automatic>
1205 ** Open drain : Enabled
1206 ** Drive strength : <Automatic>
1207 ** Passive filter : <Automatic>
1208 ** Pull select : <Automatic>
1209 ** Pull enable : <Automatic>
1210 ** Pin 84: PTC12/UART4_RTS_b/FB_AD27/FTM3_FLT0:
1211 ** Custom name, Signal name : J6_3
1212 ** Slew rate : <Automatic>
1213 ** Open drain : <Automatic>
1214 ** Drive strength : <Automatic>
1215 ** Passive filter : <Automatic>
1216 ** Pull select : <Automatic>
1217 ** Pull enable : <Automatic>
1218 ** Pin 85: PTC13/UART4_CTS_b/FB_AD26 :
1219 ** Custom name, Signal name : FXOS8700CQ_INT2
1220 ** Slew rate : <Automatic>
1221 ** Open drain : <Automatic>
1222 ** Drive strength : <Automatic>
1223 ** Passive filter : <Automatic>
1224 ** Pull select : <Automatic>
1225 ** Pull enable : <Automatic>
1226 ** Pin 86: PTC14/UART4_RX/FB_AD25 :
1227 ** Custom name, Signal name : J199_3
1228 ** Slew rate : <Automatic>
1229 ** Open drain : <Automatic>
1230 ** Drive strength : <Automatic>
1231 ** Passive filter : <Automatic>
1232 ** Pull select : <Automatic>
1233 ** Pull enable : <Automatic>
1234 ** Pin 87: PTC15/UART4_TX/FB_AD24 :
1235 ** Custom name, Signal name : J199_4
1236 ** Slew rate : <Automatic>
1237 ** Open drain : <Automatic>
1238 ** Drive strength : <Automatic>
1239 ** Passive filter : <Automatic>
1240 ** Pull select : <Automatic>
1241 ** Pull enable : <Automatic>
1242 ** Pin 88: VSS131 :
1243 ** Custom name, Signal name : VSS131
1244 ** Pin 89: VDD132 :
1245 ** Custom name, Signal name : VDD132
1246 ** Pin 90: PTC16/UART3_RX/ENET0_1588_TMR0/FB_CS5_b/FB_TSIZ1/FB_BE23_16_BLS15_8_b:
1247 ** Custom name, Signal name : J1_2
1248 ** Slew rate : <Automatic>
1249 ** Open drain : <Automatic>
1250 ** Drive strength : <Automatic>
1251 ** Passive filter : <Automatic>
1252 ** Pull select : <Automatic>
1253 ** Pull enable : <Automatic>
1254 ** Pin 91: PTC17/UART3_TX/ENET0_1588_TMR1/FB_CS4_b/FB_TSIZ0/FB_BE31_24_BLS7_0_b:
1255 ** Custom name, Signal name : J1_4
1256 ** Slew rate : <Automatic>
1257 ** Open drain : <Automatic>
1258 ** Drive strength : <Automatic>
1259 ** Passive filter : <Automatic>
1260 ** Pull select : <Automatic>
1261 ** Pull enable : <Automatic>
1262 ** Pin 92: PTC18/UART3_RTS_b/ENET0_1588_TMR2/FB_TBST_b/FB_CS2_b/FB_BE15_8_BLS23_16_b:
1263 ** Custom name, Signal name : J6_8
1264 ** Slew rate : <Automatic>
1265 ** Open drain : <Automatic>
1266 ** Drive strength : <Automatic>
1267 ** Passive filter : <Automatic>
1268 ** Pull select : <Automatic>
1269 ** Pull enable : <Automatic>
1270 ** Pin 93: PTD0/LLWU_P12/SPI0_PCS0/UART2_RTS_b/FTM3_CH0/FB_ALE/FB_CS1_b/FB_TS_b:
1271 ** Custom name, Signal name : J2_6
1272 ** Slew rate : <Automatic>
1273 ** Open drain : <Automatic>
1274 ** Drive strength : <Automatic>
1275 ** Passive filter : <Automatic>
1276 ** Pull select : <Automatic>
1277 ** Pull enable : <Automatic>
1278 ** Digital filter : <Automatic>
1279 ** Pin 94: ADC0_SE5b/PTD1/SPI0_SCK/UART2_CTS_b/FTM3_CH1/FB_CS0_b:
1280 ** Custom name, Signal name : J2_12
1281 ** Slew rate : <Automatic>
1282 ** Open drain : <Automatic>
1283 ** Drive strength : <Automatic>
1284 ** Passive filter : <Automatic>
1285 ** Pull select : <Automatic>
1286 ** Pull enable : <Automatic>
1287 ** Digital filter : <Automatic>
1288 ** Pin 95: PTD2/LLWU_P13/SPI0_SOUT/UART2_RX/FTM3_CH2/FB_AD4/I2C0_SCL:
1289 ** Custom name, Signal name : J2_8
1290 ** Slew rate : <Automatic>
1291 ** Open drain : <Automatic>
1292 ** Drive strength : <Automatic>
1293 ** Passive filter : <Automatic>
1294 ** Pull select : <Automatic>
1295 ** Pull enable : <Automatic>
1296 ** Digital filter : <Automatic>
1297 ** Pin 96: PTD3/SPI0_SIN/UART2_TX/FTM3_CH3/FB_AD3/I2C0_SDA:
1298 ** Custom name, Signal name : J2_10
1299 ** Slew rate : <Automatic>
1300 ** Open drain : <Automatic>
1301 ** Drive strength : <Automatic>
1302 ** Passive filter : <Automatic>
1303 ** Pull select : <Automatic>
1304 ** Pull enable : <Automatic>
1305 ** Digital filter : <Automatic>
1306 ** Pin 97: PTD4/LLWU_P14/SPI0_PCS1/UART0_RTS_b/FTM0_CH4/FB_AD2/EWM_IN/SPI1_PCS0:
1307 ** Custom name, Signal name : J6_4
1308 ** Slew rate : <Automatic>
1309 ** Open drain : <Automatic>
1310 ** Drive strength : <Automatic>
1311 ** Passive filter : <Automatic>
1312 ** Pull select : <Automatic>
1313 ** Pull enable : <Automatic>
1314 ** Digital filter : <Automatic>
1315 ** Pin 98: ADC0_SE6b/PTD5/SPI0_PCS2/UART0_CTS_b/UART0_COL_b/FTM0_CH5/FB_AD1/EWM_OUT_b/SPI1_SCK:
1316 ** Custom name, Signal name : J6_5
1317 ** Slew rate : <Automatic>
1318 ** Open drain : <Automatic>
1319 ** Drive strength : <Automatic>
1320 ** Passive filter : <Automatic>
1321 ** Pull select : <Automatic>
1322 ** Pull enable : <Automatic>
1323 ** Digital filter : <Automatic>
1324 ** Pin 99: ADC0_SE7b/PTD6/LLWU_P15/SPI0_PCS3/UART0_RX/FTM0_CH6/FB_AD0/FTM0_FLT0/SPI1_SOUT:
1325 ** Custom name, Signal name : J6_6
1326 ** Slew rate : <Automatic>
1327 ** Open drain : <Automatic>
1328 ** Drive strength : <Automatic>
1329 ** Passive filter : <Automatic>
1330 ** Pull select : <Automatic>
1331 ** Pull enable : <Automatic>
1332 ** Digital filter : <Automatic>
1333 ** Pin 100: PTD7/CMT_IRO/UART0_TX/FTM0_CH7/FTM0_FLT1/SPI1_SIN:
1334 ** Custom name, Signal name : J6_7
1335 ** Slew rate : <Automatic>
1336 ** Open drain : <Automatic>
1337 ** Drive strength : <Automatic>
1338 ** Passive filter : <Automatic>
1339 ** Pull select : <Automatic>
1340 ** Pull enable : <Automatic>
1341 ** Digital filter : <Automatic>
1342 ** Settings :
1343 ** Clock gates initialization mode : SIM HAL (fsl_sim_hal component)
1344 ** Inherited HAL components :
1345 ** fsl_port_hal : fsl_port_hal
1346 ** fsl_sim_hal : fsl_sim_hal
1347 ** fsl_mcg_hal : fsl_mcg_hal
1348 **
1349 ** Copyright : 1997 - 2015 Freescale Semiconductor, Inc.
1350 ** All Rights Reserved.
1351 **
1352 ** Redistribution and use in source and binary forms, with or without modification,
1353 ** are permitted provided that the following conditions are met:
1354 **
1355 ** o Redistributions of source code must retain the above copyright notice, this list
1356 ** of conditions and the following disclaimer.
1357 **
1358 ** o Redistributions in binary form must reproduce the above copyright notice, this
1359 ** list of conditions and the following disclaimer in the documentation and/or
1360 ** other materials provided with the distribution.
1361 **
1362 ** o Neither the name of Freescale Semiconductor, Inc. nor the names of its
1363 ** contributors may be used to endorse or promote products derived from this
1364 ** software without specific prior written permission.
1365 **
1366 ** THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS" AND
1367 ** ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED
1368 ** WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE
1369 ** DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT HOLDER OR CONTRIBUTORS BE LIABLE FOR
1370 ** ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES
1371 ** (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES;
1372 ** LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON
1373 ** ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
1374 ** (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
1375 ** SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
1376 **
1377 ** http: www.freescale.com
1378 ** mail: support@freescale.com
1379 ** ###################################################################*/
1380 /*!
1381 ** @file pin_init.c
1382 ** @version 1.4
1383 ** @brief
1384 **
1385 */
1386 /*!
1387 ** @addtogroup pin_init_module pin_init module documentation
1388 ** @{
1389 */
1390
1391 #include "fsl_device_registers.h"
1392 #include "board.h"
1393 #include "fsl_sim_hal.h"
1394 #include "fsl_mcg_hal.h"
1395
1396
1397 void hardware_init(void) {
1398
1399 /* Enable clock for PORTs */
1400 SIM_HAL_EnableClock(SIM,kSimClockGatePortC);
1401 SIM_HAL_EnableClock(SIM,kSimClockGatePortA);
1402 SIM_HAL_EnableClock(SIM,kSimClockGatePortB);
1403 SIM_HAL_EnableClock(SIM,kSimClockGatePortD);
1404
1405 /* Setup board clock source. */
1406 g_xtal0ClkFreq = 50000000U; /* Value of the external crystal or oscillator clock frequency of the system oscillator (OSC) in Hz */
1407 g_xtalRtcClkFreq = 32768U; /* Value of the external 32k crystal or oscillator clock frequency of the RTC in Hz */
1408
1409 init_adc_pins(ADC0_IDX);
1410 init_cmp_pins(CMP1_IDX);
1411 init_enet_pins(ENET_IDX);
1412 init_gpio_pins(PORTA_IDX);
1413 init_gpio_pins(PORTB_IDX);
1414 init_gpio_pins(PORTC_IDX);
1415 init_i2c_pins(I2C1_IDX);
1416 init_jtag_pins(JTAG_IDX);
1417 init_llwu_pins(LLWU_IDX);
1418 init_osc_pins(OSC_IDX);
1419 init_spi_pins(SPI0_IDX);
1420 init_tpiu_pins(TPIU_IDX);
1421 init_uart_pins(UART0_IDX);
1422 init_uart_pins(UART1_IDX);
1423 }
1424
1425 /*!
1426 ** @}
1427 */
1428 /*
1429 ** ###################################################################
1430 **
1431 ** This file was created by Processor Expert 10.5 [05.21]
1432 ** for the Freescale Kinetis series of microcontrollers.
1433 **
1434 ** ###################################################################
1435 */
init_jtag_pins
void init_jtag_pins(uint32_t instance)
JTAG method sets registers according routing settings. Call this method code to route desired pins in...
Definition: pin_init.c:1613
init_gpio_pins
void init_gpio_pins(uint32_t instance)
GPIO method sets registers according routing settings. Call this method code to route desired pins in...
Definition: pin_init.c:1494
init_uart_pins
void init_uart_pins(uint32_t instance)
UART method sets registers according routing settings. Call this method code to route desired pins in...
Definition: pin_init.c:1751
init_osc_pins
void init_osc_pins(uint32_t instance)
OSC method sets registers according routing settings. Call this method code to route desired pins int...
Definition: pin_init.c:1669
init_i2c_pins
void init_i2c_pins(uint32_t instance)
I2C method sets registers according routing settings. Call this method code to route desired pins int...
Definition: pin_init.c:1574
init_cmp_pins
void init_cmp_pins(uint32_t instance)
CMP method sets registers according routing settings. Call this method code to route desired pins int...
Definition: pin_init.c:1439
init_adc_pins
void init_adc_pins(uint32_t instance)
ADC method sets registers according routing settings. Call this method code to route desired pins int...
Definition: pin_init.c:1406
init_enet_pins
void init_enet_pins(uint32_t instance)
ENET method sets registers according routing settings. Call this method code to route desired pins in...
Definition: pin_init.c:1473
hardware_init
void hardware_init(void)
Definition: hardware_init.c:1397
init_llwu_pins
void init_llwu_pins(uint32_t instance)
LLWU method sets registers according routing settings. Call this method code to route desired pins in...
Definition: pin_init.c:1644
init_tpiu_pins
void init_tpiu_pins(uint32_t instance)
TPIU method sets registers according routing settings. Call this method code to route desired pins in...
Definition: pin_init.c:1730
board.h
init_spi_pins
void init_spi_pins(uint32_t instance)
SPI method sets registers according routing settings. Call this method code to route desired pins int...
Definition: pin_init.c:1690
- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.