| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
qr_config_t Struct Reference

This structure holds the quick read configuration for all
applicable mailboxes. The first 4 mailboxes are used for the
command packet read/write. All other mailboxes can be configured
as quick read. More...

`#include <ci_protocol_mbox.h>`

Collaboration diagram for qr_config_t:

## Data Fields
uint8 | appId
uint8 | byte_id

## Detailed Description

This structure holds the quick read configuration for all
applicable mailboxes. The first 4 mailboxes are used for the
command packet read/write. All other mailboxes can be configured
as quick read.

Note that this structure must be 2 bytes per Eve's command interpreter
spec.

Definition at line 186 of file ci_protocol_mbox.h.

## Field Documentation

uint8 appId

Definition at line 188 of file ci_protocol_mbox.h.

Referenced by ci_mbox_init(), ci_qr_update(), ci_update_first_data_mb(), and isf_ci_qr_update().

uint8 byte_id

Definition at line 189 of file ci_protocol_mbox.h.

Referenced by ci_mbox_init(), and isf_ci_qr_update().

The documentation for this struct was generated from the following file:

- ISF/Command_Interpreter/Include/ci_protocol_mbox.h

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.