| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

Enumerations | Variables
OutY module documentation

## Enumerations
enum | _OutY_pinNames { J1_5 = GPIO_MAKE_PIN(GPIOC_IDX, 1U) }
| Pin names. More...

## Variables
const gpio_input_pin_user_config_t | OutY_OutConfig0 []
| Configuration structure 0 for input pins. More...
const gpio_input_pin_user_config_t | OutY_OutConfig0 []
| Configuration structure 0 for input pins. More...

## Detailed Description

## Enumeration Type Documentation

enum _OutY_pinNames

Pin names.

Enumerator
J1_5 |

Definition at line 81 of file OutY.h.

## Variable Documentation

const gpio_input_pin_user_config_t OutY_OutConfig0[]

Initial value:
= {
{
.pinName = J1_5,
.config.isPullEnable = false,
.config.pullSelect = kPortPullDown,
.config.isPassiveFilterEnabled = false,
.config.isDigitalFilterEnabled = true,
.config.interrupt = kPortIntDisabled
},
{
.pinName = GPIO_PINS_OUT_OF_RANGE,
}
}
J1_5
Definition: OutX.h:82

Configuration structure 0 for input pins.

Definition at line 56 of file OutY.c.

Referenced by Components_Init().

const gpio_input_pin_user_config_t OutY_OutConfig0[]

Configuration structure 0 for input pins.

Definition at line 56 of file OutY.c.

Referenced by Components_Init().

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.