| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
ci_app_resp_packet_t Struct Reference

This structure enables an application to read from or write to the host. More...

`#include <isf_ci.h>`

Collaboration diagram for ci_app_resp_packet_t:

## Data Fields
ci_rw_enum | rw
uint8 | bytes_xfer
uint8 | bytes_left

## Detailed Description

This structure enables an application to read from or write to the host.

This structure is updated by the application's CI callback as a result of handling a command from the host.

Definition at line 221 of file isf_ci.h.

## Field Documentation

uint8 bytes_left

Number of bytes left to read from or write to the host via the mailboxes.

Definition at line 238 of file isf_ci.h.

Referenced by ci_protocol_CB_mbox(), isf_app_callback_dev_info(), and isf_app_callback_mbox().

uint8 bytes_xfer

Number of bytes actually read from or written to the host via the mailboxes.

Definition at line 233 of file isf_ci.h.

Referenced by App1_ci_app_callback(), BasicApp1_CI_Callback(), ci_protocol_CB_mbox(), isf_app_callback_dev_info(), isf_app_callback_mbox(), and rli_ci_app_callback().

ci_rw_enum rw

Application read from or write to the host:

- CI_RW_READ - application reads from the host.
- CI_RW_WRITE - application writes to the host.

Definition at line 228 of file isf_ci.h.

Referenced by ci_protocol_CB_mbox(), isf_app_callback_dev_info(), isf_app_callback_mbox(), and rli_ci_app_callback().

The documentation for this struct was generated from the following file:

- ISF/Core/Include/isf_ci.h

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.