| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

Enumerations | Variables
SPIChipSelect module documentation

## Enumerations
enum | _SPIChipSelect_pinNames { J1_13 = GPIO_MAKE_PIN(GPIOC_IDX, 7U) }
| Pin names. More...

## Variables
const gpio_output_pin_user_config_t | ChipSelect_OutConfig0 []
| Configuration structure 0 for output pins. More...
const gpio_output_pin_user_config_t | ChipSelect_OutConfig0 []
| Configuration structure 0 for output pins. More...

## Detailed Description

## Enumeration Type Documentation

enum _SPIChipSelect_pinNames

Pin names.

Enumerator
J1_13 |

Definition at line 81 of file SPIChipSelect.h.

## Variable Documentation

const gpio_output_pin_user_config_t ChipSelect_OutConfig0[]

Initial value:
= {
{
.pinName = J1_13,
.config.outputLogic = 1,
.config.slewRate = kPortSlowSlewRate,
.config.isOpenDrainEnabled = false,
.config.driveStrength = kPortLowDriveStrength,
},
{
.pinName = GPIO_PINS_OUT_OF_RANGE,
}
}
J1_13
Definition: SPIChipSelect.h:82

Configuration structure 0 for output pins.

Definition at line 56 of file SPIChipSelect.c.

const gpio_output_pin_user_config_t ChipSelect_OutConfig0[]

Configuration structure 0 for output pins.

Definition at line 56 of file ChipSelect.c.

Referenced by Components_Init(), fsl_95000_spi_slave_init(), and fsl_955x_spi_slave_init().

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.