| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

Functions
pin_init.c File Reference
`#include "fsl_device_registers.h"`
`#include "fsl_port_hal.h"`
`#include "fsl_sim_hal.h"`
`#include "pin_init.h"`
Include dependency graph for pin_init.c:

Go to the source code of this file.

## Functions
void | init_adc_pins (uint32_t instance)
| ADC method sets registers according routing settings. Call this method code to route desired pins into: ADC0, ADC1 peripherals. More...
void | deinit_adc_pins (uint32_t instance)
| ADC method sets registers according routing settings. Call this method code to disable routing of desired pins for: ADC0, ADC1 peripherals. More...
void | init_cmp_pins (uint32_t instance)
| CMP method sets registers according routing settings. Call this method code to route desired pins into: CMP0, CMP1, CMP2 peripherals. More...
void | deinit_cmp_pins (uint32_t instance)
| CMP method sets registers according routing settings. Call this method code to disable routing of desired pins for: CMP0, CMP1, CMP2 peripherals. More...
void | init_enet_pins (uint32_t instance)
| ENET method sets registers according routing settings. Call this method code to route desired pins into ENET periphery. More...
void | deinit_enet_pins (uint32_t instance)
| ENET method sets registers according routing settings. Call this method code to disable routing of desired pins for ENET periphery. More...
void | init_gpio_pins (uint32_t instance)
| GPIO method sets registers according routing settings. Call this method code to route desired pins into: PTA, PTB, PTC, PTD, PTE peripherals. More...
void | deinit_gpio_pins (uint32_t instance)
| GPIO method sets registers according routing settings. Call this method code to disable routing of desired pins for: PTA, PTB, PTC, PTD, PTE peripherals. More...
void | init_i2c_pins (uint32_t instance)
| I2C method sets registers according routing settings. Call this method code to route desired pins into: I2C0, I2C1, I2C2 peripherals. More...
void | deinit_i2c_pins (uint32_t instance)
| I2C method sets registers according routing settings. Call this method code to disable routing of desired pins for: I2C0, I2C1, I2C2 peripherals. More...
void | init_jtag_pins (uint32_t instance)
| JTAG method sets registers according routing settings. Call this method code to route desired pins into JTAG periphery. More...
void | deinit_jtag_pins (uint32_t instance)
| JTAG method sets registers according routing settings. Call this method code to disable routing of desired pins for JTAG periphery. More...
void | init_llwu_pins (uint32_t instance)
| LLWU method sets registers according routing settings. Call this method code to route desired pins into LLWU periphery. More...
void | deinit_llwu_pins (uint32_t instance)
| LLWU method sets registers according routing settings. Call this method code to disable routing of desired pins for LLWU periphery. More...
void | init_osc_pins (uint32_t instance)
| OSC method sets registers according routing settings. Call this method code to route desired pins into OSC periphery. More...
void | deinit_osc_pins (uint32_t instance)
| OSC method sets registers according routing settings. Call this method code to disable routing of desired pins for OSC periphery. More...
void | init_spi_pins (uint32_t instance)
| SPI method sets registers according routing settings. Call this method code to route desired pins into: SPI0, SPI1, SPI2 peripherals. More...
void | deinit_spi_pins (uint32_t instance)
| SPI method sets registers according routing settings. Call this method code to disable routing of desired pins for: SPI0, SPI1, SPI2 peripherals. More...
void | init_tpiu_pins (uint32_t instance)
| TPIU method sets registers according routing settings. Call this method code to route desired pins into TPIU periphery. More...
void | deinit_tpiu_pins (uint32_t instance)
| TPIU method sets registers according routing settings. Call this method code to disable routing of desired pins for TPIU periphery. More...
void | init_uart_pins (uint32_t instance)
| UART method sets registers according routing settings. Call this method code to route desired pins into: UART0, UART1, UART2, UART3, UART4, UART5 peripherals. More...
void | deinit_uart_pins (uint32_t instance)
| UART method sets registers according routing settings. Call this method code to disable routing of desired pins for: UART0, UART1, UART2, UART3, UART4, UART5 peripherals. More...

## Detailed Description

Version
  1.4

Definition in file pin_init.c.

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.