| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

Macros | Variables
FXOS8700_1 module documentation

## Macros
#define | FXOS8700_1_DATA_TYPE fxos8700_DataBuffer_t

## Variables
fxos8700_Sensor_Specific_Settings_t | FXOS8700_1_Sensor_Specific_Config
| This allows access to the sensor specific configuration for the target sensor. More...
const isf_dsa_Adapter_t | FXOS8700_1_Adapter
| This creates the sensor adapter instance for the target sensor. More...
const i2c_device_t | FXOS8700_1_DeviceInfo
| This allows access to the sensor communications specific configuration. More...
fxos8700_Sensor_Specific_Settings_t | FXOS8700_1_Sensor_Specific_Config
| This allows access to the sensor specific configuration for the target sensor. More...
const isf_dsa_Adapter_t | FXOS8700_1_Adapter
| This allows access to the sensor adapter instance for the target sensor. More...
const i2c_device_t | FXOS8700_1_DeviceInfo
| This allows access to the sensor communications specific configuration. More...

## Detailed Description

## Macro Definition Documentation

#define FXOS8700_1_DATA_TYPE fxos8700_DataBuffer_t

Definition at line 102 of file FXOS8700_1.h.

## Variable Documentation

const isf_dsa_Adapter_t FXOS8700_1_Adapter

This allows access to the sensor adapter instance for the target sensor.

This allows access to the sensor adapter instance for the target sensor.

Definition at line 142 of file FXOS8700_1.c.

const isf_dsa_Adapter_t FXOS8700_1_Adapter

Initial value:
=
{
.devInfo.pSupportedSensorTypes = fxos8700_SupportedSensorTypes,
.devInfo.pSupportedSensorDataTypes = fxos8700_SupportedDataTypes,
.devInfo.nNativeDataSetSize = sizeof(fxos8700_DataBuffer_t),
.control.Initialize = &fsl_fxos8700_i2cspi_6D_AccMag_Initialize,
.control.ValidateSettings = &fsl_fxos8700_i2cspi_6D_AccMag_ValidateSettings,
.control.Configure = &fsl_fxos8700_i2cspi_6D_AccMag_Configure,
.control.StartData = &fsl_fxos8700_i2cspi_6D_AccMag_StartData,
.control.EndData = &fsl_fxos8700_i2cspi_6D_AccMag_EndData,
.control.Calibrate = &fsl_fxos8700_i2cspi_6D_AccMag_Calibrate,
.control.Shutdown = &fsl_fxos8700_i2cspi_6D_AccMag_Shutdown,
.control.Convert = &fsl_fxos8700_i2cspi_6D_AccMag_Convert
}
fxos8700_DataBuffer_t
This structure defines the dummy DSA data buffer format.
Definition: fsl_fxos8700_i2cspi_6D_AccMag.h:104
fsl_fxos8700_i2cspi_6D_AccMag_Initialize
isf_dsa_status_t fsl_fxos8700_i2cspi_6D_AccMag_Initialize(isf_SensorHandle_t *pSensorHandle)
This is the concrete implementation of the FXOS8700 sensor adapter initialization.
Definition: fsl_fxos8700_i2cspi_6D_AccMag.c:151
fxos8700_SupportedSensorTypes
isf_SensorTypes_t fxos8700_SupportedSensorTypes[]
Supported sensor and data types for FXOS8700.
Definition: fsl_fxos8700_i2cspi_6D_AccMag.c:53
fsl_fxos8700_i2cspi_6D_AccMag_Configure
isf_dsa_status_t fsl_fxos8700_i2cspi_6D_AccMag_Configure(isf_SensorHandle_t *pSensorHandle, isf_dsa_SensorSettings_t *pSensorSettings)
This is the concrete implementation of the FXOS8700 sensor adapter for configuration.
Definition: fsl_fxos8700_i2cspi_6D_AccMag.c:282
fsl_fxos8700_i2cspi_6D_AccMag_StartData
isf_dsa_status_t fsl_fxos8700_i2cspi_6D_AccMag_StartData(isf_SensorHandle_t *pSensorHandle)
This is the concrete implementation of the FXOS8700 sensor adapter for start Data.
Definition: fsl_fxos8700_i2cspi_6D_AccMag.c:411
fsl_fxos8700_i2cspi_6D_AccMag_Calibrate
isf_dsa_status_t fsl_fxos8700_i2cspi_6D_AccMag_Calibrate(isf_SensorHandle_t *pSensorHandle, void *pCalData)
This is the concrete implementation of the FXOS8700 sensor adapter for calibration ...
Definition: fsl_fxos8700_i2cspi_6D_AccMag.c:544
fsl_fxos8700_i2cspi_6D_AccMag_Convert
isf_dsa_status_t fsl_fxos8700_i2cspi_6D_AccMag_Convert(volatile isf_SensorHandle_t *pSensorHandle, isf_SensorDataTypes_t convertToType, isf_dsa_result_types_t resultType, void *pNativeSample, void *pConvertedSample, int32 *numBytes)
This function coverts the raw sample data to the desired output type.
Definition: fsl_fxos8700_i2cspi_6D_AccMag.c:735
fxos8700_SupportedDataTypes
isf_SensorDataTypes_t fxos8700_SupportedDataTypes[]
Definition: fsl_fxos8700_i2cspi_6D_AccMag.c:54
fsl_fxos8700_i2cspi_6D_AccMag_Shutdown
isf_dsa_status_t fsl_fxos8700_i2cspi_6D_AccMag_Shutdown(isf_SensorHandle_t *pSensorHandle)
This is the concrete implementation of the FXOS8700 sensor adapter for shutdown . ...
Definition: fsl_fxos8700_i2cspi_6D_AccMag.c:561
fsl_fxos8700_i2cspi_6D_AccMag_EndData
isf_dsa_status_t fsl_fxos8700_i2cspi_6D_AccMag_EndData(isf_SensorHandle_t *pSensorHandle)
This is the concrete implementation of the FXOS8700 sensor adapter for End Data.
Definition: fsl_fxos8700_i2cspi_6D_AccMag.c:478
fsl_fxos8700_i2cspi_6D_AccMag_ValidateSettings
isf_dsa_status_t fsl_fxos8700_i2cspi_6D_AccMag_ValidateSettings(isf_SensorHandle_t *pSensorHandle, isf_dsa_SensorSettings_t *pSensorSettings)
This is the concrete implementation of the FXOS8700 sensor adapter for validating current settings...
Definition: fsl_fxos8700_i2cspi_6D_AccMag.c:241

This creates the sensor adapter instance for the target sensor.

This allows access to the sensor adapter instance for the target sensor.

Definition at line 142 of file FXOS8700_1.c.

const i2c_device_t FXOS8700_1_DeviceInfo

This allows access to the sensor communications specific configuration.

This allows access to the sensor communications specific configuration.

Definition at line 157 of file FXOS8700_1.c.

const i2c_device_t FXOS8700_1_DeviceInfo

Initial value:
=
{
.baudRate_kbps = 400,
.address = 30
}

This allows access to the sensor communications specific configuration.

This allows access to the sensor communications specific configuration.

Definition at line 157 of file FXOS8700_1.c.

fxos8700_Sensor_Specific_Settings_t FXOS8700_1_Sensor_Specific_Config

This allows access to the sensor specific configuration for the target sensor.

Definition at line 90 of file FXOS8700_1.c.

fxos8700_Sensor_Specific_Settings_t FXOS8700_1_Sensor_Specific_Config

This allows access to the sensor specific configuration for the target sensor.

Definition at line 90 of file FXOS8700_1.c.

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.