| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

Data Structures | Macros | Typedefs | Enumerations | Functions
fsl_Sensor_Analog_1_Functions.h File Reference

This is user's event module. Put your event handler code here. More...

`#include "fsl_device_registers.h"`
`#include "clockMan1.h"`
`#include "pin_init.h"`
`#include "osa1.h"`
`#include "mqx_ksdk.h"`
`#include "uart1.h"`
`#include "fsl_mpu1.h"`
`#include "fsl_hwtimer1.h"`
`#include "MainTask.h"`
`#include "I2C1.h"`
`#include "ISF_I2C1.h"`
`#include "UART2.h"`
`#include "ISF_UART1.h"`
`#include "SPI1.h"`
`#include "ISF_SPI1.h"`
`#include "ISFCore1.h"`
`#include "ISFBusManager1.h"`
`#include "BMTIMER1.h"`
`#include "EventHandler_Task1.h"`
`#include "CommChannelConfig1.h"`
`#include "Protocol1.h"`
`#include "App1.h"`
`#include "BasicApp1.h"`
`#include "RLI1.h"`
`#include "RLIChipSelect.h"`
`#include "Custom_1.h"`
`#include "FXAS21002_1.h"`
`#include "FXAS21002_2.h"`
`#include "ChipSelect.h"`
`#include "FXLC95000_1.h"`
`#include "FXLC95000_2.h"`
`#include "SPIChipSelect.h"`
`#include "SPISelect.h"`
`#include "ResetSensor.h"`
`#include "FXLS8471_1.h"`
`#include "FXLS8952_1.h"`
`#include "FXLS8471_2.h"`
`#include "FXOS8700_1.h"`
`#include "FXOS8700_2.h"`
`#include "Analog_1.h"`
`#include "ADC1.h"`
`#include "MAG3110_1.h"`
`#include "MMA8491Q_1.h"`
`#include "SensorEnable.h"`
`#include "OutX.h"`
`#include "OutY.h"`
`#include "OutZ.h"`
`#include "MMA865x_1.h"`
`#include "MMA955x_1.h"`
`#include "MMA955x_2.h"`
`#include "MPL3115_1.h"`
`#include "ORIENT_1.h"`
`#include "SensorReset.h"`
`#include "isf_devmsg.h"`
`#include "isf_sensors.h"`
`#include "isf_dsa_adapter.h"`
`#include "isf_sensor_types.h"`
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Data Structures
struct | Analog_1_device_t
| This structure stores sample Information necessary to communicate with non I2C slave device. More...
struct | Analog_1_DataBuffer_t
| This structure defines the dummy DSA data buffer format. More...
struct | Analog_1_SensorData_Fixed_t
struct | Analog_1_SensorData_Float_t
| Standard fixed type for three axis accelerometers. More...
struct | Analog_1_Sensor_Specific_Settings_t

## Macros
#define | __fsl_Sensor_Analog_1_Functions_H_
#define | MAX_ADC_CHANNELS 6
#define | Analog_1_DATA_TYPE Analog_1_DataBuffer_t
#define | __fsl_Sensor_Analog_1_Functions_H__
#define | Analog_1_SET_FIELD(name, val) (((val)<<Analog_1_##name##_SHIFT)&(Analog_1_##name##_MASK))
#define | Analog_1_GET_FIELD(name, val) ((val&Analog_1_##name##_MASK)>>Analog_1_##name##_SHIFT)

## Typedefs
typedef int32 | Analog_1_Status_t
| SENSOR internal return codes. More...
typedef int32 | isf_Analog_1_fixed_data_t
typedef float | isf_Analog_1_float_data_t

## Enumerations
enum | { Analog_1_SUCCESS, Analog_1_DATA_OVERWRITE, Analog_1_ERROR }

## Functions
void | Analog_1__Void_ ()
isf_dsa_status_t | Analog_1_float_converter (Analog_1_Sensor_Specific_Settings_t *pSensorSpecificConfig, Analog_1_DataBuffer_t *nativeSample, void *vpConvertedSample)
isf_dsa_status_t | Analog_1_fixed_converter (Analog_1_Sensor_Specific_Settings_t *pSensorSpecificConfig, Analog_1_DataBuffer_t *nativeSample, void *vpConvertedSample)
isf_dsa_status_t | fsl_Sensor_Analog_1_Convert (isf_SensorHandle_t *pSensorHandle, isf_SensorDataTypes_t convertToType, isf_dsa_result_types_t resultType, void *pNativeSample, void *pConvertedSample, int32_t *numBytes)
isf_dsa_status_t | fsl_Sensor_Analog_1_Initialize (isf_SensorHandle_t *pSensorHandle)
isf_dsa_status_t | fsl_Sensor_Analog_1_ValidateSettings (isf_SensorHandle_t *pSensorHandle, isf_dsa_SensorSettings_t *pSensorSettings)
isf_dsa_status_t | fsl_Sensor_Analog_1_Configure (isf_SensorHandle_t *pSensorHandle, isf_dsa_SensorSettings_t *pSensorSettings)
isf_dsa_status_t | fsl_Sensor_Analog_1_StartData (isf_SensorHandle_t *pSensorHandle)
isf_dsa_status_t | fsl_Sensor_Analog_1_EndData (isf_SensorHandle_t *pSensorHandle)
isf_dsa_status_t | fsl_Sensor_Analog_1_Shutdown (isf_SensorHandle_t *pSensorHandle)
void | Analog_1_fsl_Sensor_Generic_Analog_Convert (void *pSensorHandle, uint32_t convertToType, uint8_t resultType, void *pNativeSample, void *pConvertedSample, int32_t *numBytes, int8_t *retValue)
void | Analog_1_fsl_Sensor_Generic_AnalogCallback (void *pSensorHandle)
void | Analog_1_fsl_Sensor_Generic_Analog_Shutdown (void *pSensorHandle, int8_t *retValue)
void | Analog_1_fsl_Sensor_Generic_Analog_EndData (void *pSensorHandle, int8_t *retValue)
void | Analog_1_fsl_Sensor_Generic_Analog_StartData (void *pSensorHandle, int8_t *retValue)
void | Analog_1_fsl_Sensor_Generic_Analog_Configure (void *pSensorHandle, void *pSensorSettings, int8_t *retValue)
void | Analog_1_fsl_Sensor_Generic_Analog_ValidateSettings (void *pSensorHandle, void *pSensorSettings, int8_t *retValue)
void | Analog_1_fsl_Sensor_Generic_Analog_Initialize (void *pSensorHandle, int8_t *retValue)

## Detailed Description

This is user's event module. Put your event handler code here.

Version
  01.00

Definition in file fsl_Sensor_Analog_1_Functions.h.

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.