| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

Macros | Variables
MMA8491Q_1.h File Reference
`#include "I2C1.h"`
`#include "SensorEnable.h"`
`#include "OutX.h"`
`#include "OutY.h"`
`#include "OutZ.h"`
`#include <isf_sensor_types.h>`
`#include <isf_fifo.h>`
`#include <isf_accelerometer_types.h>`
`#include "mma8491q.h"`
`#include "fsl_mma8491q_i2c_3D_accel.h"`
`#include "fsl_i2c_master_driver.h"`
`#include "Cpu.h"`
Include dependency graph for MMA8491Q_1.h:
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Macros
#define | MMA8491Q_1_DATA_TYPE mma8491q_DataBuffer_t

## Variables
mma8491q_Sensor_Specific_Settings_t | MMA8491Q_1_Sensor_Specific_Config
| This allows access to the sensor specific configuration for the target sensor. More...
const isf_dsa_Adapter_t | MMA8491Q_1_Adapter
| This allows access to the sensor adapter instance for the target sensor. More...
const i2c_device_t | MMA8491Q_1_DeviceInfo
| This allows access to the sensor communications specific configuration. More...

## Detailed Description

Version
  01.00

Definition in file MMA8491Q_1.h.

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.