| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

Macros | Functions | Variables
RLI1.c File Reference
`#include "RLI1.h"`
`#include "isf_util.h"`
`#include "fsl_gpio_driver.h"`
`#include "isf_spi_master_types.h"`
Include dependency graph for RLI1.c:

Go to the source code of this file.

## Macros
#define | RLI1_TASK_NAME "RLI1_task"
#define | RLI1_TASK_STACK_SIZE 1280
#define | RLI1_TASK_PRIORITY 12

## Functions
| OSA_TASK_DEFINE (RLI1, RLI1_TASK_STACK_SIZE)
void | rli_app_task (void)
void | RLI1_MainTask (os_task_param_t task_init_data)
void | RLI1_init (void)
isf_status_t | rli_spi_slave_init (void)
isf_status_t | rli_spi_slave_write_preprocess (void *pCmdOut, uint32 offset, uint32 size, void *pWritebuffer)
isf_status_t | rli_spi_slave_write_postprocess (void *pCmdOut)
isf_status_t | rli_spi_slave_read_preprocess (void *pCmdOut, uint32 offset, uint32 size)
isf_status_t | rli_spi_slave_read_postprocess (void *pCmdOut, void *pDataOut)
spi_master_CommSpecificInfo_t | rli_spi_get_config (uint16 spiAddress)

## Variables
spi_master_slaveInfo_t | rli_spi_sensor_type
gpio_output_pin_user_config_t | gpioX_OutConfig0 []
const spi_master_CommSpecificInfo_t | RLI_SPI_DeviceInfo

## Detailed Description

Version
  01.00

Definition in file RLI1.c.

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.