| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
ci_host_cmd_packet_t Struct Reference

This structure contains host command information. More...

`#include <isf_ci.h>`

Collaboration diagram for ci_host_cmd_packet_t:

## Data Fields
uint8 | appId
uint8 | cmd
uint16 | offset
uint8 | byte_cnt

## Detailed Description

This structure contains host command information.

This structure contains the host command and parameters passed to the embedded application for processing.

Definition at line 197 of file isf_ci.h.

## Field Documentation

uint8 appId

Application ID

Definition at line 200 of file isf_ci.h.

Referenced by App1_ci_app_callback(), BasicApp1_CI_Callback(), ci_protocol_CB_mbox(), ci_qr_update(), isf_app_callback_dev_info(), isf_app_callback_mbox(), and rli_ci_app_callback().

uint8 byte_cnt

Number of bytes to read/write

Definition at line 209 of file isf_ci.h.

Referenced by App1_ci_app_callback(), BasicApp1_CI_Callback(), ci_protocol_CB_mbox(), ci_qr_update(), isf_app_callback_mbox(), and rli_ci_app_callback().

uint8 cmd

Host command

Definition at line 203 of file isf_ci.h.

Referenced by App1_ci_app_callback(), BasicApp1_CI_Callback(), ci_protocol_CB_mbox(), ci_qr_update(), isf_app_callback_mbox(), and rli_ci_app_callback().

uint16 offset

Offset into the application's data

Definition at line 206 of file isf_ci.h.

Referenced by App1_ci_app_callback(), BasicApp1_CI_Callback(), ci_protocol_CB_mbox(), ci_qr_update(), isf_app_callback_mbox(), and rli_ci_app_callback().

The documentation for this struct was generated from the following file:

- ISF/Core/Include/isf_ci.h

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.