- ### Webserver Home

- Accelerometer
- RTC
- LED Control
- Status
- Memory Game
- K70 Family
- Browse SD Card

# Kinetis K70 using Freescale MQX Web Server

Kinetis
The Kinetis K70 MCU family includes 512KB-1MB of flash memory, a single precision floating point unit, Graphic LCD Controller, IEEE 1588 Ethernet, full- and high-speed USB 2.0 On-The-Go with device charge detect, hardware encryption, tamper detection capabilities and a NAND flash controller. 256-pin devices include a DRAM controller for system expansion. The Kinetis K70 family is available in 196 and 256 pin MAPBGA packages.
MQX
Accelerate your design success with complimentary RTOS, TCP/IP and USB stacks provided by Freescale MQX Software Solutions. Available on Freescale processors for more than 15 years, Freescale MQX Software Solutions offer a straightforward API with a modular architecture, making it simple to fine tune custom applications and scalable to fit most requirements. The combination of our market-proven Freescale MQX Software Solutions and silicon portfolio provides a streamlined and powerful platform by creating a comprehensive source for hardware, software, tools and services needs.