<PE_PROJECT_SETTINGS_DOCUMENTATION>
  <PE_product_version v="version 3.07 for Freescale HC(S)08/RS08/CFV1"/>
  <PE_core_version v="Processor Expert Version 0434"/>

  <CPU_Bean name="Cpu" type="MC9S08LL64_80">
    <Enabled v="N"/>

    <Properties>
      <Component_name v="Cpu"/>
      <CPU_type v="MC9S08LL64C_LQFP80"/>
      <list name="Shared Internal properties" v="1">
      </list>
      <list name="Shared CGM module settings" v="1">
        <group name="Clock settings">
          <group name="Internal clock">
            <Internal_oscillator_frequency__kHz_ v="31.250000000000"/>
            <Internal_ref__clock_for_peripherals v="Enabled"/>
            <boolgroup name="Initialize trim value" v="yes">
              <Trim_value_address v="65455"/>
              <Fine_trim_value_address v="65454"/>
            </boolgroup>
          </group>
          <group name="Low-power modes settings">
            <boolgroup name="STOP instruction enabled" v="no" />
          </group>
        </group>
      </list>
      <Initialization_interrupt_priority v="interrupts enabled"/>
      <list name="Shared internal resource mapping - XDP512" v="1">
        <group name="Internal resource mapping">
          <group name="Interrupt vector table">
            <Address v="65490"/>
            <Size v="44"/>
          </group>
          <group name="Reset vector">
            <Address v="65534"/>
            <Size v="2"/>
          </group>
        </group>
      </list>
      <group name="Internal peripherals">
        <list name="Shared Internal bandgap settings" v="1">
          <group name="Internal bandgap">
            <Internal_bandgap_buffer v="Disabled"/>
            <Internal_bandgap_buffer_drive v="low-drive mode"/>
          </group>
        </list>
        <list name="Shared BDM settings" v="1">
          <boolgroup name="BDM pin support" v="Disabled" />
        </list>
        <list name="Shared FLASH settings" v="1">
          <group name="FLASH">
            <enumgroup name="Security state" v="Disabled">
            </enumgroup>
            <enumgroup name="Protection" v="Disabled">
            </enumgroup>
            <Vector_redirection v="no"/>
          </group>
        </list>
        <list name="Included IO settings" v="1">
          <group name="I/O module">
            <list name="Shared Unused I/O" v="1">
              <enumgroup name="Initialize unused I/O pins" v="no initialization">
              </enumgroup>
            </list>
            <group name="PORT A">
              <Slew_rate_control_for_PTA0 v="no"/>
              <Slew_rate_control_for_PTA1 v="no"/>
              <Slew_rate_control_for_PTA2 v="no"/>
              <Slew_rate_control_for_PTA3 v="no"/>
              <Slew_rate_control_for_PTA4 v="no"/>
              <Slew_rate_control_for_PTA5 v="no"/>
              <Slew_rate_control_for_PTA6 v="no"/>
              <Slew_rate_control_for_PTA7 v="no"/>
              <Drive_strength_for_PTA0 v="High"/>
              <Drive_strength_for_PTA1 v="High"/>
              <Drive_strength_for_PTA2 v="High"/>
              <Drive_strength_for_PTA3 v="High"/>
              <Drive_strength_for_PTA4 v="High"/>
              <Drive_strength_for_PTA5 v="High"/>
              <Drive_strength_for_PTA6 v="High"/>
              <Drive_strength_for_PTA7 v="High"/>
            </group>
            <group name="PORT B">
              <Slew_rate_control_for_PTB0 v="no"/>
              <Slew_rate_control_for_PTB1 v="no"/>
              <Slew_rate_control_for_PTB2 v="no"/>
              <Slew_rate_control_for_PTB4 v="no"/>
              <Slew_rate_control_for_PTB5 v="no"/>
              <Slew_rate_control_for_PTB6 v="no"/>
              <Slew_rate_control_for_PTB7 v="no"/>
              <Drive_strength_for_PTB0 v="High"/>
              <Drive_strength_for_PTB1 v="High"/>
              <Drive_strength_for_PTB2 v="High"/>
              <Drive_strength_for_PTB4 v="High"/>
              <Drive_strength_for_PTB5 v="High"/>
              <Drive_strength_for_PTB6 v="High"/>
              <Drive_strength_for_PTB7 v="High"/>
            </group>
            <group name="PORT C">
              <Slew_rate_control_for_PTC0 v="no"/>
              <Slew_rate_control_for_PTC1 v="no"/>
              <Slew_rate_control_for_PTC2 v="no"/>
              <Slew_rate_control_for_PTC3 v="no"/>
              <Slew_rate_control_for_PTC4 v="no"/>
              <Slew_rate_control_for_PTC5 v="no"/>
              <Slew_rate_control_for_PTC6 v="no"/>
              <Slew_rate_control_for_PTC7 v="no"/>
              <Drive_strength_for_PTC0 v="High"/>
              <Drive_strength_for_PTC1 v="High"/>
              <Drive_strength_for_PTC2 v="High"/>
              <Drive_strength_for_PTC3 v="High"/>
              <Drive_strength_for_PTC4 v="High"/>
              <Drive_strength_for_PTC5 v="High"/>
              <Drive_strength_for_PTC6 v="High"/>
              <Drive_strength_for_PTC7 v="High"/>
            </group>
            <group name="PORT D">
              <Slew_rate_control_for_PTD0 v="no"/>
              <Slew_rate_control_for_PTD1 v="no"/>
              <Slew_rate_control_for_PTD2 v="no"/>
              <Slew_rate_control_for_PTD3 v="no"/>
              <Slew_rate_control_for_PTD4 v="no"/>
              <Slew_rate_control_for_PTD5 v="no"/>
              <Slew_rate_control_for_PTD6 v="no"/>
              <Slew_rate_control_for_PTD7 v="no"/>
              <Drive_strength_for_PTD0 v="High"/>
              <Drive_strength_for_PTD1 v="High"/>
              <Drive_strength_for_PTD2 v="High"/>
              <Drive_strength_for_PTD3 v="High"/>
              <Drive_strength_for_PTD4 v="High"/>
              <Drive_strength_for_PTD5 v="High"/>
              <Drive_strength_for_PTD6 v="High"/>
              <Drive_strength_for_PTD7 v="High"/>
            </group>
            <group name="PORT E">
              <Slew_rate_control_for_PTE0 v="no"/>
              <Slew_rate_control_for_PTE1 v="no"/>
              <Slew_rate_control_for_PTE2 v="no"/>
              <Slew_rate_control_for_PTE3 v="no"/>
              <Slew_rate_control_for_PTE4 v="no"/>
              <Slew_rate_control_for_PTE5 v="no"/>
              <Slew_rate_control_for_PTE6 v="no"/>
              <Slew_rate_control_for_PTE7 v="no"/>
              <Drive_strength_for_PTE0 v="High"/>
              <Drive_strength_for_PTE1 v="High"/>
              <Drive_strength_for_PTE2 v="High"/>
              <Drive_strength_for_PTE3 v="High"/>
              <Drive_strength_for_PTE4 v="High"/>
              <Drive_strength_for_PTE5 v="High"/>
              <Drive_strength_for_PTE6 v="High"/>
              <Drive_strength_for_PTE7 v="High"/>
            </group>
          </group>
        </list>
        <list name="SharedClockGatingGrp" v="1">
          <group name="System Clock Gating">
            <SCI1_Clock_Gate v="Enabled"/>
            <SCI2_Clock_Gate v="Enabled"/>
            <IIC_Clock_Gate v="Enabled"/>
            <VREF1_Clock_Gate v="Enabled"/>
            <ADC_Clock_Gate v="Enabled"/>
            <TPM1_Clock_Gate v="Enabled"/>
            <TPM2_Clock_Gate v="Enabled"/>
            <VREF2_Clock_Gate v="Enabled"/>
            <SPI_Clock_Gate v="Enabled"/>
            <LCD_Clock_Gate v="Enabled"/>
            <TOD_Clock_Gate v="Enabled"/>
            <ACMP_Clock_Gate v="Enabled"/>
            <KBI_Clock_Gate v="Enabled"/>
            <IRQ_Clock_Gate v="Enabled"/>
            <FLASH_Register_Clock_Gate v="Enabled"/>
            <DBG_Clock_Gate v="Enabled"/>
          </group>
        </list>
        <list name="Shared LVD settings" v="1">
          <boolgroup name="LVD module" v="Enabled">
            <LVD_operation v="Reset"/>
            <LVW_interrupt v="Disabled"/>
            <boolgroup name="LVD module interrupt" v="Disabled" />
            <Enable_in_stop_mode v="yes"/>
            <Wake_up_on_Interupt v="no"/>
          </boolgroup>
        </list>
        <list name="Shared TMP modules setting" v="1">
        </list>
        <list name="Shared Reset pin setting" v="1">
          <boolgroup name="Reset pin support" v="Enabled">
            <Reset_pin v="PTB2_RESET"/>
            <Reset_pin_signal v=""/>
          </boolgroup>
        </list>
      </group>
      <group name="CPU interrupts">
        <list name="Shared Cpu interrupts" v="1">
        </list>
        <list name="Shared Cpu interrupts" v="1">
          <boolgroup name="SWI" v="Disabled" />
        </list>
      </group>
      <list name="Shared ICSv3 speed mode settings" v="1">
        <group name="Enabled speed modes">
          <boolgroup name="High speed mode" v="Enabled">
            <High_speed_clock v="Internal Clock"/>
            <Bus_freq__divider v="Auto select"/>
            <Internal_bus_clock v="4"/>
            <Fixed_frequency_clock__MHz_ v="0.015625"/>
            <enumgroup name="FLL mode" v="Engaged">
              <enumgroup name="Ref. clock source" v="Internal Clock">
                <Ref__clock_freq___MHz_ v="0.031250000000"/>
              </enumgroup>
              <enumgroup name="DCO mode" v="Auto select">
              </enumgroup>
              <FLL_output_clock_freq___MHz_ v="16"/>
            </enumgroup>
          </boolgroup>
          <boolgroup name="Low speed mode" v="Disabled" />
          <boolgroup name="Slow speed mode" v="Disabled" />
        </group>
      </list>
    </Properties>

    <Methods>
      <list name="SharedCpuMethods" v="1">
        <SetHighSpeed v="don&apos;t generate code"/>
        <SetLowSpeed v="don&apos;t generate code"/>
        <SetSlowSpeed v="don&apos;t generate code"/>
        <GetSpeedMode v="don&apos;t generate code"/>
        <EnableInt v="generate code"/>
        <DisableInt v="generate code"/>
        <GetResetSource v="don&apos;t generate code"/>
        <SetWaitMode v="don&apos;t generate code"/>
        <SetStopMode v="don&apos;t generate code"/>
        <GetLowVoltageWarningFlag v="don&apos;t generate code"/>
        <ClearLowVoltageWarningFlag v="don&apos;t generate code"/>
        <GetPartialPowerDownFlag v="don&apos;t generate code"/>
        <ClearPartialPowerDownFlag v="don&apos;t generate code"/>
        <GetIdentification v="don&apos;t generate code"/>
        <SetBackdoorKey v="don&apos;t generate code"/>
        <Delay100US v="don&apos;t generate code"/>
      </list>
    </Methods>

    <Events>
      <Event_module_name v="Events"/>
      <list name="HCS08EventsGrp" v="1">
        <event name="OnSwINT" v="don&apos;t generate code" />
      </list>
      <list name="CommonEventsGrp" v="1">
        <event name="OnReset" v="don&apos;t generate code" />
      </list>
    </Events>
    <Compiler v="CodeWarrior HCS08 C Compiler"/>

    <CompilerProperties>
      <Compiler v="CodeWarrior HCS08 C Compiler"/>
      <enumgroup name="Unhandled vectors" v="One handler for all">
        <Unhandled_int_code>
asm(BGND);
        </Unhandled_int_code>
      </enumgroup>
      <Generate_macros v="yes"/>
      <group name="User initialization">
        <User_data_declarations>
        </User_data_declarations>
        <User_code_before_PE_initialization>
        </User_code_before_PE_initialization>
        <User_code_after_PE_initialization>
        </User_code_after_PE_initialization>
      </group>
      <Memory_model v="Small"/>
      <boolgroup name="Generate PRM file" v="yes">
        <enumgroup name="Stack specification" v="size">
          <Stack_size v="128"/>
        </enumgroup>
        <Set_memory_areas_default v="Click to set default &gt;"/>
        <list name="ROM/RAM Areas" v="0">
        </list>
      </boolgroup>
    </CompilerProperties>
  </CPU_Bean>

  <CPU_Bean name="Cpu" type="MC9S08LL64_80">
    <Enabled v="Y"/>

    <Properties>
      <Component_name v="Cpu"/>
      <CPU_type v="MC9S08LL64C_LQFP80"/>
      <list name="Shared Internal properties" v="1">
      </list>
      <list name="Shared CGM module settings" v="1">
        <group name="Clock settings">
          <group name="Internal clock">
            <Internal_oscillator_frequency__kHz_ v="31.250000000000"/>
            <Internal_ref__clock_for_peripherals v="Enabled"/>
            <boolgroup name="Initialize trim value" v="yes">
              <Trim_value_address v="65455"/>
              <Fine_trim_value_address v="65454"/>
            </boolgroup>
          </group>
          <boolgroup name="External clock" v="Enabled">
            <enumgroup name="Clock source" v="External crystal">
              <Clock_frequency__MHz_ v="0.032768000000"/>
              <group name="Clock input pin">
                <Pin_name v="PTB0_EXTAL"/>
                <Pin_signal v=""/>
              </group>
              <group name="Clock output pin">
                <Pin_name v="PTB1_XTAL"/>
                <Pin_signal v=""/>
              </group>
              <Clock_range v="Low frequency"/>
              <Oscillator_operating_mode v="Low power"/>
              <External_ref__clock_for_peripherals v="Enabled"/>
            </enumgroup>
          </boolgroup>
          <group name="Low-power modes settings">
            <boolgroup name="STOP instruction enabled" v="yes">
              <Partial_power_down_mode v="Enabled"/>
              <Internal_clock_in_stop_mode v="Disabled"/>
              <External_clock_in_stop_mode v="Enabled"/>
            </boolgroup>
          </group>
        </group>
      </list>
      <Initialization_interrupt_priority v="interrupts enabled"/>
      <list name="Shared internal resource mapping - XDP512" v="1">
        <group name="Internal resource mapping">
          <group name="Interrupt vector table">
            <Address v="65490"/>
            <Size v="44"/>
          </group>
          <group name="Reset vector">
            <Address v="65534"/>
            <Size v="2"/>
          </group>
        </group>
      </list>
      <group name="Internal peripherals">
        <list name="Shared Internal bandgap settings" v="1">
          <group name="Internal bandgap">
            <Internal_bandgap_buffer v="Disabled"/>
            <Internal_bandgap_buffer_drive v="high-drive mode"/>
          </group>
        </list>
        <list name="Shared BDM settings" v="1">
          <boolgroup name="BDM pin support" v="Enabled">
            <BDM_pin v="PTC6_ACMPO_BKGD_MS"/>
            <BDM_pin_signal v=""/>
          </boolgroup>
        </list>
        <list name="Shared FLASH settings" v="1">
          <group name="FLASH">
            <enumgroup name="Security state" v="Disabled">
            </enumgroup>
            <enumgroup name="Protection" v="Disabled">
            </enumgroup>
            <Vector_redirection v="no"/>
          </group>
        </list>
        <list name="Included IO settings" v="1">
          <group name="I/O module">
            <list name="Shared Unused I/O" v="1">
              <enumgroup name="Initialize unused I/O pins" v="output">
                <Pull_resistor v="no initialization"/>
                <Output_value v="1"/>
              </enumgroup>
            </list>
            <group name="PORT A">
              <Slew_rate_control_for_PTA0 v="no"/>
              <Slew_rate_control_for_PTA1 v="no"/>
              <Slew_rate_control_for_PTA2 v="no"/>
              <Slew_rate_control_for_PTA3 v="no"/>
              <Slew_rate_control_for_PTA4 v="no"/>
              <Slew_rate_control_for_PTA5 v="no"/>
              <Slew_rate_control_for_PTA6 v="no"/>
              <Slew_rate_control_for_PTA7 v="no"/>
              <Drive_strength_for_PTA0 v="High"/>
              <Drive_strength_for_PTA1 v="High"/>
              <Drive_strength_for_PTA2 v="High"/>
              <Drive_strength_for_PTA3 v="High"/>
              <Drive_strength_for_PTA4 v="High"/>
              <Drive_strength_for_PTA5 v="High"/>
              <Drive_strength_for_PTA6 v="High"/>
              <Drive_strength_for_PTA7 v="High"/>
            </group>
            <group name="PORT B">
              <Slew_rate_control_for_PTB0 v="no"/>
              <Slew_rate_control_for_PTB1 v="no"/>
              <Slew_rate_control_for_PTB2 v="no"/>
              <Slew_rate_control_for_PTB4 v="no"/>
              <Slew_rate_control_for_PTB5 v="no"/>
              <Slew_rate_control_for_PTB6 v="no"/>
              <Slew_rate_control_for_PTB7 v="no"/>
              <Drive_strength_for_PTB0 v="High"/>
              <Drive_strength_for_PTB1 v="High"/>
              <Drive_strength_for_PTB2 v="High"/>
              <Drive_strength_for_PTB4 v="Low"/>
              <Drive_strength_for_PTB5 v="Low"/>
              <Drive_strength_for_PTB6 v="Low"/>
              <Drive_strength_for_PTB7 v="Low"/>
            </group>
            <group name="PORT C">
              <Slew_rate_control_for_PTC0 v="no"/>
              <Slew_rate_control_for_PTC1 v="no"/>
              <Slew_rate_control_for_PTC2 v="no"/>
              <Slew_rate_control_for_PTC3 v="no"/>
              <Slew_rate_control_for_PTC4 v="no"/>
              <Slew_rate_control_for_PTC5 v="no"/>
              <Slew_rate_control_for_PTC6 v="no"/>
              <Slew_rate_control_for_PTC7 v="no"/>
              <Drive_strength_for_PTC0 v="High"/>
              <Drive_strength_for_PTC1 v="High"/>
              <Drive_strength_for_PTC2 v="Low"/>
              <Drive_strength_for_PTC3 v="Low"/>
              <Drive_strength_for_PTC4 v="High"/>
              <Drive_strength_for_PTC5 v="High"/>
              <Drive_strength_for_PTC6 v="High"/>
              <Drive_strength_for_PTC7 v="High"/>
            </group>
            <group name="PORT D">
              <Slew_rate_control_for_PTD0 v="no"/>
              <Slew_rate_control_for_PTD1 v="no"/>
              <Slew_rate_control_for_PTD2 v="no"/>
              <Slew_rate_control_for_PTD3 v="no"/>
              <Slew_rate_control_for_PTD4 v="no"/>
              <Slew_rate_control_for_PTD5 v="no"/>
              <Slew_rate_control_for_PTD6 v="no"/>
              <Slew_rate_control_for_PTD7 v="no"/>
              <Drive_strength_for_PTD0 v="High"/>
              <Drive_strength_for_PTD1 v="High"/>
              <Drive_strength_for_PTD2 v="High"/>
              <Drive_strength_for_PTD3 v="High"/>
              <Drive_strength_for_PTD4 v="High"/>
              <Drive_strength_for_PTD5 v="High"/>
              <Drive_strength_for_PTD6 v="High"/>
              <Drive_strength_for_PTD7 v="High"/>
            </group>
            <group name="PORT E">
              <Slew_rate_control_for_PTE0 v="no"/>
              <Slew_rate_control_for_PTE1 v="no"/>
              <Slew_rate_control_for_PTE2 v="no"/>
              <Slew_rate_control_for_PTE3 v="no"/>
              <Slew_rate_control_for_PTE4 v="no"/>
              <Slew_rate_control_for_PTE5 v="no"/>
              <Slew_rate_control_for_PTE6 v="no"/>
              <Slew_rate_control_for_PTE7 v="no"/>
              <Drive_strength_for_PTE0 v="High"/>
              <Drive_strength_for_PTE1 v="High"/>
              <Drive_strength_for_PTE2 v="High"/>
              <Drive_strength_for_PTE3 v="High"/>
              <Drive_strength_for_PTE4 v="High"/>
              <Drive_strength_for_PTE5 v="High"/>
              <Drive_strength_for_PTE6 v="High"/>
              <Drive_strength_for_PTE7 v="High"/>
            </group>
          </group>
        </list>
        <list name="SharedClockGatingGrp" v="1">
          <group name="System Clock Gating">
            <SCI1_Clock_Gate v="Enabled"/>
            <SCI2_Clock_Gate v="Disabled"/>
            <IIC_Clock_Gate v="Disabled"/>
            <VREF1_Clock_Gate v="Disabled"/>
            <ADC_Clock_Gate v="Enabled"/>
            <TPM1_Clock_Gate v="Enabled"/>
            <TPM2_Clock_Gate v="Disabled"/>
            <VREF2_Clock_Gate v="Disabled"/>
            <SPI_Clock_Gate v="Disabled"/>
            <LCD_Clock_Gate v="Enabled"/>
            <TOD_Clock_Gate v="Enabled"/>
            <ACMP_Clock_Gate v="Disabled"/>
            <KBI_Clock_Gate v="Enabled"/>
            <IRQ_Clock_Gate v="Enabled"/>
            <FLASH_Register_Clock_Gate v="Enabled"/>
            <DBG_Clock_Gate v="Enabled"/>
          </group>
        </list>
        <list name="Shared LVD settings" v="1">
          <boolgroup name="LVD module" v="Disabled" />
        </list>
        <list name="Shared TMP modules setting" v="1">
        </list>
        <list name="Shared Reset pin setting" v="1">
          <boolgroup name="Reset pin support" v="Enabled">
            <Reset_pin v="PTB2_RESET"/>
            <Reset_pin_signal v=""/>
          </boolgroup>
        </list>
      </group>
      <group name="CPU interrupts">
        <list name="Shared Cpu interrupts" v="1">
        </list>
        <list name="Shared Cpu interrupts" v="1">
          <boolgroup name="SWI" v="Disabled" />
        </list>
      </group>
      <list name="Shared ICSv3 speed mode settings" v="1">
        <group name="Enabled speed modes">
          <boolgroup name="High speed mode" v="Enabled">
            <High_speed_clock v="External Clock"/>
            <Bus_freq__divider v="1"/>
            <Internal_bus_clock v="9.961472000000"/>
            <Fixed_frequency_clock__MHz_ v="0.016384"/>
            <enumgroup name="FLL mode" v="Engaged">
              <enumgroup name="Ref. clock source" v="External Clock">
                <Ref__clock_source_freq___MHz_ v="0.032768000000"/>
                <Ref__clock_divider v="1"/>
                <Ref__clock_freq___MHz_ v="0.032768000000"/>
              </enumgroup>
              <enumgroup name="DCO mode" v="Fine tuned 32kHz">
                <FLL_mult__factor v="608"/>
              </enumgroup>
              <FLL_output_clock_freq___MHz_ v="19.922944000000"/>
            </enumgroup>
          </boolgroup>
          <boolgroup name="Low speed mode" v="Disabled" />
          <boolgroup name="Slow speed mode" v="Disabled" />
        </group>
      </list>
    </Properties>

    <Methods>
      <list name="SharedCpuMethods" v="1">
        <SetHighSpeed v="don&apos;t generate code"/>
        <SetLowSpeed v="don&apos;t generate code"/>
        <SetSlowSpeed v="don&apos;t generate code"/>
        <GetSpeedMode v="don&apos;t generate code"/>
        <SetIntVect v="don&apos;t generate code"/>
        <GetIntVect v="don&apos;t generate code"/>
        <EnableInt v="generate code"/>
        <DisableInt v="generate code"/>
        <GetResetSource v="don&apos;t generate code"/>
        <SetWaitMode v="don&apos;t generate code"/>
        <SetStopMode v="don&apos;t generate code"/>
        <GetLowVoltageFlag v="don&apos;t generate code"/>
        <ClearLowVoltageFlag v="don&apos;t generate code"/>
        <GetLowVoltageWarningFlag v="don&apos;t generate code"/>
        <ClearLowVoltageWarningFlag v="don&apos;t generate code"/>
        <GetPartialPowerDownFlag v="don&apos;t generate code"/>
        <ClearPartialPowerDownFlag v="don&apos;t generate code"/>
        <GetIdentification v="don&apos;t generate code"/>
        <SetBackdoorKey v="don&apos;t generate code"/>
        <Delay100US v="don&apos;t generate code"/>
      </list>
    </Methods>

    <Events>
      <Event_module_name v="Events"/>
      <list name="HCS08EventsGrp" v="1">
        <event name="OnSwINT" v="don&apos;t generate code" />
      </list>
      <list name="CommonEventsGrp" v="1">
        <event name="OnReset" v="don&apos;t generate code" />
        <event name="OnLvdINT" v="don&apos;t generate code" />
        <event name="OnLvwINT" v="don&apos;t generate code" />
      </list>
    </Events>
    <Compiler v="CodeWarrior HCS08 C Compiler"/>

    <CompilerProperties>
      <Compiler v="CodeWarrior HCS08 C Compiler"/>
      <enumgroup name="Unhandled vectors" v="One handler for all">
        <Unhandled_int_code>
asm(BGND);
        </Unhandled_int_code>
      </enumgroup>
      <Generate_macros v="yes"/>
      <group name="User initialization">
        <User_data_declarations>
        </User_data_declarations>
        <User_code_before_PE_initialization>
        </User_code_before_PE_initialization>
        <User_code_after_PE_initialization>
        </User_code_after_PE_initialization>
      </group>
      <Memory_model v="Banked"/>
      <boolgroup name="Generate PRM file" v="no" />
    </CompilerProperties>
  </CPU_Bean>

  <Bean name="LCD1" type="Init_LCD">
    <Enabled v="Y"/>

    <Properties>
      <Component_name v="LCD1"/>
      <Device v="LCD"/>
      <group name="Settings">
        <group name="Clock settings">
          <LCD_Clock_Gate v="Enabled"/>
          <Clock_source_select v="External clock reference"/>
          <Base_clock_prescaler v="8"/>
          <LCD_module_clock v="33 kHz"/>
          <Base_clock v="64.453 Hz"/>
          <Charge_pump_clock_adjust v="Fastest clock"/>
          <Charge_pump_clock v="5.5 kHz"/>
          <Blink_rate_bits_value v="4"/>
          <Blink_rate v="0.50354 Hz"/>
          <Display_mode v="2 backplanes"/>
          <Duty v="1/2"/>
          <Frame_frequency v="32.226 Hz"/>
        </group>
        <Stop_in_Wait_mode v="no"/>
        <Stop_in_Stop_mode v="no"/>
        <Full_complementary_drive v="Disabled"/>
        <Charge_pump v="Enabled"/>
        <Op_Amp_control v="Buffered mode"/>
        <Charge_pump_mode v="Voltage doubler"/>
        <Regulated_voltage v="Enabled"/>
        <Regulated_voltage_trim v="0"/>
        <Voltage_supply_control v="Drive VLL3 externally"/>
        <Blink_mode_select v="Alternate Display"/>
      </group>
      <group name="Pins">
        <list name="Frontplane pins" v="28">
          <group name="Frontplane pin0">
            <Frontplane_pin v="PTD0_LCD0"/>
            <Frontplane_pin_signal v="PIN1"/>
          </group>
          <group name="Frontplane pin1">
            <Frontplane_pin v="PTD1_LCD1"/>
            <Frontplane_pin_signal v="PIN2"/>
          </group>
          <group name="Frontplane pin2">
            <Frontplane_pin v="PTD2_LCD2"/>
            <Frontplane_pin_signal v="PIN3"/>
          </group>
          <group name="Frontplane pin3">
            <Frontplane_pin v="PTD3_LCD3"/>
            <Frontplane_pin_signal v="PIN4"/>
          </group>
          <group name="Frontplane pin4">
            <Frontplane_pin v="PTD4_LCD4"/>
            <Frontplane_pin_signal v="PIN5"/>
          </group>
          <group name="Frontplane pin5">
            <Frontplane_pin v="PTD5_LCD5"/>
            <Frontplane_pin_signal v="PIN6"/>
          </group>
          <group name="Frontplane pin6">
            <Frontplane_pin v="PTD6_LCD6"/>
            <Frontplane_pin_signal v="PIN7"/>
          </group>
          <group name="Frontplane pin7">
            <Frontplane_pin v="PTD7_LCD7"/>
            <Frontplane_pin_signal v="PIN8"/>
          </group>
          <group name="Frontplane pin8">
            <Frontplane_pin v="PTE0_LCD13"/>
            <Frontplane_pin_signal v="PIN9"/>
          </group>
          <group name="Frontplane pin9">
            <Frontplane_pin v="PTE1_LCD14"/>
            <Frontplane_pin_signal v="PIN10"/>
          </group>
          <group name="Frontplane pin10">
            <Frontplane_pin v="PTE2_LCD15"/>
            <Frontplane_pin_signal v="PIN11"/>
          </group>
          <group name="Frontplane pin11">
            <Frontplane_pin v="PTE3_LCD16"/>
            <Frontplane_pin_signal v="PIN12"/>
          </group>
          <group name="Frontplane pin12">
            <Frontplane_pin v="PTE4_LCD17"/>
            <Frontplane_pin_signal v="PIN13"/>
          </group>
          <group name="Frontplane pin13">
            <Frontplane_pin v="PTE5_LCD18"/>
            <Frontplane_pin_signal v="PIN14"/>
          </group>
          <group name="Frontplane pin14">
            <Frontplane_pin v="PTE6_LCD19"/>
            <Frontplane_pin_signal v="PIN15"/>
          </group>
          <group name="Frontplane pin15">
            <Frontplane_pin v="PTE7_LCD20"/>
            <Frontplane_pin_signal v="PIN16"/>
          </group>
          <group name="Frontplane pin16">
            <Frontplane_pin v="LCD21"/>
            <Frontplane_pin_signal v="PIN17"/>
          </group>
          <group name="Frontplane pin17">
            <Frontplane_pin v="LCD22"/>
            <Frontplane_pin_signal v="PIN18"/>
          </group>
          <group name="Frontplane pin18">
            <Frontplane_pin v="LCD23"/>
            <Frontplane_pin_signal v="PIN19"/>
          </group>
          <group name="Frontplane pin19">
            <Frontplane_pin v="LCD24"/>
            <Frontplane_pin_signal v="PIN20"/>
          </group>
          <group name="Frontplane pin20">
            <Frontplane_pin v="LCD25"/>
            <Frontplane_pin_signal v="PIN21"/>
          </group>
          <group name="Frontplane pin21">
            <Frontplane_pin v="LCD26"/>
            <Frontplane_pin_signal v="PIN22"/>
          </group>
          <group name="Frontplane pin22">
            <Frontplane_pin v="LCD27"/>
            <Frontplane_pin_signal v="PIN23"/>
          </group>
          <group name="Frontplane pin23">
            <Frontplane_pin v="LCD28"/>
            <Frontplane_pin_signal v="PIN24"/>
          </group>
          <group name="Frontplane pin24">
            <Frontplane_pin v="LCD29"/>
            <Frontplane_pin_signal v="PIN25"/>
          </group>
          <group name="Frontplane pin25">
            <Frontplane_pin v="LCD30"/>
            <Frontplane_pin_signal v="PIN26"/>
          </group>
          <group name="Frontplane pin26">
            <Frontplane_pin v="LCD38"/>
            <Frontplane_pin_signal v="PIN27"/>
          </group>
          <group name="Frontplane pin27">
            <Frontplane_pin v="LCD39"/>
            <Frontplane_pin_signal v="PIN28"/>
          </group>
        </list>
        <boolgroup name="Backplane pin 0" v="Enabled">
          <Backplane_pin v="LCD40"/>
          <Backplane_pin_signal v=""/>
        </boolgroup>
        <boolgroup name="Backplane pin 1" v="Enabled">
          <Backplane_pin v="LCD41"/>
          <Backplane_pin_signal v=""/>
        </boolgroup>
        <boolgroup name="Backplane pin 2" v="Disabled" />
        <boolgroup name="Backplane pin 3" v="Disabled" />
        <boolgroup name="Backplane pin 4" v="Disabled" />
        <boolgroup name="Backplane pin 5" v="Disabled" />
        <boolgroup name="Backplane pin 6" v="Disabled" />
        <boolgroup name="Backplane pin 7" v="Disabled" />
      </group>
      <group name="Interrupts">
        <Interrupt v="Vlcd"/>
        <LCD_frame_frequency_interrupt v="Disabled"/>
        <ISR_name v=""/>
      </group>
      <group name="Initialization">
        <Call_Init_method v="yes"/>
        <LCD_module v="Enabled"/>
        <Blink_command v="Disabled"/>
        <Blank_mode v="Disabled"/>
        <Alternate_display v="Disabled"/>
      </group>
    </Properties>

    <Methods>
      <Init v="generate code"/>
    </Methods>

    <Events>
    </Events>
  </Bean>

  <Bean name="ADC1" type="Init_ADC">
    <Enabled v="Y"/>

    <Properties>
      <Component_name v="ADC1"/>
      <Device v="ADC"/>
      <group name="Settings">
        <group name="Clock settings">
          <Input_clock_select v="BusClk"/>
          <External_ref__clock_for_peripherals v="Enabled"/>
          <ADC_Clock_Gate v="Enabled"/>
          <Prescaler v="8"/>
          <High_speed_conversion_mode v="Disabled"/>
          <Asynchro_clock_output v="Disabled"/>
          <Long_sample_time v="yes"/>
          <Long_sample_time_length v="20"/>
          <Frequency v="1245.184 kHz"/>
          <enumgroup name="ADC timing details" v="Complex">
            <Single_conversion_time v="32.63 us; not supported"/>
            <Continuous_conversion_time v="29.71 us; not supported"/>
          </enumgroup>
        </group>
        <Conversion_mode v="Single conversion"/>
        <Result_data_format v="8-bit right"/>
        <Low_power_mode v="Disabled"/>
        <Conversion_trigger v="Software"/>
        <Hardware_trigger_select v="TOD"/>
        <group name="Compare Function">
          <Compare_function v="Disabled"/>
          <Compare_type v="less than"/>
          <Compare_value v="0"/>
        </group>
        <Internal_bandgap_buffer v="Disabled"/>
      </group>
      <group name="Pins">
        <list name="ADC Input Pins" v="5">
          <group name="Input Pin0">
            <Pin v="PTA0_KBIP0_SS_ADP4"/>
            <Pin_Signal v=""/>
            <Pin_I_O_control_disable v="yes"/>
          </group>
          <group name="Input Pin1">
            <Pin v="PTA1_KBIP1_SPSCK_ADP5"/>
            <Pin_Signal v=""/>
            <Pin_I_O_control_disable v="yes"/>
          </group>
          <group name="Input Pin2">
            <Pin v="PTA2_KBIP2_SDA_MISO_ADP6"/>
            <Pin_Signal v=""/>
            <Pin_I_O_control_disable v="yes"/>
          </group>
          <group name="Input Pin3">
            <Pin v="PTA3_KBIP3_SCL_MOSI_ADP7"/>
            <Pin_Signal v=""/>
            <Pin_I_O_control_disable v="yes"/>
          </group>
          <group name="Input Pin4">
            <Pin v="PTA6_KBIP6_ADP10_ACMPPLUS"/>
            <Pin_Signal v=""/>
            <Pin_I_O_control_disable v="yes"/>
          </group>
        </list>
      </group>
      <group name="Interrupts/DMA">
        <group name="Conversion complete">
          <Interrupt v="Vadc"/>
          <enumgroup name="ADC type" v="ADC12V1 or ADC10V1 or ADC8V1">
            <Conversion_complete_interrupt v="Disabled"/>
          </enumgroup>
          <ISR_name v=""/>
        </group>
      </group>
      <group name="Initialization">
        <enumgroup name="ADC type" v="ADC12V1 or ADC10V1 or ADC8V1">
          <Initial_channel_select v="ADC Disabled"/>
        </enumgroup>
        <Call_Init_method v="yes"/>
      </group>
    </Properties>

    <Methods>
      <Init v="generate code"/>
    </Methods>

    <Events>
    </Events>
  </Bean>

  <Bean name="LED1" type="BitIO">
    <Enabled v="Y"/>

    <Properties>
      <Component_name v="LED1"/>
      <Pin_for_I_O v="PTC2_TPM1CH0"/>
      <Pin_signal v="LED5"/>
      <Pull_resistor v="no pull resistor"/>
      <Open_drain v="push-pull"/>
      <Slew_rate_control_for_PTC2 v="no"/>
      <Drive_strength_for_PTC2 v="Low"/>
      <Direction v="Output"/>
      <group name="Initialization">
        <Init__direction v="Output"/>
        <Init__value v="1"/>
      </group>
      <Safe_mode v="yes"/>
      <Optimization_for v="speed"/>
    </Properties>

    <Methods>
      <GetDir v="don&apos;t generate code"/>
      <SetDir v="don&apos;t generate code"/>
      <SetInput v="don&apos;t generate code"/>
      <SetOutput v="don&apos;t generate code"/>
      <GetVal v="generate code"/>
      <PutVal v="generate code"/>
      <ClrVal v="generate code"/>
      <SetVal v="generate code"/>
      <NegVal v="don&apos;t generate code"/>
    </Methods>

    <Events>
    </Events>
  </Bean>

  <Bean name="LED2" type="BitIO">
    <Enabled v="Y"/>

    <Properties>
      <Component_name v="LED2"/>
      <Pin_for_I_O v="PTC3_TPM1CH1"/>
      <Pin_signal v="LED6"/>
      <Pull_resistor v="no pull resistor"/>
      <Open_drain v="push-pull"/>
      <Slew_rate_control_for_PTC3 v="no"/>
      <Drive_strength_for_PTC3 v="Low"/>
      <Direction v="Output"/>
      <group name="Initialization">
        <Init__direction v="Output"/>
        <Init__value v="1"/>
      </group>
      <Safe_mode v="yes"/>
      <Optimization_for v="speed"/>
    </Properties>

    <Methods>
      <GetDir v="don&apos;t generate code"/>
      <SetDir v="don&apos;t generate code"/>
      <SetInput v="don&apos;t generate code"/>
      <SetOutput v="don&apos;t generate code"/>
      <GetVal v="generate code"/>
      <PutVal v="generate code"/>
      <ClrVal v="generate code"/>
      <SetVal v="generate code"/>
      <NegVal v="don&apos;t generate code"/>
    </Methods>

    <Events>
    </Events>
  </Bean>

  <Bean name="LED3" type="BitIO">
    <Enabled v="Y"/>

    <Properties>
      <Component_name v="LED3"/>
      <Pin_for_I_O v="PTC4_TPM2CH0"/>
      <Pin_signal v="LED7"/>
      <Pull_resistor v="no pull resistor"/>
      <Open_drain v="push-pull"/>
      <Slew_rate_control_for_PTC4 v="no"/>
      <Drive_strength_for_PTC4 v="High"/>
      <Direction v="Output"/>
      <group name="Initialization">
        <Init__direction v="Output"/>
        <Init__value v="1"/>
      </group>
      <Safe_mode v="yes"/>
      <Optimization_for v="speed"/>
    </Properties>

    <Methods>
      <GetDir v="don&apos;t generate code"/>
      <SetDir v="don&apos;t generate code"/>
      <SetInput v="don&apos;t generate code"/>
      <SetOutput v="don&apos;t generate code"/>
      <GetVal v="generate code"/>
      <PutVal v="generate code"/>
      <ClrVal v="generate code"/>
      <SetVal v="generate code"/>
      <NegVal v="don&apos;t generate code"/>
    </Methods>

    <Events>
    </Events>
  </Bean>

  <Bean name="LED4" type="BitIO">
    <Enabled v="Y"/>

    <Properties>
      <Component_name v="LED4"/>
      <Pin_for_I_O v="PTC5_TPM2CH1"/>
      <Pin_signal v="LED8"/>
      <Pull_resistor v="no pull resistor"/>
      <Open_drain v="push-pull"/>
      <Slew_rate_control_for_PTC5 v="no"/>
      <Drive_strength_for_PTC5 v="High"/>
      <Direction v="Output"/>
      <group name="Initialization">
        <Init__direction v="Output"/>
        <Init__value v="1"/>
      </group>
      <Safe_mode v="yes"/>
      <Optimization_for v="speed"/>
    </Properties>

    <Methods>
      <GetDir v="don&apos;t generate code"/>
      <SetDir v="don&apos;t generate code"/>
      <SetInput v="don&apos;t generate code"/>
      <SetOutput v="don&apos;t generate code"/>
      <GetVal v="generate code"/>
      <PutVal v="generate code"/>
      <ClrVal v="generate code"/>
      <SetVal v="generate code"/>
      <NegVal v="don&apos;t generate code"/>
    </Methods>

    <Events>
    </Events>
  </Bean>

  <Bean name="TOD1" type="Init_TOD">
    <Enabled v="Y"/>

    <Properties>
      <Component_name v="TOD1"/>
      <Device v="TOD"/>
      <group name="Settings">
        <group name="Clock settings">
          <TOD_Clock_Gate v="Enabled"/>
          <Clock_select v="External clock"/>
          <Prescaler v="divide by 8192"/>
          <Counter_frequency v="0.2500 ms"/>
          <TOD_clock v="Disabled"/>
        </group>
        <Match_function v="Disabled"/>
        <Match_value v="0"/>
      </group>
      <group name="Interrupts">
        <Interrupt v="Vtod"/>
        <Quarter_second_interrupt v="Disabled"/>
        <One_second_interrupt v="Enabled"/>
        <Match_interrupt v="Enabled"/>
        <ISR_name v="TOD_isr"/>
      </group>
      <group name="Initialization">
        <Enable_TOD v="yes"/>
        <Reset_TOD v="no"/>
        <Call_Init_method v="yes"/>
      </group>
    </Properties>

    <Methods>
      <Init v="generate code"/>
    </Methods>

    <Events>
    </Events>
  </Bean>

  <Bean name="IRQ1" type="Init_IRQ">
    <Enabled v="Y"/>

    <Properties>
      <Component_name v="IRQ1"/>
      <Device v="IRQModule"/>
      <list name="Pins" v="1">
        <group name="Pin IRQ1">
          <Pin v="PTC7_IRQ_TCLK"/>
          <Pin_signal v=""/>
          <Pin_enable v="yes"/>
          <Pull_resistor v="pull enable"/>
          <Detection_mode v="edge only"/>
          <IRQ_Clock_Gate v="Enabled"/>
          <Edge_select v="falling edge and/or low level"/>
          <group name="Interrupts">
            <Interrupt v="Virq"/>
            <IRQ_interrupt v="Enabled"/>
            <ISR_name v="IRQ_ISR"/>
          </group>
        </group>
      </list>
      <group name="Initialization">
        <Call_Init_Method v="yes"/>
      </group>
    </Properties>

    <Methods>
      <Init v="generate code"/>
    </Methods>

    <Events>
    </Events>
  </Bean>

  <Bean name="AS1" type="AsynchroSerial">
    <Enabled v="Y"/>

    <Properties>
      <Component_name v="AS1"/>
      <Channel v="SCI1"/>
      <boolgroup name="Interrupt service/event" v="Disabled" />
      <group name="Settings">
        <Parity v="none"/>
        <Width v="8 bits"/>
        <Stop_bit v="1"/>
        <enumgroup name="SCI output mode" v="Normal">
        </enumgroup>
        <boolgroup name="Receiver" v="Enabled">
          <RxD v="PTC0_RxD1"/>
          <RxD_pin_signal v=""/>
        </boolgroup>
        <boolgroup name="Transmitter" v="Enabled">
          <TxD v="PTC1_TxD1"/>
          <TxD_pin_signal v=""/>
        </boolgroup>
        <Baud_rate v="19200 baud"/>
        <Break_signal v="Disabled"/>
        <Wakeup_condition v="Idle line wakeup"/>
        <Transmitter_output v="Not inverted"/>
        <Receiver_input v="Not inverted"/>
        <Stop_in_wait_mode v="yes"/>
        <Idle_line_mode v="starts after start bit"/>
        <Break_generation_length v="10/11 bits"/>
        <Active_edge_detection v="Disabled"/>
      </group>
      <group name="Initialization">
        <Enabled_in_init__code v="yes"/>
        <Events_enabled_in_init_ v="yes"/>
      </group>
      <group name="CPU clock/speed selection">
        <High_speed_mode v="This component enabled"/>
        <Low_speed_mode v="This component disabled"/>
        <Slow_speed_mode v="This component disabled"/>
      </group>
    </Properties>

    <Methods>
      <Enable v="don&apos;t generate code"/>
      <Disable v="don&apos;t generate code"/>
      <EnableEvent v="don&apos;t generate code"/>
      <DisableEvent v="don&apos;t generate code"/>
      <RecvChar v="generate code"/>
      <SendChar v="generate code"/>
      <RecvBlock v="don&apos;t generate code"/>
      <SendBlock v="don&apos;t generate code"/>
      <ClearRxBuf v="don&apos;t generate code"/>
      <ClearTxBuf v="don&apos;t generate code"/>
      <CharsInRxBuf v="don&apos;t generate code"/>
      <GetCharsInRxBuf v="generate code"/>
      <CharsInTxBuf v="don&apos;t generate code"/>
      <GetCharsInTxBuf v="generate code"/>
      <SetBaudRateMode v="don&apos;t generate code"/>
      <GetError v="don&apos;t generate code"/>
      <GetBreak v="don&apos;t generate code"/>
      <SetBreak v="don&apos;t generate code"/>
      <TurnTxOn v="don&apos;t generate code"/>
      <TurnTxOff v="don&apos;t generate code"/>
      <TurnRxOn v="don&apos;t generate code"/>
      <TurnRxOff v="don&apos;t generate code"/>
      <LoopMode v="don&apos;t generate code"/>
      <SetIdle v="don&apos;t generate code"/>
      <Standby v="don&apos;t generate code"/>
      <SetDirection v="don&apos;t generate code"/>
      <GetRxIdle v="don&apos;t generate code"/>
      <GetTxComplete v="don&apos;t generate code"/>
      <EnableRxEdgeDetect v="don&apos;t generate code"/>
      <DisableRxEdgeDetect v="don&apos;t generate code"/>
    </Methods>

    <Events>
      <Event_module_name v="Events"/>
      <event name="BeforeNewSpeed" v="don&apos;t generate code" />
      <event name="AfterNewSpeed" v="don&apos;t generate code" />
      <event name="OnError" v="don&apos;t generate code" />
      <event name="OnRxChar" v="don&apos;t generate code" />
      <event name="OnRxCharExt" v="don&apos;t generate code" />
      <event name="OnTxChar" v="don&apos;t generate code" />
      <event name="OnFullRxBuf" v="don&apos;t generate code" />
      <event name="OnFreeTxBuf" v="don&apos;t generate code" />
      <event name="OnBreak" v="don&apos;t generate code" />
      <event name="OnIdle" v="don&apos;t generate code" />
      <event name="OnTxComplete" v="don&apos;t generate code" />
      <event name="OnRxActiveEdge" v="don&apos;t generate code" />
    </Events>
  </Bean>

  <Bean name="ACCEL_SLEEP_B" type="BitIO">
    <Enabled v="Y"/>

    <Properties>
      <Component_name v="ACCEL_SLEEP_B"/>
      <Pin_for_I_O v="PTB5_MOSI_SCL"/>
      <Pin_signal v=""/>
      <Pull_resistor v="pull up"/>
      <Open_drain v="push-pull"/>
      <Slew_rate_control_for_PTB5 v="no"/>
      <Drive_strength_for_PTB5 v="Low"/>
      <Direction v="Input/Output"/>
      <group name="Initialization">
        <Init__direction v="Output"/>
        <Init__value v="0"/>
      </group>
      <Safe_mode v="yes"/>
      <Optimization_for v="speed"/>
    </Properties>

    <Methods>
      <GetDir v="don&apos;t generate code"/>
      <SetDir v="generate code"/>
      <SetInput v="don&apos;t generate code"/>
      <SetOutput v="don&apos;t generate code"/>
      <GetVal v="generate code"/>
      <PutVal v="generate code"/>
      <ClrVal v="generate code"/>
      <SetVal v="generate code"/>
      <NegVal v="don&apos;t generate code"/>
    </Methods>

    <Events>
    </Events>
  </Bean>

  <Bean name="KBI1" type="Init_KBI">
    <Enabled v="Y"/>

    <Properties>
      <Component_name v="KBI1"/>
      <Device v="KBI"/>
      <group name="Settings">
        <Triggering_sensitivity v="edge"/>
        <KBI_Clock_Gate v="Enabled"/>
      </group>
      <group name="Pins">
        <boolgroup name="Pin0" v="Disabled" />
        <boolgroup name="Pin1" v="Disabled" />
        <boolgroup name="Pin2" v="Disabled" />
        <boolgroup name="Pin3" v="Disabled" />
        <boolgroup name="Pin4" v="Enabled">
          <Pin v="PTA4_KBIP4_ADP8_LCD43"/>
          <Pin_signal v=""/>
          <Pull_resistor v="pull enabled"/>
          <Interrupt_polarity v="low level and/or falling edge"/>
        </boolgroup>
        <boolgroup name="Pin5" v="Disabled" />
        <boolgroup name="Pin6" v="Disabled" />
        <boolgroup name="Pin7" v="Enabled">
          <Pin v="PTA7_KBIP7_ADP11_ACMPMINUS"/>
          <Pin_signal v=""/>
          <Pull_resistor v="pull enabled"/>
          <Interrupt_polarity v="low level and/or falling edge"/>
        </boolgroup>
      </group>
      <group name="Interrupts/DMA">
        <group name="Keyboard request">
          <Interrupt v="Vkeyboard"/>
          <Keyboard_request_interrupt v="Enabled"/>
          <ISR_name v="KBI_ISR"/>
        </group>
      </group>
      <group name="Initialization">
        <Call_Init_method v="yes"/>
      </group>
    </Properties>

    <Methods>
      <Init v="generate code"/>
    </Methods>

    <Events>
    </Events>
  </Bean>

</PE_PROJECT_SETTINGS_DOCUMENTATION>
