/*!
\page page_pinalloc Pin Allocation

		<h2 style='font-family: Arial;'>Pin Allocation Report</h2>
		<table cellpadding='2' border='1' style='border: 2px solid #000000;' bgcolor='WHITE' align='center'>
			<tr bgcolor='#E8E8E8'><th>Peripheral</th><th>Custom peripheral name</th><th>Peripheral description</th></tr>
			<tr bgcolor='#F8FF9A'><td>ADC0</td><td>ADC0</td><td><small>Analog-to-Digital Converter</small></td></tr>
			<tr bgcolor='#F8FF9A'><td>ADC1</td><td>ADC1</td><td><small>Analog-to-Digital Converter</small></td></tr>
			<tr bgcolor='#EFF174'><td>CMP0</td><td>CMP0</td><td><small>High-Speed Comparator (CMP), Voltage Reference (VREF) Digital-to-Analog Converter (DAC), and Analog Mux (ANMUX)</small></td></tr>
			<tr bgcolor='#EFF174'><td>CMP1</td><td>CMP1</td><td><small>High-Speed Comparator (CMP), Voltage Reference (VREF) Digital-to-Analog Converter (DAC), and Analog Mux (ANMUX)</small></td></tr>
			<tr bgcolor='#FFE1C7'><td>CoreDebug</td><td>CoreDebug</td><td><small>ARM Core M0+ debugger</small></td></tr>
			<tr bgcolor='#E5E44D'><td>DAC0</td><td>DAC0</td><td><small>12-Bit Digital-to-Analog Converter</small></td></tr>
			<tr bgcolor='#CEFFFF'><td>EWM</td><td>EWM</td><td><small>External Watchdog Monitor</small></td></tr>
			<tr bgcolor='#B3EAFF'><td>FTM0</td><td>FTM0</td><td><small>FlexTimer Module</small></td></tr>
			<tr bgcolor='#B3EAFF'><td>FTM1</td><td>FTM1</td><td><small>FlexTimer Module</small></td></tr>
			<tr bgcolor='#B3EAFF'><td>FTM2</td><td>FTM2</td><td><small>FlexTimer Module</small></td></tr>
			<tr bgcolor='#F7DCFF'><td>GPIOA</td><td>GPIOA</td><td><small>General Purpose Input/Output</small></td></tr>
			<tr bgcolor='#F7DCFF'><td>GPIOB</td><td>GPIOB</td><td><small>General Purpose Input/Output</small></td></tr>
			<tr bgcolor='#F7DCFF'><td>GPIOC</td><td>GPIOC</td><td><small>General Purpose Input/Output</small></td></tr>
			<tr bgcolor='#F7DCFF'><td>GPIOD</td><td>GPIOD</td><td><small>General Purpose Input/Output</small></td></tr>
			<tr bgcolor='#F7DCFF'><td>GPIOE</td><td>GPIOE</td><td><small>General Purpose Input/Output</small></td></tr>
			<tr bgcolor='#AFFF8E'><td>I2C0</td><td>I2C0</td><td><small>Inter-integrated circuit bus</small></td></tr>
			<tr bgcolor='#DDC7B5'><td>LLWU</td><td>LLWU</td><td><small>Low Leakage Wake-up Unit</small></td></tr>
			<tr bgcolor='#86DAFF'><td>LPTMR0</td><td>LPTMR0</td><td><small>Low Power Timer Module</small></td></tr>
			<tr bgcolor='#CCB6A0'><td>OSC0</td><td>OSC0</td><td><small>Oscillator</small></td></tr>
			<tr bgcolor='#58C7FF'><td>PDB0</td><td>PDB0</td><td><small>Programmable Delay Block</small></td></tr>
			<tr bgcolor='#C7A886'><td>PMC</td><td>PMC</td><td><small>Power Management Controller</small></td></tr>
			<tr bgcolor='#FFE1C7'><td>RCM</td><td>RCM</td><td><small>Reset Control Module</small></td></tr>
			<tr bgcolor='#DDC7B5'><td>SIM</td><td>SIM</td><td><small>System Integration Module</small></td></tr>
			<tr bgcolor='#90EE67'><td>SPI0</td><td>SPI0</td><td><small>Deserial Serial Peripheral Interface 0</small></td></tr>
			<tr bgcolor='#EBD4BD'><td>SystemControl</td><td>SystemControl</td><td><small>System control</small></td></tr>
			<tr bgcolor='#5FE356'><td>UART0</td><td>UART0</td><td><small>Serial Communications Interface Module UART0</small></td></tr>
			<tr bgcolor='#5FE356'><td>UART1</td><td>UART1</td><td><small>Serial Communications Interface Module UART1</small></td></tr>
		</table>
		<br/>
		<br/>

		<h2 style='font-family: Arial;'>Routed Pins</h2>
		<table cellpadding='2' border='1' style='border: 2px solid #000000;' bgcolor='WHITE' width='100%' align='center'>
			<tr><td colspan='3'></td><th colspan='4' align='center' bgcolor='#D0D0D0'>Assigned Pin Function(s)</th></tr>
			<tr>
				<th bgcolor='#E8E8E8'>Package Pin #</th><th bgcolor='#E8E8E8'>Pin Name</th><th bgcolor='#E8E8E8'>User Assigned Signal Name</th><th bgcolor='#E8E8E8'>Assigned Peripheral</th><th bgcolor='#E8E8E8'>Assigned Function</th><th bgcolor='#E8E8E8'>Package Function</th><th bgcolor='#E8E8E8'>Dir</th>
			</tr>
			<tr>
				<td>1</td><td>VDD1</td><td><small><i>same</i></small></td>
				<td bgcolor='#C7A886'>PMC</td><td bgcolor='#C7A886'>vdd1</td><td bgcolor='#C7A886'>alt0</td><td bgcolor='#C7A886'>Input</td>
			</tr>
			<tr>
				<td>2</td><td>VSS2</td><td><small><i>same</i></small></td>
				<td bgcolor='#C7A886'>PMC</td><td bgcolor='#C7A886'>vss2</td><td bgcolor='#C7A886'>alt0</td><td bgcolor='#C7A886'>Input</td>
			</tr>
			<tr>
				<td rowspan='3'>3</td><td rowspan='3'>ADC0_SE1/ADC0_DP1/ADC1_SE0/PTE16/SPI0_PCS0/SS_b/UART1_TX/FTM_CLKIN0/FTM0_FLT3</td><td rowspan='3'><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_se1</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#F8FF9A'><td>ADC0</td><td>adc_dp1</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#F8FF9A'><td>ADC1</td><td>adc_se0</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td rowspan='3'>4</td><td rowspan='3'>ADC0_SE5/ADC0_DM1/ADC1_SE5/PTE17/SPI0_SCK/UART1_RX/FTM_CLKIN1/LPTMR0_ALT3</td><td rowspan='3'><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_sea5</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#F8FF9A'><td>ADC0</td><td>adc_dm1</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#F8FF9A'><td>ADC1</td><td>adc_sea5</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td rowspan='3'>5</td><td rowspan='3'>ADC0_SE6/ADC1_SE1/ADC1_DP1/PTE18/SPI0_SOUT/UART1_CTS_b/I2C0_SDA/SPI0_SIN</td><td rowspan='3'><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_sea6</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#F8FF9A'><td>ADC1</td><td>adc_se1</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#F8FF9A'><td>ADC1</td><td>adc_dp1</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td rowspan='3'>6</td><td rowspan='3'>ADC0_SE7/ADC1_SE7/ADC1_DM1/PTE19/SPI0_SIN/UART1_RTS_b/I2C0_SCL/SPI0_SOUT</td><td rowspan='3'><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_sea7</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#F8FF9A'><td>ADC1</td><td>adc_sea7</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#F8FF9A'><td>ADC1</td><td>adc_dm1</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td rowspan='2'>7</td><td rowspan='2'>ADC0_SE0/ADC0_DP0/PTE20/FTM1_CH0/UART0_TX</td><td rowspan='2'><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_se0</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#F8FF9A'><td>ADC0</td><td>adc_dp0</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td rowspan='2'>8</td><td rowspan='2'>ADC0_SE4/ADC0_DM0/PTE21/FTM1_CH1/UART0_RX</td><td rowspan='2'><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_sea4</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#F8FF9A'><td>ADC0</td><td>adc_dm0</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td>9</td><td>VDDA</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td rowspan='6'>10</td><td rowspan='6'>VREFH</td><td rowspan='6'><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_vrefh</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#F8FF9A'><td>ADC0</td><td>adc_se29</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#F8FF9A'><td>ADC0</td><td>adc_dp29</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#F8FF9A'><td>ADC1</td><td>adc_vrefh</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#F8FF9A'><td>ADC1</td><td>adc_se29</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#F8FF9A'><td>ADC1</td><td>adc_dp29</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td rowspan='6'>11</td><td rowspan='6'>VREFL</td><td rowspan='6'><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_vrefl</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#F8FF9A'><td>ADC0</td><td>adc_se30</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#F8FF9A'><td>ADC0</td><td>adc_dm29</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#F8FF9A'><td>ADC1</td><td>adc_vrefl</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#F8FF9A'><td>ADC1</td><td>adc_se30</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#F8FF9A'><td>ADC1</td><td>adc_dm29</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td>12</td><td>VSSA</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>13</td><td>CMP1_IN5/CMP0_IN5/PTE29/FTM0_CH2/FTM_CLKIN0</td><td><small><i>same</i></small></td>
				<td bgcolor='#B3EAFF'>FTM0</td><td bgcolor='#B3EAFF'>tmr_ch2</td><td bgcolor='#B3EAFF'>alt3</td><td bgcolor='#B3EAFF'>Output</td>
			</tr>
			<tr>
				<td rowspan='9'>14</td><td rowspan='9'>ADC1_SE4/CMP0_IN4/CMP1_IN4/DAC0_OUT/PTE30/FTM0_CH3/FTM_CLKIN1</td><td rowspan='9'><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC1</td><td bgcolor='#F8FF9A'>adc_sea4</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#EFF174'><td>CMP0</td><td>cmp_in4</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#EFF174'><td>CMP0</td><td>Positive4</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#EFF174'><td>CMP0</td><td>Negative4</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#EFF174'><td>CMP1</td><td>cmp_in4</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#EFF174'><td>CMP1</td><td>Positive4</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#EFF174'><td>CMP1</td><td>Negative4</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#E5E44D'><td>DAC0</td><td>dacout</td><td>alt0</td><td>Output</td></tr>
			<tr bgcolor='#E5E44D'><td>DAC0</td><td>dac_out</td><td>alt0</td><td>Output</td></tr>
			<tr>
				<td>15</td><td>PTE24/FTM0_CH0/I2C0_SCL/EWM_OUT_b</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>16</td><td>PTE25/FTM0_CH1/I2C0_SDA/EWM_IN</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>17</td><td>PTA0/UART0_CTS_b/FTM0_CH5/SWD_CLK</td><td><small><i>same</i></small></td>
				<td bgcolor='#FFE1C7'>CoreDebug</td><td bgcolor='#FFE1C7'>swd_clk</td><td bgcolor='#FFE1C7'>alt7</td><td bgcolor='#FFE1C7'>Input/Output</td>
			</tr>
			<tr>
				<td>18</td><td>PTA1/UART0_RX/FTM2_CH0/CMP0_OUT/FTM2_QD_PHA/FTM1_CH1</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>19</td><td>PTA2/UART0_TX/FTM2_CH1/CMP1_OUT/FTM2_QD_PHB/FTM1_CH0</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>20</td><td>PTA3/UART0_RTS_b/FTM0_CH0/FTM2_FLT0/EWM_OUT_b/SWD_DIO</td><td><small><i>same</i></small></td>
				<td bgcolor='#FFE1C7'>CoreDebug</td><td bgcolor='#FFE1C7'>swd_dio</td><td bgcolor='#FFE1C7'>alt7</td><td bgcolor='#FFE1C7'>Input/Output</td>
			</tr>
			<tr>
				<td rowspan='2'>21</td><td rowspan='2'>PTA4/LLWU_P3/FTM0_CH1/FTM0_FLT3/NMI_b</td><td rowspan='2'><small><i>same</i></small></td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port4</td><td bgcolor='#F7DCFF'>alt1</td><td bgcolor='#F7DCFF'>Output</td>
			</tr>
			<tr bgcolor='#DDC7B5'><td>LLWU</td><td>wake_up3</td><td>alt1</td><td>Input</td></tr>
			<tr>
				<td>22</td><td>VDD22</td><td><small><i>same</i></small></td>
				<td bgcolor='#C7A886'>PMC</td><td bgcolor='#C7A886'>vdd22</td><td bgcolor='#C7A886'>alt0</td><td bgcolor='#C7A886'>Input</td>
			</tr>
			<tr>
				<td>23</td><td>VSS23</td><td><small><i>same</i></small></td>
				<td bgcolor='#C7A886'>PMC</td><td bgcolor='#C7A886'>vss23</td><td bgcolor='#C7A886'>alt0</td><td bgcolor='#C7A886'>Input</td>
			</tr>
			<tr>
				<td>24</td><td>EXTAL0/PTA18/FTM0_FLT2/FTM_CLKIN0</td><td><small><i>same</i></small></td>
				<td bgcolor='#CCB6A0'>OSC0</td><td bgcolor='#CCB6A0'>extal</td><td bgcolor='#CCB6A0'>alt0</td><td bgcolor='#CCB6A0'>Input</td>
			</tr>
			<tr>
				<td>25</td><td>XTAL0/PTA19/FTM0_FLT0/FTM1_FLT0/FTM_CLKIN1/LPTMR0_ALT1</td><td><small><i>same</i></small></td>
				<td bgcolor='#CCB6A0'>OSC0</td><td bgcolor='#CCB6A0'>xtal</td><td bgcolor='#CCB6A0'>alt0</td><td bgcolor='#CCB6A0'>Output</td>
			</tr>
			<tr>
				<td rowspan='2'>26</td><td rowspan='2'>PTA20/RESET_b</td><td rowspan='2'><small><i>same</i></small></td>
				<td bgcolor='#FFE1C7'>RCM</td><td bgcolor='#FFE1C7'>reset</td><td bgcolor='#FFE1C7'>alt7</td><td bgcolor='#FFE1C7'>Input</td>
			</tr>
			<tr bgcolor='#969696'><td>non-peripheral</td><td>RESET</td><td>alt7</td><td>Not Specified</td></tr>
			<tr>
				<td rowspan='2'>27</td><td rowspan='2'>ADC0_SE8/ADC1_SE8/PTB0/LLWU_P5/I2C0_SCL/FTM1_CH0/FTM1_QD_PHA/UART0_RX</td><td rowspan='2'><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_se8</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#F8FF9A'><td>ADC1</td><td>adc_se8</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td rowspan='2'>28</td><td rowspan='2'>ADC0_SE9/ADC1_SE9/PTB1/I2C0_SDA/FTM1_CH1/FTM0_FLT2/EWM_IN/FTM1_QD_PHB/UART0_TX</td><td rowspan='2'><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_se9</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#F8FF9A'><td>ADC1</td><td>adc_se9</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td rowspan='3'>29</td><td rowspan='3'>ADC0_SE10/ADC1_SE10/ADC1_DM2/PTB2/I2C0_SCL/UART0_RTS_b/FTM0_FLT1/FTM0_FLT3</td><td rowspan='3'><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_se10</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#F8FF9A'><td>ADC1</td><td>adc_se10</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#F8FF9A'><td>ADC1</td><td>adc_dm2</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td rowspan='2'>30</td><td rowspan='2'>ADC1_SE2/ADC1_DP2/PTB3/I2C0_SDA/UART0_CTS_b/FTM0_FLT0</td><td rowspan='2'><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC1</td><td bgcolor='#F8FF9A'>adc_se2</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#F8FF9A'><td>ADC1</td><td>adc_dp2</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td>31</td><td>PTB16/UART0_RX/FTM_CLKIN2/EWM_IN</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>32</td><td>PTB17/UART0_TX/FTM_CLKIN1/EWM_OUT_b</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>33</td><td>ADC1_SE11/PTC0/SPI0_PCS4/PDB0_EXTRG/CMP0_OUT/FTM0_FLT0/SPI0_PCS0/SS_b</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC1</td><td bgcolor='#F8FF9A'>adc_se11</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr>
				<td>34</td><td>ADC1_SE3/PTC1/LLWU_P6/SPI0_PCS3/UART1_RTS_b/FTM0_CH0/FTM2_CH0</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC1</td><td bgcolor='#F8FF9A'>adc_se3</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr>
				<td rowspan='4'>35</td><td rowspan='4'>ADC0_SE11/CMP1_IN0/PTC2/SPI0_PCS2/UART1_CTS_b/FTM0_CH1/FTM2_CH1</td><td rowspan='4'><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_se11</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#EFF174'><td>CMP1</td><td>cmp_in0</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#EFF174'><td>CMP1</td><td>Positive0</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#EFF174'><td>CMP1</td><td>Negative0</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td rowspan='3'>36</td><td rowspan='3'>CMP1_IN1/PTC3/LLWU_P7/SPI0_PCS1/UART1_RX/FTM0_CH2/CLKOUT</td><td rowspan='3'><small><i>same</i></small></td>
				<td bgcolor='#EFF174'>CMP1</td><td bgcolor='#EFF174'>cmp_in1</td><td bgcolor='#EFF174'>alt0</td><td bgcolor='#EFF174'>Input</td>
			</tr>
			<tr bgcolor='#EFF174'><td>CMP1</td><td>Positive1</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#EFF174'><td>CMP1</td><td>Negative1</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td>37</td><td>PTC4/LLWU_P8/SPI0_PCS0/SS_b/UART1_TX/FTM0_CH3/CMP1_OUT</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>38</td><td>PTC5/LLWU_P9/SPI0_SCK/LPTMR0_ALT2/CMP0_OUT/FTM0_CH2</td><td><small><i>same</i></small></td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_sck</td><td bgcolor='#90EE67'>alt2</td><td bgcolor='#90EE67'>Output</td>
			</tr>
			<tr>
				<td>39</td><td>CMP0_IN0/PTC6/LLWU_P10/SPI0_SOUT/PDB0_EXTRG/UART0_RX/I2C0_SCL</td><td><small><i>same</i></small></td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_txd</td><td bgcolor='#90EE67'>alt2</td><td bgcolor='#90EE67'>Output</td>
			</tr>
			<tr>
				<td rowspan='3'>40</td><td rowspan='3'>CMP0_IN1/PTC7/SPI0_SIN/UART0_TX/I2C0_SDA</td><td rowspan='3'><small><i>same</i></small></td>
				<td bgcolor='#EFF174'>CMP0</td><td bgcolor='#EFF174'>cmp_in1</td><td bgcolor='#EFF174'>alt0</td><td bgcolor='#EFF174'>Input</td>
			</tr>
			<tr bgcolor='#EFF174'><td>CMP0</td><td>Positive1</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#EFF174'><td>CMP0</td><td>Negative1</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td>41</td><td>PTD0/LLWU_P12/SPI0_PCS0/SS_b/UART0_CTS_b/FTM0_CH0/UART1_RX</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>42</td><td>ADC0_SE2/PTD1/SPI0_SCK/UART0_RTS_b/FTM0_CH1/UART1_TX</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_se2</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr>
				<td>43</td><td>PTD2/LLWU_P13/SPI0_SOUT/UART0_RX/FTM0_CH2/I2C0_SCL</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>44</td><td>PTD3/SPI0_SIN/UART0_TX/FTM0_CH3/I2C0_SDA</td><td><small><i>same</i></small></td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_rxd</td><td bgcolor='#90EE67'>alt2</td><td bgcolor='#90EE67'>Input</td>
			</tr>
			<tr>
				<td>45</td><td>PTD4/LLWU_P14/SPI0_PCS1/UART0_RTS_b/FTM0_CH4/FTM2_CH0/EWM_IN</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>46</td><td>ADC0_SE3/PTD5/SPI0_PCS2/UART0_CTS_b/FTM0_CH5/FTM2_CH1/EWM_OUT_b</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_se3</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr>
				<td rowspan='2'>47</td><td rowspan='2'>ADC1_SE6/PTD6/LLWU_P15/SPI0_PCS3/UART0_RX/FTM0_CH0/FTM1_CH0/FTM0_FLT0</td><td rowspan='2'><small><i>same</i></small></td>
				<td bgcolor='#F7DCFF'>GPIOD</td><td bgcolor='#F7DCFF'>port6</td><td bgcolor='#F7DCFF'>alt1</td><td bgcolor='#F7DCFF'>Output</td>
			</tr>
			<tr bgcolor='#DDC7B5'><td>LLWU</td><td>wake_up15</td><td>alt1</td><td>Input</td></tr>
			<tr>
				<td>48</td><td>PTD7/UART0_TX/FTM0_CH1/FTM1_CH1/FTM0_FLT1</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td><td></td>
			</tr>
		</table>

		<h2 style='font-family: Arial;'>Routable Pins</h2>
		<table cellpadding='2' border='1' style='border: 2px solid #000000;' bgcolor='WHITE' width='100%' align='center'>
			<tr><td colspan='3'></td><th colspan='3' align='center' bgcolor='#D0D0D0'>alt0</th><th colspan='3' align='center' bgcolor='#D0D0D0'>alt1</th><th colspan='3' align='center' bgcolor='#D0D0D0'>alt2</th><th colspan='3' align='center' bgcolor='#D0D0D0'>alt3</th><th colspan='3' align='center' bgcolor='#D0D0D0'>alt4</th><th colspan='3' align='center' bgcolor='#D0D0D0'>alt5</th><th colspan='3' align='center' bgcolor='#D0D0D0'>alt6</th><th colspan='3' align='center' bgcolor='#D0D0D0'>alt7</th></tr>
			<tr>
				<th bgcolor='#E8E8E8'>Package Pin #</th><th bgcolor='#E8E8E8'>Pin Name</th><th bgcolor='#E8E8E8'>User Assigned Signal Name</th>
				<th bgcolor='#E8E8E8'>Peripheral</th><th bgcolor='#E8E8E8'>Function</th><th bgcolor='#E8E8E8'>Dir</th>
				<th bgcolor='#E8E8E8'>Peripheral</th><th bgcolor='#E8E8E8'>Function</th><th bgcolor='#E8E8E8'>Dir</th>
				<th bgcolor='#E8E8E8'>Peripheral</th><th bgcolor='#E8E8E8'>Function</th><th bgcolor='#E8E8E8'>Dir</th>
				<th bgcolor='#E8E8E8'>Peripheral</th><th bgcolor='#E8E8E8'>Function</th><th bgcolor='#E8E8E8'>Dir</th>
				<th bgcolor='#E8E8E8'>Peripheral</th><th bgcolor='#E8E8E8'>Function</th><th bgcolor='#E8E8E8'>Dir</th>
				<th bgcolor='#E8E8E8'>Peripheral</th><th bgcolor='#E8E8E8'>Function</th><th bgcolor='#E8E8E8'>Dir</th>
				<th bgcolor='#E8E8E8'>Peripheral</th><th bgcolor='#E8E8E8'>Function</th><th bgcolor='#E8E8E8'>Dir</th>
				<th bgcolor='#E8E8E8'>Peripheral</th><th bgcolor='#E8E8E8'>Function</th><th bgcolor='#E8E8E8'>Dir</th>
			</tr>
			<tr>
				<td>1</td><td>VDD1</td><td><small><i>same</i></small></td>
				<td bgcolor='#C7A886'>PMC</td><td bgcolor='#C7A886'>vdd1</td><td bgcolor='#C7A886'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>2</td><td>VSS2</td><td><small><i>same</i></small></td>
				<td bgcolor='#C7A886'>PMC</td><td bgcolor='#C7A886'>vss2</td><td bgcolor='#C7A886'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>3</td><td>ADC0_SE1/ADC0_DP1/ADC1_SE0/PTE16/SPI0_PCS0/SS_b/UART1_TX/FTM_CLKIN0/FTM0_FLT3</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0<br/>ADC0<br/>ADC1</td><td bgcolor='#F8FF9A'>adc_se1<br/>adc_dp1<br/>adc_se0</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port16</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_cs0</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#FFFFFF'>UART1<br/>SIM</td><td bgcolor='#FFFFFF'>uart_tx<br/>uart_tx1</td><td bgcolor='#FFFFFF'>Output</td>
				<td bgcolor='#B3EAFF'>FTM0<br/>FTM1<br/>FTM2</td><td bgcolor='#B3EAFF'>tmr_clk</td><td bgcolor='#B3EAFF'>Input</td>
				<td></td><td></td><td></td>
				<td bgcolor='#B3EAFF'>FTM0</td><td bgcolor='#B3EAFF'>tmr_fault3</td><td bgcolor='#B3EAFF'>Input</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>4</td><td>ADC0_SE5/ADC0_DM1/ADC1_SE5/PTE17/SPI0_SCK/UART1_RX/FTM_CLKIN1/LPTMR0_ALT3</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0<br/>ADC0<br/>ADC1</td><td bgcolor='#F8FF9A'>adc_sea5<br/>adc_dm1<br/>adc_sea5</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port17</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_sck</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#5FE356'>UART1</td><td bgcolor='#5FE356'>uart_rx</td><td bgcolor='#5FE356'>Input</td>
				<td bgcolor='#B3EAFF'>FTM0<br/>FTM1<br/>FTM2</td><td bgcolor='#B3EAFF'>tmr_clk</td><td bgcolor='#B3EAFF'>Input</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>LPTMR0</td><td bgcolor='#86DAFF'>tmr_clk3</td><td bgcolor='#86DAFF'>Input</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>5</td><td>ADC0_SE6/ADC1_SE1/ADC1_DP1/PTE18/SPI0_SOUT/UART1_CTS_b/I2C0_SDA/SPI0_SIN</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0<br/>ADC1<br/>ADC1</td><td bgcolor='#F8FF9A'>adc_sea6<br/>adc_se1<br/>adc_dp1</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port18</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_txd</td><td bgcolor='#90EE67'>Output</td>
				<td bgcolor='#5FE356'>UART1</td><td bgcolor='#5FE356'>uart_cts</td><td bgcolor='#5FE356'>Input</td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sda</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_rxd</td><td bgcolor='#90EE67'>Input</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>6</td><td>ADC0_SE7/ADC1_SE7/ADC1_DM1/PTE19/SPI0_SIN/UART1_RTS_b/I2C0_SCL/SPI0_SOUT</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0<br/>ADC1<br/>ADC1</td><td bgcolor='#F8FF9A'>adc_sea7<br/>adc_sea7<br/>adc_dm1</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port19</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_rxd</td><td bgcolor='#90EE67'>Input</td>
				<td bgcolor='#5FE356'>UART1</td><td bgcolor='#5FE356'>uart_rts</td><td bgcolor='#5FE356'>Output</td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sclk</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_txd</td><td bgcolor='#90EE67'>Output</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>7</td><td>ADC0_SE0/ADC0_DP0/PTE20/FTM1_CH0/UART0_TX</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_se0<br/>adc_dp0</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port20</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#B3EAFF'>FTM1</td><td bgcolor='#B3EAFF'>tmr_ch0</td><td bgcolor='#B3EAFF'>Input, Output</td>
				<td bgcolor='#FFFFFF'>UART0<br/>SIM</td><td bgcolor='#FFFFFF'>uart_tx<br/>uart_tx0</td><td bgcolor='#FFFFFF'>Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>8</td><td>ADC0_SE4/ADC0_DM0/PTE21/FTM1_CH1/UART0_RX</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_sea4<br/>adc_dm0</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port21</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>FTM1<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch1<br/>tmr_xorFTM1_CH1</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#5FE356'>UART0</td><td bgcolor='#5FE356'>uart_rx</td><td bgcolor='#5FE356'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>9</td><td>VDDA</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0<br/>ADC0<br/>ADC0<br/>ADC0<br/>ADC1<br/>ADC1<br/>ADC1</td><td bgcolor='#F8FF9A'>adc_vdda_se29_dp29<br/>adc_vrefh<br/>adc_se29<br/>adc_dp29<br/>adc_vrefh<br/>adc_se29<br/>adc_dp29</td><td bgcolor='#F8FF9A'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>10</td><td>VREFH</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0<br/>ADC0<br/>ADC0<br/>ADC0<br/>ADC1<br/>ADC1<br/>ADC1</td><td bgcolor='#F8FF9A'>adc_vrefh_se29_dp29<br/>adc_vrefh<br/>adc_se29<br/>adc_dp29<br/>adc_vrefh<br/>adc_se29<br/>adc_dp29</td><td bgcolor='#F8FF9A'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>11</td><td>VREFL</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0<br/>ADC0<br/>ADC0<br/>ADC0<br/>ADC1<br/>ADC1<br/>ADC1</td><td bgcolor='#F8FF9A'>adc_vrefl_se30_dm29<br/>adc_vrefl<br/>adc_se30<br/>adc_dm29<br/>adc_vrefl<br/>adc_se30<br/>adc_dm29</td><td bgcolor='#F8FF9A'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>12</td><td>VSSA</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0<br/>ADC0<br/>ADC0<br/>ADC0<br/>ADC1<br/>ADC1<br/>ADC1</td><td bgcolor='#F8FF9A'>adc_vssa_se30_dm29<br/>adc_vrefl<br/>adc_se30<br/>adc_dm29<br/>adc_vrefl<br/>adc_se30<br/>adc_dm29</td><td bgcolor='#F8FF9A'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>13</td><td>CMP1_IN5/CMP0_IN5/PTE29/FTM0_CH2/FTM_CLKIN0</td><td><small><i>same</i></small></td>
				<td bgcolor='#EFF174'>CMP1<br/>CMP1<br/>CMP1<br/>CMP0<br/>CMP0<br/>CMP0</td><td bgcolor='#EFF174'>cmp_in5<br/>Positive5<br/>Negative5<br/>cmp_in5<br/>Positive5<br/>Negative5</td><td bgcolor='#EFF174'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port29</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch2<br/>tmr0_ch2</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#B3EAFF'>FTM0<br/>FTM1<br/>FTM2</td><td bgcolor='#B3EAFF'>tmr_clk</td><td bgcolor='#B3EAFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>14</td><td>ADC1_SE4/CMP0_IN4/CMP1_IN4/DAC0_OUT/PTE30/FTM0_CH3/FTM_CLKIN1</td><td><small><i>same</i></small></td>
				<td bgcolor='#FFFFFF'>ADC1<br/>CMP0<br/>CMP0<br/>CMP0<br/>CMP1<br/>CMP1<br/>CMP1<br/>DAC0<br/>DAC0</td><td bgcolor='#FFFFFF'>adc_sea4<br/>cmp_in4<br/>Positive4<br/>Negative4<br/>cmp_in4<br/>Positive4<br/>Negative4<br/>dacout<br/>dac_out</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port30</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch3<br/>tmr0_ch3</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#B3EAFF'>FTM0<br/>FTM1<br/>FTM2</td><td bgcolor='#B3EAFF'>tmr_clk</td><td bgcolor='#B3EAFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>15</td><td>PTE24/FTM0_CH0/I2C0_SCL/EWM_OUT_b</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port24</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch0<br/>tmr0_ch0</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sclk</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td bgcolor='#CEFFFF'>EWM</td><td bgcolor='#CEFFFF'>ewmoutput<br/>ewm_out</td><td bgcolor='#CEFFFF'>Output</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>16</td><td>PTE25/FTM0_CH1/I2C0_SDA/EWM_IN</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port25</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch1<br/>tmr0_ch1</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sda</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td bgcolor='#CEFFFF'>EWM</td><td bgcolor='#CEFFFF'>ewminput<br/>ewm_in</td><td bgcolor='#CEFFFF'>Input</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>17</td><td>PTA0/UART0_CTS_b/FTM0_CH5/SWD_CLK</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port0</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#5FE356'>UART0</td><td bgcolor='#5FE356'>uart_cts</td><td bgcolor='#5FE356'>Input</td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch5<br/>tmr0_ch5</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFE1C7'>CoreDebug</td><td bgcolor='#FFE1C7'>swd_clk</td><td bgcolor='#FFE1C7'>Input/Output</td>
			</tr>
			<tr>
				<td>18</td><td>PTA1/UART0_RX/FTM2_CH0/CMP0_OUT/FTM2_QD_PHA/FTM1_CH1</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port1</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#5FE356'>UART0</td><td bgcolor='#5FE356'>uart_rx</td><td bgcolor='#5FE356'>Input</td>
				<td bgcolor='#FFFFFF'>FTM2<br/>SIM<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch0<br/>tmr2_ch0<br/>tmr_xorFTM2_CH0</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#EFF174'>CMP0</td><td bgcolor='#EFF174'>Output</td><td bgcolor='#EFF174'>Output</td>
				<td bgcolor='#B3EAFF'>FTM2</td><td bgcolor='#B3EAFF'>tmr_qd_phA</td><td bgcolor='#B3EAFF'>Input</td>
				<td bgcolor='#FFFFFF'>FTM1<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch1<br/>tmr_xorFTM1_CH1</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>19</td><td>PTA2/UART0_TX/FTM2_CH1/CMP1_OUT/FTM2_QD_PHB/FTM1_CH0</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port2</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#FFFFFF'>UART0<br/>SIM</td><td bgcolor='#FFFFFF'>uart_tx<br/>uart_tx0</td><td bgcolor='#FFFFFF'>Output</td>
				<td bgcolor='#FFFFFF'>FTM2<br/>SIM<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch1<br/>tmr2_ch1<br/>tmr_xorFTM2_CH1</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#EFF174'>CMP1</td><td bgcolor='#EFF174'>Output</td><td bgcolor='#EFF174'>Output</td>
				<td bgcolor='#B3EAFF'>FTM2</td><td bgcolor='#B3EAFF'>tmr_qd_phB</td><td bgcolor='#B3EAFF'>Input</td>
				<td bgcolor='#B3EAFF'>FTM1</td><td bgcolor='#B3EAFF'>tmr_ch0</td><td bgcolor='#B3EAFF'>Input, Output</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>20</td><td>PTA3/UART0_RTS_b/FTM0_CH0/FTM2_FLT0/EWM_OUT_b/SWD_DIO</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port3</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#5FE356'>UART0</td><td bgcolor='#5FE356'>uart_rts</td><td bgcolor='#5FE356'>Output</td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch0<br/>tmr0_ch0</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#B3EAFF'>FTM2</td><td bgcolor='#B3EAFF'>tmr_fault0</td><td bgcolor='#B3EAFF'>Input</td>
				<td bgcolor='#CEFFFF'>EWM</td><td bgcolor='#CEFFFF'>ewmoutput<br/>ewm_out</td><td bgcolor='#CEFFFF'>Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFE1C7'>CoreDebug</td><td bgcolor='#FFE1C7'>swd_dio</td><td bgcolor='#FFE1C7'>Input/Output</td>
			</tr>
			<tr>
				<td>21</td><td>PTA4/LLWU_P3/FTM0_CH1/FTM0_FLT3/NMI_b</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>GPIOA<br/>LLWU</td><td bgcolor='#FFFFFF'>port4<br/>wake_up3</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch1<br/>tmr0_ch1</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#B3EAFF'>FTM0</td><td bgcolor='#B3EAFF'>tmr_fault3</td><td bgcolor='#B3EAFF'>Input</td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>SystemControl<br/>non-peripheral</td><td bgcolor='#FFFFFF'>scb_nmi<br/>NMI</td><td bgcolor='#FFFFFF'>Input</td>
			</tr>
			<tr>
				<td>22</td><td>VDD22</td><td><small><i>same</i></small></td>
				<td bgcolor='#C7A886'>PMC</td><td bgcolor='#C7A886'>vdd22</td><td bgcolor='#C7A886'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>23</td><td>VSS23</td><td><small><i>same</i></small></td>
				<td bgcolor='#C7A886'>PMC</td><td bgcolor='#C7A886'>vss23</td><td bgcolor='#C7A886'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>24</td><td>EXTAL0/PTA18/FTM0_FLT2/FTM_CLKIN0</td><td><small><i>same</i></small></td>
				<td bgcolor='#CCB6A0'>OSC0</td><td bgcolor='#CCB6A0'>extal</td><td bgcolor='#CCB6A0'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port18</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#B3EAFF'>FTM0</td><td bgcolor='#B3EAFF'>tmr_fault2</td><td bgcolor='#B3EAFF'>Input</td>
				<td bgcolor='#B3EAFF'>FTM0<br/>FTM1<br/>FTM2</td><td bgcolor='#B3EAFF'>tmr_clk</td><td bgcolor='#B3EAFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>25</td><td>XTAL0/PTA19/FTM0_FLT0/FTM1_FLT0/FTM_CLKIN1/LPTMR0_ALT1</td><td><small><i>same</i></small></td>
				<td bgcolor='#CCB6A0'>OSC0</td><td bgcolor='#CCB6A0'>xtal</td><td bgcolor='#CCB6A0'>Output</td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port19</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#B3EAFF'>FTM0</td><td bgcolor='#B3EAFF'>tmr_fault0</td><td bgcolor='#B3EAFF'>Input</td>
				<td bgcolor='#B3EAFF'>FTM1</td><td bgcolor='#B3EAFF'>tmr_fault0</td><td bgcolor='#B3EAFF'>Input</td>
				<td bgcolor='#B3EAFF'>FTM0<br/>FTM1<br/>FTM2</td><td bgcolor='#B3EAFF'>tmr_clk</td><td bgcolor='#B3EAFF'>Input</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>LPTMR0</td><td bgcolor='#86DAFF'>tmr_clk1</td><td bgcolor='#86DAFF'>Input</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>26</td><td>PTA20/RESET_b</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port20</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>RCM<br/>non-peripheral</td><td bgcolor='#FFFFFF'>reset<br/>RESET</td><td bgcolor='#FFFFFF'>Input</td>
			</tr>
			<tr>
				<td>27</td><td>ADC0_SE8/ADC1_SE8/PTB0/LLWU_P5/I2C0_SCL/FTM1_CH0/FTM1_QD_PHA/UART0_RX</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0<br/>ADC1</td><td bgcolor='#F8FF9A'>adc_se8</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#FFFFFF'>GPIOB<br/>LLWU</td><td bgcolor='#FFFFFF'>port0<br/>wake_up5</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sclk</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td bgcolor='#B3EAFF'>FTM1</td><td bgcolor='#B3EAFF'>tmr_ch0</td><td bgcolor='#B3EAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#B3EAFF'>FTM1</td><td bgcolor='#B3EAFF'>tmr_qd_phA</td><td bgcolor='#B3EAFF'>Input</td>
				<td bgcolor='#5FE356'>UART0</td><td bgcolor='#5FE356'>uart_rx</td><td bgcolor='#5FE356'>Input</td>
			</tr>
			<tr>
				<td>28</td><td>ADC0_SE9/ADC1_SE9/PTB1/I2C0_SDA/FTM1_CH1/FTM0_FLT2/EWM_IN/FTM1_QD_PHB/UART0_TX</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0<br/>ADC1</td><td bgcolor='#F8FF9A'>adc_se9</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOB</td><td bgcolor='#F7DCFF'>port1</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sda</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td bgcolor='#FFFFFF'>FTM1<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch1<br/>tmr_xorFTM1_CH1</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#B3EAFF'>FTM0</td><td bgcolor='#B3EAFF'>tmr_fault2</td><td bgcolor='#B3EAFF'>Input</td>
				<td bgcolor='#CEFFFF'>EWM</td><td bgcolor='#CEFFFF'>ewminput<br/>ewm_in</td><td bgcolor='#CEFFFF'>Input</td>
				<td bgcolor='#B3EAFF'>FTM1</td><td bgcolor='#B3EAFF'>tmr_qd_phB</td><td bgcolor='#B3EAFF'>Input</td>
				<td bgcolor='#FFFFFF'>UART0<br/>SIM</td><td bgcolor='#FFFFFF'>uart_tx<br/>uart_tx0</td><td bgcolor='#FFFFFF'>Output</td>
			</tr>
			<tr>
				<td>29</td><td>ADC0_SE10/ADC1_SE10/ADC1_DM2/PTB2/I2C0_SCL/UART0_RTS_b/FTM0_FLT1/FTM0_FLT3</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0<br/>ADC1<br/>ADC1</td><td bgcolor='#F8FF9A'>adc_se10<br/>adc_se10<br/>adc_dm2</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOB</td><td bgcolor='#F7DCFF'>port2</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sclk</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td bgcolor='#5FE356'>UART0</td><td bgcolor='#5FE356'>uart_rts</td><td bgcolor='#5FE356'>Output</td>
				<td bgcolor='#B3EAFF'>FTM0</td><td bgcolor='#B3EAFF'>tmr_fault1</td><td bgcolor='#B3EAFF'>Input</td>
				<td></td><td></td><td></td>
				<td bgcolor='#B3EAFF'>FTM0</td><td bgcolor='#B3EAFF'>tmr_fault3</td><td bgcolor='#B3EAFF'>Input</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>30</td><td>ADC1_SE2/ADC1_DP2/PTB3/I2C0_SDA/UART0_CTS_b/FTM0_FLT0</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC1</td><td bgcolor='#F8FF9A'>adc_se2<br/>adc_dp2</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOB</td><td bgcolor='#F7DCFF'>port3</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sda</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td bgcolor='#5FE356'>UART0</td><td bgcolor='#5FE356'>uart_cts</td><td bgcolor='#5FE356'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#B3EAFF'>FTM0</td><td bgcolor='#B3EAFF'>tmr_fault0</td><td bgcolor='#B3EAFF'>Input</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>31</td><td>PTB16/UART0_RX/FTM_CLKIN2/EWM_IN</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOB</td><td bgcolor='#F7DCFF'>port16</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#5FE356'>UART0</td><td bgcolor='#5FE356'>uart_rx</td><td bgcolor='#5FE356'>Input</td>
				<td bgcolor='#B3EAFF'>FTM0<br/>FTM1<br/>FTM2</td><td bgcolor='#B3EAFF'>tmr_clk</td><td bgcolor='#B3EAFF'>Input</td>
				<td></td><td></td><td></td>
				<td bgcolor='#CEFFFF'>EWM</td><td bgcolor='#CEFFFF'>ewminput<br/>ewm_in</td><td bgcolor='#CEFFFF'>Input</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>32</td><td>PTB17/UART0_TX/FTM_CLKIN1/EWM_OUT_b</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOB</td><td bgcolor='#F7DCFF'>port17</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>UART0<br/>SIM</td><td bgcolor='#FFFFFF'>uart_tx<br/>uart_tx0</td><td bgcolor='#FFFFFF'>Output</td>
				<td bgcolor='#B3EAFF'>FTM0<br/>FTM1<br/>FTM2</td><td bgcolor='#B3EAFF'>tmr_clk</td><td bgcolor='#B3EAFF'>Input</td>
				<td></td><td></td><td></td>
				<td bgcolor='#CEFFFF'>EWM</td><td bgcolor='#CEFFFF'>ewmoutput<br/>ewm_out</td><td bgcolor='#CEFFFF'>Output</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>33</td><td>ADC1_SE11/PTC0/SPI0_PCS4/PDB0_EXTRG/CMP0_OUT/FTM0_FLT0/SPI0_PCS0/SS_b</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC1</td><td bgcolor='#F8FF9A'>adc_se11</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOC</td><td bgcolor='#F7DCFF'>port0</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_cs4</td><td bgcolor='#90EE67'>Output</td>
				<td bgcolor='#FFFFFF'>PDB0<br/>PDB0<br/>ADC0<br/>ADC0<br/>ADC1<br/>ADC1</td><td bgcolor='#FFFFFF'>PDBtrigger<br/>pdb_trig0<br/>ADCtriggerA<br/>ADCtriggerB<br/>ADCtriggerA<br/>ADCtriggerB</td><td bgcolor='#FFFFFF'>Input</td>
				<td></td><td></td><td></td>
				<td bgcolor='#EFF174'>CMP0</td><td bgcolor='#EFF174'>Output</td><td bgcolor='#EFF174'>Output</td>
				<td bgcolor='#B3EAFF'>FTM0</td><td bgcolor='#B3EAFF'>tmr_fault0</td><td bgcolor='#B3EAFF'>Input</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_cs0</td><td bgcolor='#90EE67'>Input, Output</td>
			</tr>
			<tr>
				<td>34</td><td>ADC1_SE3/PTC1/LLWU_P6/SPI0_PCS3/UART1_RTS_b/FTM0_CH0/FTM2_CH0</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC1</td><td bgcolor='#F8FF9A'>adc_se3</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#FFFFFF'>GPIOC<br/>LLWU</td><td bgcolor='#FFFFFF'>port1<br/>wake_up6</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_cs3</td><td bgcolor='#90EE67'>Output</td>
				<td bgcolor='#5FE356'>UART1</td><td bgcolor='#5FE356'>uart_rts</td><td bgcolor='#5FE356'>Output</td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch0<br/>tmr0_ch0</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#FFFFFF'>FTM2<br/>SIM<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch0<br/>tmr2_ch0<br/>tmr_xorFTM2_CH0</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>35</td><td>ADC0_SE11/CMP1_IN0/PTC2/SPI0_PCS2/UART1_CTS_b/FTM0_CH1/FTM2_CH1</td><td><small><i>same</i></small></td>
				<td bgcolor='#FFFFFF'>ADC0<br/>CMP1<br/>CMP1<br/>CMP1</td><td bgcolor='#FFFFFF'>adc_se11<br/>cmp_in0<br/>Positive0<br/>Negative0</td><td bgcolor='#FFFFFF'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOC</td><td bgcolor='#F7DCFF'>port2</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_cs2</td><td bgcolor='#90EE67'>Output</td>
				<td bgcolor='#5FE356'>UART1</td><td bgcolor='#5FE356'>uart_cts</td><td bgcolor='#5FE356'>Input</td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch1<br/>tmr0_ch1</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#FFFFFF'>FTM2<br/>SIM<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch1<br/>tmr2_ch1<br/>tmr_xorFTM2_CH1</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>36</td><td>CMP1_IN1/PTC3/LLWU_P7/SPI0_PCS1/UART1_RX/FTM0_CH2/CLKOUT</td><td><small><i>same</i></small></td>
				<td bgcolor='#EFF174'>CMP1</td><td bgcolor='#EFF174'>cmp_in1<br/>Positive1<br/>Negative1</td><td bgcolor='#EFF174'>Input</td>
				<td bgcolor='#FFFFFF'>GPIOC<br/>LLWU</td><td bgcolor='#FFFFFF'>port3<br/>wake_up7</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_cs1</td><td bgcolor='#90EE67'>Output</td>
				<td bgcolor='#5FE356'>UART1</td><td bgcolor='#5FE356'>uart_rx</td><td bgcolor='#5FE356'>Input</td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch2<br/>tmr0_ch2</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#DDC7B5'>SIM</td><td bgcolor='#DDC7B5'>ClockOutput0</td><td bgcolor='#DDC7B5'>Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>37</td><td>PTC4/LLWU_P8/SPI0_PCS0/SS_b/UART1_TX/FTM0_CH3/CMP1_OUT</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>GPIOC<br/>LLWU</td><td bgcolor='#FFFFFF'>port4<br/>wake_up8</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_cs0</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#FFFFFF'>UART1<br/>SIM</td><td bgcolor='#FFFFFF'>uart_tx<br/>uart_tx1</td><td bgcolor='#FFFFFF'>Output</td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch3<br/>tmr0_ch3</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#EFF174'>CMP1</td><td bgcolor='#EFF174'>Output</td><td bgcolor='#EFF174'>Output</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>38</td><td>PTC5/LLWU_P9/SPI0_SCK/LPTMR0_ALT2/CMP0_OUT/FTM0_CH2</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>GPIOC<br/>LLWU</td><td bgcolor='#FFFFFF'>port5<br/>wake_up9</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_sck</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#86DAFF'>LPTMR0</td><td bgcolor='#86DAFF'>tmr_clk2</td><td bgcolor='#86DAFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#EFF174'>CMP0</td><td bgcolor='#EFF174'>Output</td><td bgcolor='#EFF174'>Output</td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch2<br/>tmr0_ch2</td><td bgcolor='#FFFFFF'>Input, Output</td>
			</tr>
			<tr>
				<td>39</td><td>CMP0_IN0/PTC6/LLWU_P10/SPI0_SOUT/PDB0_EXTRG/UART0_RX/I2C0_SCL</td><td><small><i>same</i></small></td>
				<td bgcolor='#EFF174'>CMP0</td><td bgcolor='#EFF174'>cmp_in0<br/>Positive0<br/>Negative0</td><td bgcolor='#EFF174'>Input</td>
				<td bgcolor='#FFFFFF'>GPIOC<br/>LLWU</td><td bgcolor='#FFFFFF'>port6<br/>wake_up10</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_txd</td><td bgcolor='#90EE67'>Output</td>
				<td bgcolor='#FFFFFF'>PDB0<br/>PDB0<br/>ADC0<br/>ADC0<br/>ADC1<br/>ADC1</td><td bgcolor='#FFFFFF'>PDBtrigger<br/>pdb_trig0<br/>ADCtriggerA<br/>ADCtriggerB<br/>ADCtriggerA<br/>ADCtriggerB</td><td bgcolor='#FFFFFF'>Input</td>
				<td></td><td></td><td></td>
				<td bgcolor='#5FE356'>UART0</td><td bgcolor='#5FE356'>uart_rx</td><td bgcolor='#5FE356'>Input</td>
				<td></td><td></td><td></td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sclk</td><td bgcolor='#AFFF8E'>Input/Output</td>
			</tr>
			<tr>
				<td>40</td><td>CMP0_IN1/PTC7/SPI0_SIN/UART0_TX/I2C0_SDA</td><td><small><i>same</i></small></td>
				<td bgcolor='#EFF174'>CMP0</td><td bgcolor='#EFF174'>cmp_in1<br/>Positive1<br/>Negative1</td><td bgcolor='#EFF174'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOC</td><td bgcolor='#F7DCFF'>port7</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_rxd</td><td bgcolor='#90EE67'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>UART0<br/>SIM</td><td bgcolor='#FFFFFF'>uart_tx<br/>uart_tx0</td><td bgcolor='#FFFFFF'>Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sda</td><td bgcolor='#AFFF8E'>Input/Output</td>
			</tr>
			<tr>
				<td>41</td><td>PTD0/LLWU_P12/SPI0_PCS0/SS_b/UART0_CTS_b/FTM0_CH0/UART1_RX</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>GPIOD<br/>LLWU</td><td bgcolor='#FFFFFF'>port0<br/>wake_up12</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_cs0</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#5FE356'>UART0</td><td bgcolor='#5FE356'>uart_cts</td><td bgcolor='#5FE356'>Input</td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch0<br/>tmr0_ch0</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#5FE356'>UART1</td><td bgcolor='#5FE356'>uart_rx</td><td bgcolor='#5FE356'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>42</td><td>ADC0_SE2/PTD1/SPI0_SCK/UART0_RTS_b/FTM0_CH1/UART1_TX</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_se2</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOD</td><td bgcolor='#F7DCFF'>port1</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_sck</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#5FE356'>UART0</td><td bgcolor='#5FE356'>uart_rts</td><td bgcolor='#5FE356'>Output</td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch1<br/>tmr0_ch1</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#FFFFFF'>UART1<br/>SIM</td><td bgcolor='#FFFFFF'>uart_tx<br/>uart_tx1</td><td bgcolor='#FFFFFF'>Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>43</td><td>PTD2/LLWU_P13/SPI0_SOUT/UART0_RX/FTM0_CH2/I2C0_SCL</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>GPIOD<br/>LLWU</td><td bgcolor='#FFFFFF'>port2<br/>wake_up13</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_txd</td><td bgcolor='#90EE67'>Output</td>
				<td bgcolor='#5FE356'>UART0</td><td bgcolor='#5FE356'>uart_rx</td><td bgcolor='#5FE356'>Input</td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch2<br/>tmr0_ch2</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sclk</td><td bgcolor='#AFFF8E'>Input/Output</td>
			</tr>
			<tr>
				<td>44</td><td>PTD3/SPI0_SIN/UART0_TX/FTM0_CH3/I2C0_SDA</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOD</td><td bgcolor='#F7DCFF'>port3</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_rxd</td><td bgcolor='#90EE67'>Input</td>
				<td bgcolor='#FFFFFF'>UART0<br/>SIM</td><td bgcolor='#FFFFFF'>uart_tx<br/>uart_tx0</td><td bgcolor='#FFFFFF'>Output</td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch3<br/>tmr0_ch3</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sda</td><td bgcolor='#AFFF8E'>Input/Output</td>
			</tr>
			<tr>
				<td>45</td><td>PTD4/LLWU_P14/SPI0_PCS1/UART0_RTS_b/FTM0_CH4/FTM2_CH0/EWM_IN</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>GPIOD<br/>LLWU</td><td bgcolor='#FFFFFF'>port4<br/>wake_up14</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_cs1</td><td bgcolor='#90EE67'>Output</td>
				<td bgcolor='#5FE356'>UART0</td><td bgcolor='#5FE356'>uart_rts</td><td bgcolor='#5FE356'>Output</td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch4<br/>tmr0_ch4</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#FFFFFF'>FTM2<br/>SIM<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch0<br/>tmr2_ch0<br/>tmr_xorFTM2_CH0</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#CEFFFF'>EWM</td><td bgcolor='#CEFFFF'>ewminput<br/>ewm_in</td><td bgcolor='#CEFFFF'>Input</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>46</td><td>ADC0_SE3/PTD5/SPI0_PCS2/UART0_CTS_b/FTM0_CH5/FTM2_CH1/EWM_OUT_b</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_se3</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOD</td><td bgcolor='#F7DCFF'>port5</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_cs2</td><td bgcolor='#90EE67'>Output</td>
				<td bgcolor='#5FE356'>UART0</td><td bgcolor='#5FE356'>uart_cts</td><td bgcolor='#5FE356'>Input</td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch5<br/>tmr0_ch5</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#FFFFFF'>FTM2<br/>SIM<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch1<br/>tmr2_ch1<br/>tmr_xorFTM2_CH1</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#CEFFFF'>EWM</td><td bgcolor='#CEFFFF'>ewmoutput<br/>ewm_out</td><td bgcolor='#CEFFFF'>Output</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>47</td><td>ADC1_SE6/PTD6/LLWU_P15/SPI0_PCS3/UART0_RX/FTM0_CH0/FTM1_CH0/FTM0_FLT0</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC1</td><td bgcolor='#F8FF9A'>adc_sea6</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#FFFFFF'>GPIOD<br/>LLWU</td><td bgcolor='#FFFFFF'>port6<br/>wake_up15</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_cs3</td><td bgcolor='#90EE67'>Output</td>
				<td bgcolor='#5FE356'>UART0</td><td bgcolor='#5FE356'>uart_rx</td><td bgcolor='#5FE356'>Input</td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch0<br/>tmr0_ch0</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#B3EAFF'>FTM1</td><td bgcolor='#B3EAFF'>tmr_ch0</td><td bgcolor='#B3EAFF'>Input, Output</td>
				<td bgcolor='#B3EAFF'>FTM0</td><td bgcolor='#B3EAFF'>tmr_fault0</td><td bgcolor='#B3EAFF'>Input</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>48</td><td>PTD7/UART0_TX/FTM0_CH1/FTM1_CH1/FTM0_FLT1</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOD</td><td bgcolor='#F7DCFF'>port7</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>UART0<br/>SIM</td><td bgcolor='#FFFFFF'>uart_tx<br/>uart_tx0</td><td bgcolor='#FFFFFF'>Output</td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch1<br/>tmr0_ch1</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#FFFFFF'>FTM1<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch1<br/>tmr_xorFTM1_CH1</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#B3EAFF'>FTM0</td><td bgcolor='#B3EAFF'>tmr_fault1</td><td bgcolor='#B3EAFF'>Input</td>
				<td></td><td></td><td></td>
			</tr>
		</table>

*/
/*!
\page page_pinalloc Pin Allocation

		<h2 style='font-family: Arial;'>Pin Allocation Report</h2>
		<table cellpadding='2' border='1' style='border: 2px solid #000000;' bgcolor='WHITE' align='center'>
			<tr bgcolor='#E8E8E8'><th>Peripheral</th><th>Custom peripheral name</th><th>Peripheral description</th></tr>
			<tr bgcolor='#F8FF9A'><td>ADC0</td><td>ADC0</td><td><small>Analog-to-Digital Converter</small></td></tr>
			<tr bgcolor='#F8FF9A'><td>ADC1</td><td>ADC1</td><td><small>Analog-to-Digital Converter</small></td></tr>
			<tr bgcolor='#EFF174'><td>CMP0</td><td>CMP0</td><td><small>High-Speed Comparator (CMP), Voltage Reference (VREF) Digital-to-Analog Converter (DAC), and Analog Mux (ANMUX)</small></td></tr>
			<tr bgcolor='#EFF174'><td>CMP1</td><td>CMP1</td><td><small>High-Speed Comparator (CMP), Voltage Reference (VREF) Digital-to-Analog Converter (DAC), and Analog Mux (ANMUX)</small></td></tr>
			<tr bgcolor='#FFE1C7'><td>CoreDebug</td><td>CoreDebug</td><td><small>ARM Core M0+ debugger</small></td></tr>
			<tr bgcolor='#E5E44D'><td>DAC0</td><td>DAC0</td><td><small>12-Bit Digital-to-Analog Converter</small></td></tr>
			<tr bgcolor='#CEFFFF'><td>EWM</td><td>EWM</td><td><small>External Watchdog Monitor</small></td></tr>
			<tr bgcolor='#B3EAFF'><td>FTM0</td><td>FTM0</td><td><small>FlexTimer Module</small></td></tr>
			<tr bgcolor='#B3EAFF'><td>FTM1</td><td>FTM1</td><td><small>FlexTimer Module</small></td></tr>
			<tr bgcolor='#B3EAFF'><td>FTM2</td><td>FTM2</td><td><small>FlexTimer Module</small></td></tr>
			<tr bgcolor='#F7DCFF'><td>GPIOA</td><td>GPIOA</td><td><small>General Purpose Input/Output</small></td></tr>
			<tr bgcolor='#F7DCFF'><td>GPIOB</td><td>GPIOB</td><td><small>General Purpose Input/Output</small></td></tr>
			<tr bgcolor='#F7DCFF'><td>GPIOC</td><td>GPIOC</td><td><small>General Purpose Input/Output</small></td></tr>
			<tr bgcolor='#F7DCFF'><td>GPIOD</td><td>GPIOD</td><td><small>General Purpose Input/Output</small></td></tr>
			<tr bgcolor='#F7DCFF'><td>GPIOE</td><td>GPIOE</td><td><small>General Purpose Input/Output</small></td></tr>
			<tr bgcolor='#AFFF8E'><td>I2C0</td><td>I2C0</td><td><small>Inter-integrated circuit bus</small></td></tr>
			<tr bgcolor='#DDC7B5'><td>LLWU</td><td>LLWU</td><td><small>Low Leakage Wake-up Unit</small></td></tr>
			<tr bgcolor='#86DAFF'><td>LPTMR0</td><td>LPTMR0</td><td><small>Low Power Timer Module</small></td></tr>
			<tr bgcolor='#CCB6A0'><td>OSC0</td><td>OSC0</td><td><small>Oscillator</small></td></tr>
			<tr bgcolor='#58C7FF'><td>PDB0</td><td>PDB0</td><td><small>Programmable Delay Block</small></td></tr>
			<tr bgcolor='#C7A886'><td>PMC</td><td>PMC</td><td><small>Power Management Controller</small></td></tr>
			<tr bgcolor='#FFE1C7'><td>RCM</td><td>RCM</td><td><small>Reset Control Module</small></td></tr>
			<tr bgcolor='#DDC7B5'><td>SIM</td><td>SIM</td><td><small>System Integration Module</small></td></tr>
			<tr bgcolor='#90EE67'><td>SPI0</td><td>SPI0</td><td><small>Deserial Serial Peripheral Interface 0</small></td></tr>
			<tr bgcolor='#EBD4BD'><td>SystemControl</td><td>SystemControl</td><td><small>System control</small></td></tr>
			<tr bgcolor='#5FE356'><td>UART0</td><td>UART0</td><td><small>Serial Communications Interface Module UART0</small></td></tr>
			<tr bgcolor='#5FE356'><td>UART1</td><td>UART1</td><td><small>Serial Communications Interface Module UART1</small></td></tr>
		</table>
		<br/>
		<br/>

		<h2 style='font-family: Arial;'>Routed Pins</h2>
		<table cellpadding='2' border='1' style='border: 2px solid #000000;' bgcolor='WHITE' width='100%' align='center'>
			<tr><td colspan='3'></td><th colspan='4' align='center' bgcolor='#D0D0D0'>Assigned Pin Function(s)</th></tr>
			<tr>
				<th bgcolor='#E8E8E8'>Package Pin #</th><th bgcolor='#E8E8E8'>Pin Name</th><th bgcolor='#E8E8E8'>User Assigned Signal Name</th><th bgcolor='#E8E8E8'>Assigned Peripheral</th><th bgcolor='#E8E8E8'>Assigned Function</th><th bgcolor='#E8E8E8'>Package Function</th><th bgcolor='#E8E8E8'>Dir</th>
			</tr>
			<tr>
				<td>1</td><td>VDD1</td><td><small><i>same</i></small></td>
				<td bgcolor='#C7A886'>PMC</td><td bgcolor='#C7A886'>vdd1</td><td bgcolor='#C7A886'>alt0</td><td bgcolor='#C7A886'>Input</td>
			</tr>
			<tr>
				<td>2</td><td>VSS2</td><td><small><i>same</i></small></td>
				<td bgcolor='#C7A886'>PMC</td><td bgcolor='#C7A886'>vss2</td><td bgcolor='#C7A886'>alt0</td><td bgcolor='#C7A886'>Input</td>
			</tr>
			<tr>
				<td rowspan='3'>3</td><td rowspan='3'>ADC0_SE1/ADC0_DP1/ADC1_SE0/PTE16/SPI0_PCS0/SS_b/UART1_TX/FTM_CLKIN0/FTM0_FLT3</td><td rowspan='3'><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_se1</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#F8FF9A'><td>ADC0</td><td>adc_dp1</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#F8FF9A'><td>ADC1</td><td>adc_se0</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td rowspan='3'>4</td><td rowspan='3'>ADC0_SE5/ADC0_DM1/ADC1_SE5/PTE17/SPI0_SCK/UART1_RX/FTM_CLKIN1/LPTMR0_ALT3</td><td rowspan='3'><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_sea5</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#F8FF9A'><td>ADC0</td><td>adc_dm1</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#F8FF9A'><td>ADC1</td><td>adc_sea5</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td rowspan='3'>5</td><td rowspan='3'>ADC0_SE6/ADC1_SE1/ADC1_DP1/PTE18/SPI0_SOUT/UART1_CTS_b/I2C0_SDA/SPI0_SIN</td><td rowspan='3'><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_sea6</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#F8FF9A'><td>ADC1</td><td>adc_se1</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#F8FF9A'><td>ADC1</td><td>adc_dp1</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td rowspan='3'>6</td><td rowspan='3'>ADC0_SE7/ADC1_SE7/ADC1_DM1/PTE19/SPI0_SIN/UART1_RTS_b/I2C0_SCL/SPI0_SOUT</td><td rowspan='3'><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_sea7</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#F8FF9A'><td>ADC1</td><td>adc_sea7</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#F8FF9A'><td>ADC1</td><td>adc_dm1</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td rowspan='2'>7</td><td rowspan='2'>ADC0_SE0/ADC0_DP0/PTE20/FTM1_CH0/UART0_TX</td><td rowspan='2'><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_se0</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#F8FF9A'><td>ADC0</td><td>adc_dp0</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td rowspan='2'>8</td><td rowspan='2'>ADC0_SE4/ADC0_DM0/PTE21/FTM1_CH1/UART0_RX</td><td rowspan='2'><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_sea4</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#F8FF9A'><td>ADC0</td><td>adc_dm0</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td>9</td><td>VDDA</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td rowspan='6'>10</td><td rowspan='6'>VREFH</td><td rowspan='6'><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_vrefh</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#F8FF9A'><td>ADC0</td><td>adc_se29</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#F8FF9A'><td>ADC0</td><td>adc_dp29</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#F8FF9A'><td>ADC1</td><td>adc_vrefh</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#F8FF9A'><td>ADC1</td><td>adc_se29</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#F8FF9A'><td>ADC1</td><td>adc_dp29</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td rowspan='6'>11</td><td rowspan='6'>VREFL</td><td rowspan='6'><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_vrefl</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#F8FF9A'><td>ADC0</td><td>adc_se30</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#F8FF9A'><td>ADC0</td><td>adc_dm29</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#F8FF9A'><td>ADC1</td><td>adc_vrefl</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#F8FF9A'><td>ADC1</td><td>adc_se30</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#F8FF9A'><td>ADC1</td><td>adc_dm29</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td>12</td><td>VSSA</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>13</td><td>CMP1_IN5/CMP0_IN5/PTE29/FTM0_CH2/FTM_CLKIN0</td><td><small><i>same</i></small></td>
				<td bgcolor='#B3EAFF'>FTM0</td><td bgcolor='#B3EAFF'>tmr_ch2</td><td bgcolor='#B3EAFF'>alt3</td><td bgcolor='#B3EAFF'>Output</td>
			</tr>
			<tr>
				<td rowspan='9'>14</td><td rowspan='9'>ADC1_SE4/CMP0_IN4/CMP1_IN4/DAC0_OUT/PTE30/FTM0_CH3/FTM_CLKIN1</td><td rowspan='9'><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC1</td><td bgcolor='#F8FF9A'>adc_sea4</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#EFF174'><td>CMP0</td><td>cmp_in4</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#EFF174'><td>CMP0</td><td>Positive4</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#EFF174'><td>CMP0</td><td>Negative4</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#EFF174'><td>CMP1</td><td>cmp_in4</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#EFF174'><td>CMP1</td><td>Positive4</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#EFF174'><td>CMP1</td><td>Negative4</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#E5E44D'><td>DAC0</td><td>dacout</td><td>alt0</td><td>Output</td></tr>
			<tr bgcolor='#E5E44D'><td>DAC0</td><td>dac_out</td><td>alt0</td><td>Output</td></tr>
			<tr>
				<td>15</td><td>PTE24/FTM0_CH0/I2C0_SCL/EWM_OUT_b</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>16</td><td>PTE25/FTM0_CH1/I2C0_SDA/EWM_IN</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>17</td><td>PTA0/UART0_CTS_b/FTM0_CH5/SWD_CLK</td><td><small><i>same</i></small></td>
				<td bgcolor='#FFE1C7'>CoreDebug</td><td bgcolor='#FFE1C7'>swd_clk</td><td bgcolor='#FFE1C7'>alt7</td><td bgcolor='#FFE1C7'>Input/Output</td>
			</tr>
			<tr>
				<td>18</td><td>PTA1/UART0_RX/FTM2_CH0/CMP0_OUT/FTM2_QD_PHA/FTM1_CH1</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>19</td><td>PTA2/UART0_TX/FTM2_CH1/CMP1_OUT/FTM2_QD_PHB/FTM1_CH0</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>20</td><td>PTA3/UART0_RTS_b/FTM0_CH0/FTM2_FLT0/EWM_OUT_b/SWD_DIO</td><td><small><i>same</i></small></td>
				<td bgcolor='#FFE1C7'>CoreDebug</td><td bgcolor='#FFE1C7'>swd_dio</td><td bgcolor='#FFE1C7'>alt7</td><td bgcolor='#FFE1C7'>Input/Output</td>
			</tr>
			<tr>
				<td rowspan='2'>21</td><td rowspan='2'>PTA4/LLWU_P3/FTM0_CH1/FTM0_FLT3/NMI_b</td><td rowspan='2'><small><i>same</i></small></td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port4</td><td bgcolor='#F7DCFF'>alt1</td><td bgcolor='#F7DCFF'>Output</td>
			</tr>
			<tr bgcolor='#DDC7B5'><td>LLWU</td><td>wake_up3</td><td>alt1</td><td>Input</td></tr>
			<tr>
				<td>22</td><td>VDD22</td><td><small><i>same</i></small></td>
				<td bgcolor='#C7A886'>PMC</td><td bgcolor='#C7A886'>vdd22</td><td bgcolor='#C7A886'>alt0</td><td bgcolor='#C7A886'>Input</td>
			</tr>
			<tr>
				<td>23</td><td>VSS23</td><td><small><i>same</i></small></td>
				<td bgcolor='#C7A886'>PMC</td><td bgcolor='#C7A886'>vss23</td><td bgcolor='#C7A886'>alt0</td><td bgcolor='#C7A886'>Input</td>
			</tr>
			<tr>
				<td>24</td><td>EXTAL0/PTA18/FTM0_FLT2/FTM_CLKIN0</td><td><small><i>same</i></small></td>
				<td bgcolor='#CCB6A0'>OSC0</td><td bgcolor='#CCB6A0'>extal</td><td bgcolor='#CCB6A0'>alt0</td><td bgcolor='#CCB6A0'>Input</td>
			</tr>
			<tr>
				<td>25</td><td>XTAL0/PTA19/FTM0_FLT0/FTM1_FLT0/FTM_CLKIN1/LPTMR0_ALT1</td><td><small><i>same</i></small></td>
				<td bgcolor='#CCB6A0'>OSC0</td><td bgcolor='#CCB6A0'>xtal</td><td bgcolor='#CCB6A0'>alt0</td><td bgcolor='#CCB6A0'>Output</td>
			</tr>
			<tr>
				<td rowspan='2'>26</td><td rowspan='2'>PTA20/RESET_b</td><td rowspan='2'><small><i>same</i></small></td>
				<td bgcolor='#FFE1C7'>RCM</td><td bgcolor='#FFE1C7'>reset</td><td bgcolor='#FFE1C7'>alt7</td><td bgcolor='#FFE1C7'>Input</td>
			</tr>
			<tr bgcolor='#969696'><td>non-peripheral</td><td>RESET</td><td>alt7</td><td>Not Specified</td></tr>
			<tr>
				<td rowspan='2'>27</td><td rowspan='2'>ADC0_SE8/ADC1_SE8/PTB0/LLWU_P5/I2C0_SCL/FTM1_CH0/FTM1_QD_PHA/UART0_RX</td><td rowspan='2'><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_se8</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#F8FF9A'><td>ADC1</td><td>adc_se8</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td rowspan='2'>28</td><td rowspan='2'>ADC0_SE9/ADC1_SE9/PTB1/I2C0_SDA/FTM1_CH1/FTM0_FLT2/EWM_IN/FTM1_QD_PHB/UART0_TX</td><td rowspan='2'><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_se9</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#F8FF9A'><td>ADC1</td><td>adc_se9</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td rowspan='3'>29</td><td rowspan='3'>ADC0_SE10/ADC1_SE10/ADC1_DM2/PTB2/I2C0_SCL/UART0_RTS_b/FTM0_FLT1/FTM0_FLT3</td><td rowspan='3'><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_se10</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#F8FF9A'><td>ADC1</td><td>adc_se10</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#F8FF9A'><td>ADC1</td><td>adc_dm2</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td rowspan='2'>30</td><td rowspan='2'>ADC1_SE2/ADC1_DP2/PTB3/I2C0_SDA/UART0_CTS_b/FTM0_FLT0</td><td rowspan='2'><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC1</td><td bgcolor='#F8FF9A'>adc_se2</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#F8FF9A'><td>ADC1</td><td>adc_dp2</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td>31</td><td>PTB16/UART0_RX/FTM_CLKIN2/EWM_IN</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>32</td><td>PTB17/UART0_TX/FTM_CLKIN1/EWM_OUT_b</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>33</td><td>ADC1_SE11/PTC0/SPI0_PCS4/PDB0_EXTRG/CMP0_OUT/FTM0_FLT0/SPI0_PCS0/SS_b</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC1</td><td bgcolor='#F8FF9A'>adc_se11</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr>
				<td>34</td><td>ADC1_SE3/PTC1/LLWU_P6/SPI0_PCS3/UART1_RTS_b/FTM0_CH0/FTM2_CH0</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC1</td><td bgcolor='#F8FF9A'>adc_se3</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr>
				<td rowspan='4'>35</td><td rowspan='4'>ADC0_SE11/CMP1_IN0/PTC2/SPI0_PCS2/UART1_CTS_b/FTM0_CH1/FTM2_CH1</td><td rowspan='4'><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_se11</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr bgcolor='#EFF174'><td>CMP1</td><td>cmp_in0</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#EFF174'><td>CMP1</td><td>Positive0</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#EFF174'><td>CMP1</td><td>Negative0</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td rowspan='3'>36</td><td rowspan='3'>CMP1_IN1/PTC3/LLWU_P7/SPI0_PCS1/UART1_RX/FTM0_CH2/CLKOUT</td><td rowspan='3'><small><i>same</i></small></td>
				<td bgcolor='#EFF174'>CMP1</td><td bgcolor='#EFF174'>cmp_in1</td><td bgcolor='#EFF174'>alt0</td><td bgcolor='#EFF174'>Input</td>
			</tr>
			<tr bgcolor='#EFF174'><td>CMP1</td><td>Positive1</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#EFF174'><td>CMP1</td><td>Negative1</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td>37</td><td>PTC4/LLWU_P8/SPI0_PCS0/SS_b/UART1_TX/FTM0_CH3/CMP1_OUT</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>38</td><td>PTC5/LLWU_P9/SPI0_SCK/LPTMR0_ALT2/CMP0_OUT/FTM0_CH2</td><td><small><i>same</i></small></td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_sck</td><td bgcolor='#90EE67'>alt2</td><td bgcolor='#90EE67'>Output</td>
			</tr>
			<tr>
				<td>39</td><td>CMP0_IN0/PTC6/LLWU_P10/SPI0_SOUT/PDB0_EXTRG/UART0_RX/I2C0_SCL</td><td><small><i>same</i></small></td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_txd</td><td bgcolor='#90EE67'>alt2</td><td bgcolor='#90EE67'>Output</td>
			</tr>
			<tr>
				<td rowspan='3'>40</td><td rowspan='3'>CMP0_IN1/PTC7/SPI0_SIN/UART0_TX/I2C0_SDA</td><td rowspan='3'><small><i>same</i></small></td>
				<td bgcolor='#EFF174'>CMP0</td><td bgcolor='#EFF174'>cmp_in1</td><td bgcolor='#EFF174'>alt0</td><td bgcolor='#EFF174'>Input</td>
			</tr>
			<tr bgcolor='#EFF174'><td>CMP0</td><td>Positive1</td><td>alt0</td><td>Input</td></tr>
			<tr bgcolor='#EFF174'><td>CMP0</td><td>Negative1</td><td>alt0</td><td>Input</td></tr>
			<tr>
				<td>41</td><td>PTD0/LLWU_P12/SPI0_PCS0/SS_b/UART0_CTS_b/FTM0_CH0/UART1_RX</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>42</td><td>ADC0_SE2/PTD1/SPI0_SCK/UART0_RTS_b/FTM0_CH1/UART1_TX</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_se2</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr>
				<td>43</td><td>PTD2/LLWU_P13/SPI0_SOUT/UART0_RX/FTM0_CH2/I2C0_SCL</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>44</td><td>PTD3/SPI0_SIN/UART0_TX/FTM0_CH3/I2C0_SDA</td><td><small><i>same</i></small></td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_rxd</td><td bgcolor='#90EE67'>alt2</td><td bgcolor='#90EE67'>Input</td>
			</tr>
			<tr>
				<td>45</td><td>PTD4/LLWU_P14/SPI0_PCS1/UART0_RTS_b/FTM0_CH4/FTM2_CH0/EWM_IN</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td><td></td>
			</tr>
			<tr>
				<td>46</td><td>ADC0_SE3/PTD5/SPI0_PCS2/UART0_CTS_b/FTM0_CH5/FTM2_CH1/EWM_OUT_b</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_se3</td><td bgcolor='#F8FF9A'>alt0</td><td bgcolor='#F8FF9A'>Input</td>
			</tr>
			<tr>
				<td rowspan='2'>47</td><td rowspan='2'>ADC1_SE6/PTD6/LLWU_P15/SPI0_PCS3/UART0_RX/FTM0_CH0/FTM1_CH0/FTM0_FLT0</td><td rowspan='2'><small><i>same</i></small></td>
				<td bgcolor='#F7DCFF'>GPIOD</td><td bgcolor='#F7DCFF'>port6</td><td bgcolor='#F7DCFF'>alt1</td><td bgcolor='#F7DCFF'>Output</td>
			</tr>
			<tr bgcolor='#DDC7B5'><td>LLWU</td><td>wake_up15</td><td>alt1</td><td>Input</td></tr>
			<tr>
				<td>48</td><td>PTD7/UART0_TX/FTM0_CH1/FTM1_CH1/FTM0_FLT1</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td><td></td>
			</tr>
		</table>

		<h2 style='font-family: Arial;'>Routable Pins</h2>
		<table cellpadding='2' border='1' style='border: 2px solid #000000;' bgcolor='WHITE' width='100%' align='center'>
			<tr><td colspan='3'></td><th colspan='3' align='center' bgcolor='#D0D0D0'>alt0</th><th colspan='3' align='center' bgcolor='#D0D0D0'>alt1</th><th colspan='3' align='center' bgcolor='#D0D0D0'>alt2</th><th colspan='3' align='center' bgcolor='#D0D0D0'>alt3</th><th colspan='3' align='center' bgcolor='#D0D0D0'>alt4</th><th colspan='3' align='center' bgcolor='#D0D0D0'>alt5</th><th colspan='3' align='center' bgcolor='#D0D0D0'>alt6</th><th colspan='3' align='center' bgcolor='#D0D0D0'>alt7</th></tr>
			<tr>
				<th bgcolor='#E8E8E8'>Package Pin #</th><th bgcolor='#E8E8E8'>Pin Name</th><th bgcolor='#E8E8E8'>User Assigned Signal Name</th>
				<th bgcolor='#E8E8E8'>Peripheral</th><th bgcolor='#E8E8E8'>Function</th><th bgcolor='#E8E8E8'>Dir</th>
				<th bgcolor='#E8E8E8'>Peripheral</th><th bgcolor='#E8E8E8'>Function</th><th bgcolor='#E8E8E8'>Dir</th>
				<th bgcolor='#E8E8E8'>Peripheral</th><th bgcolor='#E8E8E8'>Function</th><th bgcolor='#E8E8E8'>Dir</th>
				<th bgcolor='#E8E8E8'>Peripheral</th><th bgcolor='#E8E8E8'>Function</th><th bgcolor='#E8E8E8'>Dir</th>
				<th bgcolor='#E8E8E8'>Peripheral</th><th bgcolor='#E8E8E8'>Function</th><th bgcolor='#E8E8E8'>Dir</th>
				<th bgcolor='#E8E8E8'>Peripheral</th><th bgcolor='#E8E8E8'>Function</th><th bgcolor='#E8E8E8'>Dir</th>
				<th bgcolor='#E8E8E8'>Peripheral</th><th bgcolor='#E8E8E8'>Function</th><th bgcolor='#E8E8E8'>Dir</th>
				<th bgcolor='#E8E8E8'>Peripheral</th><th bgcolor='#E8E8E8'>Function</th><th bgcolor='#E8E8E8'>Dir</th>
			</tr>
			<tr>
				<td>1</td><td>VDD1</td><td><small><i>same</i></small></td>
				<td bgcolor='#C7A886'>PMC</td><td bgcolor='#C7A886'>vdd1</td><td bgcolor='#C7A886'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>2</td><td>VSS2</td><td><small><i>same</i></small></td>
				<td bgcolor='#C7A886'>PMC</td><td bgcolor='#C7A886'>vss2</td><td bgcolor='#C7A886'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>3</td><td>ADC0_SE1/ADC0_DP1/ADC1_SE0/PTE16/SPI0_PCS0/SS_b/UART1_TX/FTM_CLKIN0/FTM0_FLT3</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0<br/>ADC0<br/>ADC1</td><td bgcolor='#F8FF9A'>adc_se1<br/>adc_dp1<br/>adc_se0</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port16</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_cs0</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#FFFFFF'>UART1<br/>SIM</td><td bgcolor='#FFFFFF'>uart_tx<br/>uart_tx1</td><td bgcolor='#FFFFFF'>Output</td>
				<td bgcolor='#B3EAFF'>FTM0<br/>FTM1<br/>FTM2</td><td bgcolor='#B3EAFF'>tmr_clk</td><td bgcolor='#B3EAFF'>Input</td>
				<td></td><td></td><td></td>
				<td bgcolor='#B3EAFF'>FTM0</td><td bgcolor='#B3EAFF'>tmr_fault3</td><td bgcolor='#B3EAFF'>Input</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>4</td><td>ADC0_SE5/ADC0_DM1/ADC1_SE5/PTE17/SPI0_SCK/UART1_RX/FTM_CLKIN1/LPTMR0_ALT3</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0<br/>ADC0<br/>ADC1</td><td bgcolor='#F8FF9A'>adc_sea5<br/>adc_dm1<br/>adc_sea5</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port17</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_sck</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#5FE356'>UART1</td><td bgcolor='#5FE356'>uart_rx</td><td bgcolor='#5FE356'>Input</td>
				<td bgcolor='#B3EAFF'>FTM0<br/>FTM1<br/>FTM2</td><td bgcolor='#B3EAFF'>tmr_clk</td><td bgcolor='#B3EAFF'>Input</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>LPTMR0</td><td bgcolor='#86DAFF'>tmr_clk3</td><td bgcolor='#86DAFF'>Input</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>5</td><td>ADC0_SE6/ADC1_SE1/ADC1_DP1/PTE18/SPI0_SOUT/UART1_CTS_b/I2C0_SDA/SPI0_SIN</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0<br/>ADC1<br/>ADC1</td><td bgcolor='#F8FF9A'>adc_sea6<br/>adc_se1<br/>adc_dp1</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port18</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_txd</td><td bgcolor='#90EE67'>Output</td>
				<td bgcolor='#5FE356'>UART1</td><td bgcolor='#5FE356'>uart_cts</td><td bgcolor='#5FE356'>Input</td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sda</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_rxd</td><td bgcolor='#90EE67'>Input</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>6</td><td>ADC0_SE7/ADC1_SE7/ADC1_DM1/PTE19/SPI0_SIN/UART1_RTS_b/I2C0_SCL/SPI0_SOUT</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0<br/>ADC1<br/>ADC1</td><td bgcolor='#F8FF9A'>adc_sea7<br/>adc_sea7<br/>adc_dm1</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port19</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_rxd</td><td bgcolor='#90EE67'>Input</td>
				<td bgcolor='#5FE356'>UART1</td><td bgcolor='#5FE356'>uart_rts</td><td bgcolor='#5FE356'>Output</td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sclk</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_txd</td><td bgcolor='#90EE67'>Output</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>7</td><td>ADC0_SE0/ADC0_DP0/PTE20/FTM1_CH0/UART0_TX</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_se0<br/>adc_dp0</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port20</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#B3EAFF'>FTM1</td><td bgcolor='#B3EAFF'>tmr_ch0</td><td bgcolor='#B3EAFF'>Input, Output</td>
				<td bgcolor='#FFFFFF'>UART0<br/>SIM</td><td bgcolor='#FFFFFF'>uart_tx<br/>uart_tx0</td><td bgcolor='#FFFFFF'>Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>8</td><td>ADC0_SE4/ADC0_DM0/PTE21/FTM1_CH1/UART0_RX</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_sea4<br/>adc_dm0</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port21</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>FTM1<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch1<br/>tmr_xorFTM1_CH1</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#5FE356'>UART0</td><td bgcolor='#5FE356'>uart_rx</td><td bgcolor='#5FE356'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>9</td><td>VDDA</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0<br/>ADC0<br/>ADC0<br/>ADC0<br/>ADC1<br/>ADC1<br/>ADC1</td><td bgcolor='#F8FF9A'>adc_vdda_se29_dp29<br/>adc_vrefh<br/>adc_se29<br/>adc_dp29<br/>adc_vrefh<br/>adc_se29<br/>adc_dp29</td><td bgcolor='#F8FF9A'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>10</td><td>VREFH</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0<br/>ADC0<br/>ADC0<br/>ADC0<br/>ADC1<br/>ADC1<br/>ADC1</td><td bgcolor='#F8FF9A'>adc_vrefh_se29_dp29<br/>adc_vrefh<br/>adc_se29<br/>adc_dp29<br/>adc_vrefh<br/>adc_se29<br/>adc_dp29</td><td bgcolor='#F8FF9A'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>11</td><td>VREFL</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0<br/>ADC0<br/>ADC0<br/>ADC0<br/>ADC1<br/>ADC1<br/>ADC1</td><td bgcolor='#F8FF9A'>adc_vrefl_se30_dm29<br/>adc_vrefl<br/>adc_se30<br/>adc_dm29<br/>adc_vrefl<br/>adc_se30<br/>adc_dm29</td><td bgcolor='#F8FF9A'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>12</td><td>VSSA</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0<br/>ADC0<br/>ADC0<br/>ADC0<br/>ADC1<br/>ADC1<br/>ADC1</td><td bgcolor='#F8FF9A'>adc_vssa_se30_dm29<br/>adc_vrefl<br/>adc_se30<br/>adc_dm29<br/>adc_vrefl<br/>adc_se30<br/>adc_dm29</td><td bgcolor='#F8FF9A'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>13</td><td>CMP1_IN5/CMP0_IN5/PTE29/FTM0_CH2/FTM_CLKIN0</td><td><small><i>same</i></small></td>
				<td bgcolor='#EFF174'>CMP1<br/>CMP1<br/>CMP1<br/>CMP0<br/>CMP0<br/>CMP0</td><td bgcolor='#EFF174'>cmp_in5<br/>Positive5<br/>Negative5<br/>cmp_in5<br/>Positive5<br/>Negative5</td><td bgcolor='#EFF174'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port29</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch2<br/>tmr0_ch2</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#B3EAFF'>FTM0<br/>FTM1<br/>FTM2</td><td bgcolor='#B3EAFF'>tmr_clk</td><td bgcolor='#B3EAFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>14</td><td>ADC1_SE4/CMP0_IN4/CMP1_IN4/DAC0_OUT/PTE30/FTM0_CH3/FTM_CLKIN1</td><td><small><i>same</i></small></td>
				<td bgcolor='#FFFFFF'>ADC1<br/>CMP0<br/>CMP0<br/>CMP0<br/>CMP1<br/>CMP1<br/>CMP1<br/>DAC0<br/>DAC0</td><td bgcolor='#FFFFFF'>adc_sea4<br/>cmp_in4<br/>Positive4<br/>Negative4<br/>cmp_in4<br/>Positive4<br/>Negative4<br/>dacout<br/>dac_out</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port30</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch3<br/>tmr0_ch3</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#B3EAFF'>FTM0<br/>FTM1<br/>FTM2</td><td bgcolor='#B3EAFF'>tmr_clk</td><td bgcolor='#B3EAFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>15</td><td>PTE24/FTM0_CH0/I2C0_SCL/EWM_OUT_b</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port24</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch0<br/>tmr0_ch0</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sclk</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td bgcolor='#CEFFFF'>EWM</td><td bgcolor='#CEFFFF'>ewmoutput<br/>ewm_out</td><td bgcolor='#CEFFFF'>Output</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>16</td><td>PTE25/FTM0_CH1/I2C0_SDA/EWM_IN</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOE</td><td bgcolor='#F7DCFF'>port25</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch1<br/>tmr0_ch1</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sda</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td bgcolor='#CEFFFF'>EWM</td><td bgcolor='#CEFFFF'>ewminput<br/>ewm_in</td><td bgcolor='#CEFFFF'>Input</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>17</td><td>PTA0/UART0_CTS_b/FTM0_CH5/SWD_CLK</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port0</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#5FE356'>UART0</td><td bgcolor='#5FE356'>uart_cts</td><td bgcolor='#5FE356'>Input</td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch5<br/>tmr0_ch5</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFE1C7'>CoreDebug</td><td bgcolor='#FFE1C7'>swd_clk</td><td bgcolor='#FFE1C7'>Input/Output</td>
			</tr>
			<tr>
				<td>18</td><td>PTA1/UART0_RX/FTM2_CH0/CMP0_OUT/FTM2_QD_PHA/FTM1_CH1</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port1</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#5FE356'>UART0</td><td bgcolor='#5FE356'>uart_rx</td><td bgcolor='#5FE356'>Input</td>
				<td bgcolor='#FFFFFF'>FTM2<br/>SIM<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch0<br/>tmr2_ch0<br/>tmr_xorFTM2_CH0</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#EFF174'>CMP0</td><td bgcolor='#EFF174'>Output</td><td bgcolor='#EFF174'>Output</td>
				<td bgcolor='#B3EAFF'>FTM2</td><td bgcolor='#B3EAFF'>tmr_qd_phA</td><td bgcolor='#B3EAFF'>Input</td>
				<td bgcolor='#FFFFFF'>FTM1<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch1<br/>tmr_xorFTM1_CH1</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>19</td><td>PTA2/UART0_TX/FTM2_CH1/CMP1_OUT/FTM2_QD_PHB/FTM1_CH0</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port2</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#FFFFFF'>UART0<br/>SIM</td><td bgcolor='#FFFFFF'>uart_tx<br/>uart_tx0</td><td bgcolor='#FFFFFF'>Output</td>
				<td bgcolor='#FFFFFF'>FTM2<br/>SIM<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch1<br/>tmr2_ch1<br/>tmr_xorFTM2_CH1</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#EFF174'>CMP1</td><td bgcolor='#EFF174'>Output</td><td bgcolor='#EFF174'>Output</td>
				<td bgcolor='#B3EAFF'>FTM2</td><td bgcolor='#B3EAFF'>tmr_qd_phB</td><td bgcolor='#B3EAFF'>Input</td>
				<td bgcolor='#B3EAFF'>FTM1</td><td bgcolor='#B3EAFF'>tmr_ch0</td><td bgcolor='#B3EAFF'>Input, Output</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>20</td><td>PTA3/UART0_RTS_b/FTM0_CH0/FTM2_FLT0/EWM_OUT_b/SWD_DIO</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port3</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#5FE356'>UART0</td><td bgcolor='#5FE356'>uart_rts</td><td bgcolor='#5FE356'>Output</td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch0<br/>tmr0_ch0</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#B3EAFF'>FTM2</td><td bgcolor='#B3EAFF'>tmr_fault0</td><td bgcolor='#B3EAFF'>Input</td>
				<td bgcolor='#CEFFFF'>EWM</td><td bgcolor='#CEFFFF'>ewmoutput<br/>ewm_out</td><td bgcolor='#CEFFFF'>Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFE1C7'>CoreDebug</td><td bgcolor='#FFE1C7'>swd_dio</td><td bgcolor='#FFE1C7'>Input/Output</td>
			</tr>
			<tr>
				<td>21</td><td>PTA4/LLWU_P3/FTM0_CH1/FTM0_FLT3/NMI_b</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>GPIOA<br/>LLWU</td><td bgcolor='#FFFFFF'>port4<br/>wake_up3</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch1<br/>tmr0_ch1</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#B3EAFF'>FTM0</td><td bgcolor='#B3EAFF'>tmr_fault3</td><td bgcolor='#B3EAFF'>Input</td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>SystemControl<br/>non-peripheral</td><td bgcolor='#FFFFFF'>scb_nmi<br/>NMI</td><td bgcolor='#FFFFFF'>Input</td>
			</tr>
			<tr>
				<td>22</td><td>VDD22</td><td><small><i>same</i></small></td>
				<td bgcolor='#C7A886'>PMC</td><td bgcolor='#C7A886'>vdd22</td><td bgcolor='#C7A886'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>23</td><td>VSS23</td><td><small><i>same</i></small></td>
				<td bgcolor='#C7A886'>PMC</td><td bgcolor='#C7A886'>vss23</td><td bgcolor='#C7A886'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>24</td><td>EXTAL0/PTA18/FTM0_FLT2/FTM_CLKIN0</td><td><small><i>same</i></small></td>
				<td bgcolor='#CCB6A0'>OSC0</td><td bgcolor='#CCB6A0'>extal</td><td bgcolor='#CCB6A0'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port18</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#B3EAFF'>FTM0</td><td bgcolor='#B3EAFF'>tmr_fault2</td><td bgcolor='#B3EAFF'>Input</td>
				<td bgcolor='#B3EAFF'>FTM0<br/>FTM1<br/>FTM2</td><td bgcolor='#B3EAFF'>tmr_clk</td><td bgcolor='#B3EAFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>25</td><td>XTAL0/PTA19/FTM0_FLT0/FTM1_FLT0/FTM_CLKIN1/LPTMR0_ALT1</td><td><small><i>same</i></small></td>
				<td bgcolor='#CCB6A0'>OSC0</td><td bgcolor='#CCB6A0'>xtal</td><td bgcolor='#CCB6A0'>Output</td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port19</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#B3EAFF'>FTM0</td><td bgcolor='#B3EAFF'>tmr_fault0</td><td bgcolor='#B3EAFF'>Input</td>
				<td bgcolor='#B3EAFF'>FTM1</td><td bgcolor='#B3EAFF'>tmr_fault0</td><td bgcolor='#B3EAFF'>Input</td>
				<td bgcolor='#B3EAFF'>FTM0<br/>FTM1<br/>FTM2</td><td bgcolor='#B3EAFF'>tmr_clk</td><td bgcolor='#B3EAFF'>Input</td>
				<td></td><td></td><td></td>
				<td bgcolor='#86DAFF'>LPTMR0</td><td bgcolor='#86DAFF'>tmr_clk1</td><td bgcolor='#86DAFF'>Input</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>26</td><td>PTA20/RESET_b</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOA</td><td bgcolor='#F7DCFF'>port20</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>RCM<br/>non-peripheral</td><td bgcolor='#FFFFFF'>reset<br/>RESET</td><td bgcolor='#FFFFFF'>Input</td>
			</tr>
			<tr>
				<td>27</td><td>ADC0_SE8/ADC1_SE8/PTB0/LLWU_P5/I2C0_SCL/FTM1_CH0/FTM1_QD_PHA/UART0_RX</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0<br/>ADC1</td><td bgcolor='#F8FF9A'>adc_se8</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#FFFFFF'>GPIOB<br/>LLWU</td><td bgcolor='#FFFFFF'>port0<br/>wake_up5</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sclk</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td bgcolor='#B3EAFF'>FTM1</td><td bgcolor='#B3EAFF'>tmr_ch0</td><td bgcolor='#B3EAFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#B3EAFF'>FTM1</td><td bgcolor='#B3EAFF'>tmr_qd_phA</td><td bgcolor='#B3EAFF'>Input</td>
				<td bgcolor='#5FE356'>UART0</td><td bgcolor='#5FE356'>uart_rx</td><td bgcolor='#5FE356'>Input</td>
			</tr>
			<tr>
				<td>28</td><td>ADC0_SE9/ADC1_SE9/PTB1/I2C0_SDA/FTM1_CH1/FTM0_FLT2/EWM_IN/FTM1_QD_PHB/UART0_TX</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0<br/>ADC1</td><td bgcolor='#F8FF9A'>adc_se9</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOB</td><td bgcolor='#F7DCFF'>port1</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sda</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td bgcolor='#FFFFFF'>FTM1<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch1<br/>tmr_xorFTM1_CH1</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#B3EAFF'>FTM0</td><td bgcolor='#B3EAFF'>tmr_fault2</td><td bgcolor='#B3EAFF'>Input</td>
				<td bgcolor='#CEFFFF'>EWM</td><td bgcolor='#CEFFFF'>ewminput<br/>ewm_in</td><td bgcolor='#CEFFFF'>Input</td>
				<td bgcolor='#B3EAFF'>FTM1</td><td bgcolor='#B3EAFF'>tmr_qd_phB</td><td bgcolor='#B3EAFF'>Input</td>
				<td bgcolor='#FFFFFF'>UART0<br/>SIM</td><td bgcolor='#FFFFFF'>uart_tx<br/>uart_tx0</td><td bgcolor='#FFFFFF'>Output</td>
			</tr>
			<tr>
				<td>29</td><td>ADC0_SE10/ADC1_SE10/ADC1_DM2/PTB2/I2C0_SCL/UART0_RTS_b/FTM0_FLT1/FTM0_FLT3</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0<br/>ADC1<br/>ADC1</td><td bgcolor='#F8FF9A'>adc_se10<br/>adc_se10<br/>adc_dm2</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOB</td><td bgcolor='#F7DCFF'>port2</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sclk</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td bgcolor='#5FE356'>UART0</td><td bgcolor='#5FE356'>uart_rts</td><td bgcolor='#5FE356'>Output</td>
				<td bgcolor='#B3EAFF'>FTM0</td><td bgcolor='#B3EAFF'>tmr_fault1</td><td bgcolor='#B3EAFF'>Input</td>
				<td></td><td></td><td></td>
				<td bgcolor='#B3EAFF'>FTM0</td><td bgcolor='#B3EAFF'>tmr_fault3</td><td bgcolor='#B3EAFF'>Input</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>30</td><td>ADC1_SE2/ADC1_DP2/PTB3/I2C0_SDA/UART0_CTS_b/FTM0_FLT0</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC1</td><td bgcolor='#F8FF9A'>adc_se2<br/>adc_dp2</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOB</td><td bgcolor='#F7DCFF'>port3</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sda</td><td bgcolor='#AFFF8E'>Input/Output</td>
				<td bgcolor='#5FE356'>UART0</td><td bgcolor='#5FE356'>uart_cts</td><td bgcolor='#5FE356'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#B3EAFF'>FTM0</td><td bgcolor='#B3EAFF'>tmr_fault0</td><td bgcolor='#B3EAFF'>Input</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>31</td><td>PTB16/UART0_RX/FTM_CLKIN2/EWM_IN</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOB</td><td bgcolor='#F7DCFF'>port16</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#5FE356'>UART0</td><td bgcolor='#5FE356'>uart_rx</td><td bgcolor='#5FE356'>Input</td>
				<td bgcolor='#B3EAFF'>FTM0<br/>FTM1<br/>FTM2</td><td bgcolor='#B3EAFF'>tmr_clk</td><td bgcolor='#B3EAFF'>Input</td>
				<td></td><td></td><td></td>
				<td bgcolor='#CEFFFF'>EWM</td><td bgcolor='#CEFFFF'>ewminput<br/>ewm_in</td><td bgcolor='#CEFFFF'>Input</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>32</td><td>PTB17/UART0_TX/FTM_CLKIN1/EWM_OUT_b</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOB</td><td bgcolor='#F7DCFF'>port17</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>UART0<br/>SIM</td><td bgcolor='#FFFFFF'>uart_tx<br/>uart_tx0</td><td bgcolor='#FFFFFF'>Output</td>
				<td bgcolor='#B3EAFF'>FTM0<br/>FTM1<br/>FTM2</td><td bgcolor='#B3EAFF'>tmr_clk</td><td bgcolor='#B3EAFF'>Input</td>
				<td></td><td></td><td></td>
				<td bgcolor='#CEFFFF'>EWM</td><td bgcolor='#CEFFFF'>ewmoutput<br/>ewm_out</td><td bgcolor='#CEFFFF'>Output</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>33</td><td>ADC1_SE11/PTC0/SPI0_PCS4/PDB0_EXTRG/CMP0_OUT/FTM0_FLT0/SPI0_PCS0/SS_b</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC1</td><td bgcolor='#F8FF9A'>adc_se11</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOC</td><td bgcolor='#F7DCFF'>port0</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_cs4</td><td bgcolor='#90EE67'>Output</td>
				<td bgcolor='#FFFFFF'>PDB0<br/>PDB0<br/>ADC0<br/>ADC0<br/>ADC1<br/>ADC1</td><td bgcolor='#FFFFFF'>PDBtrigger<br/>pdb_trig0<br/>ADCtriggerA<br/>ADCtriggerB<br/>ADCtriggerA<br/>ADCtriggerB</td><td bgcolor='#FFFFFF'>Input</td>
				<td></td><td></td><td></td>
				<td bgcolor='#EFF174'>CMP0</td><td bgcolor='#EFF174'>Output</td><td bgcolor='#EFF174'>Output</td>
				<td bgcolor='#B3EAFF'>FTM0</td><td bgcolor='#B3EAFF'>tmr_fault0</td><td bgcolor='#B3EAFF'>Input</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_cs0</td><td bgcolor='#90EE67'>Input, Output</td>
			</tr>
			<tr>
				<td>34</td><td>ADC1_SE3/PTC1/LLWU_P6/SPI0_PCS3/UART1_RTS_b/FTM0_CH0/FTM2_CH0</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC1</td><td bgcolor='#F8FF9A'>adc_se3</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#FFFFFF'>GPIOC<br/>LLWU</td><td bgcolor='#FFFFFF'>port1<br/>wake_up6</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_cs3</td><td bgcolor='#90EE67'>Output</td>
				<td bgcolor='#5FE356'>UART1</td><td bgcolor='#5FE356'>uart_rts</td><td bgcolor='#5FE356'>Output</td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch0<br/>tmr0_ch0</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#FFFFFF'>FTM2<br/>SIM<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch0<br/>tmr2_ch0<br/>tmr_xorFTM2_CH0</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>35</td><td>ADC0_SE11/CMP1_IN0/PTC2/SPI0_PCS2/UART1_CTS_b/FTM0_CH1/FTM2_CH1</td><td><small><i>same</i></small></td>
				<td bgcolor='#FFFFFF'>ADC0<br/>CMP1<br/>CMP1<br/>CMP1</td><td bgcolor='#FFFFFF'>adc_se11<br/>cmp_in0<br/>Positive0<br/>Negative0</td><td bgcolor='#FFFFFF'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOC</td><td bgcolor='#F7DCFF'>port2</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_cs2</td><td bgcolor='#90EE67'>Output</td>
				<td bgcolor='#5FE356'>UART1</td><td bgcolor='#5FE356'>uart_cts</td><td bgcolor='#5FE356'>Input</td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch1<br/>tmr0_ch1</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#FFFFFF'>FTM2<br/>SIM<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch1<br/>tmr2_ch1<br/>tmr_xorFTM2_CH1</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>36</td><td>CMP1_IN1/PTC3/LLWU_P7/SPI0_PCS1/UART1_RX/FTM0_CH2/CLKOUT</td><td><small><i>same</i></small></td>
				<td bgcolor='#EFF174'>CMP1</td><td bgcolor='#EFF174'>cmp_in1<br/>Positive1<br/>Negative1</td><td bgcolor='#EFF174'>Input</td>
				<td bgcolor='#FFFFFF'>GPIOC<br/>LLWU</td><td bgcolor='#FFFFFF'>port3<br/>wake_up7</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_cs1</td><td bgcolor='#90EE67'>Output</td>
				<td bgcolor='#5FE356'>UART1</td><td bgcolor='#5FE356'>uart_rx</td><td bgcolor='#5FE356'>Input</td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch2<br/>tmr0_ch2</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#DDC7B5'>SIM</td><td bgcolor='#DDC7B5'>ClockOutput0</td><td bgcolor='#DDC7B5'>Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>37</td><td>PTC4/LLWU_P8/SPI0_PCS0/SS_b/UART1_TX/FTM0_CH3/CMP1_OUT</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>GPIOC<br/>LLWU</td><td bgcolor='#FFFFFF'>port4<br/>wake_up8</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_cs0</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#FFFFFF'>UART1<br/>SIM</td><td bgcolor='#FFFFFF'>uart_tx<br/>uart_tx1</td><td bgcolor='#FFFFFF'>Output</td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch3<br/>tmr0_ch3</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#EFF174'>CMP1</td><td bgcolor='#EFF174'>Output</td><td bgcolor='#EFF174'>Output</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>38</td><td>PTC5/LLWU_P9/SPI0_SCK/LPTMR0_ALT2/CMP0_OUT/FTM0_CH2</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>GPIOC<br/>LLWU</td><td bgcolor='#FFFFFF'>port5<br/>wake_up9</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_sck</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#86DAFF'>LPTMR0</td><td bgcolor='#86DAFF'>tmr_clk2</td><td bgcolor='#86DAFF'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#EFF174'>CMP0</td><td bgcolor='#EFF174'>Output</td><td bgcolor='#EFF174'>Output</td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch2<br/>tmr0_ch2</td><td bgcolor='#FFFFFF'>Input, Output</td>
			</tr>
			<tr>
				<td>39</td><td>CMP0_IN0/PTC6/LLWU_P10/SPI0_SOUT/PDB0_EXTRG/UART0_RX/I2C0_SCL</td><td><small><i>same</i></small></td>
				<td bgcolor='#EFF174'>CMP0</td><td bgcolor='#EFF174'>cmp_in0<br/>Positive0<br/>Negative0</td><td bgcolor='#EFF174'>Input</td>
				<td bgcolor='#FFFFFF'>GPIOC<br/>LLWU</td><td bgcolor='#FFFFFF'>port6<br/>wake_up10</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_txd</td><td bgcolor='#90EE67'>Output</td>
				<td bgcolor='#FFFFFF'>PDB0<br/>PDB0<br/>ADC0<br/>ADC0<br/>ADC1<br/>ADC1</td><td bgcolor='#FFFFFF'>PDBtrigger<br/>pdb_trig0<br/>ADCtriggerA<br/>ADCtriggerB<br/>ADCtriggerA<br/>ADCtriggerB</td><td bgcolor='#FFFFFF'>Input</td>
				<td></td><td></td><td></td>
				<td bgcolor='#5FE356'>UART0</td><td bgcolor='#5FE356'>uart_rx</td><td bgcolor='#5FE356'>Input</td>
				<td></td><td></td><td></td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sclk</td><td bgcolor='#AFFF8E'>Input/Output</td>
			</tr>
			<tr>
				<td>40</td><td>CMP0_IN1/PTC7/SPI0_SIN/UART0_TX/I2C0_SDA</td><td><small><i>same</i></small></td>
				<td bgcolor='#EFF174'>CMP0</td><td bgcolor='#EFF174'>cmp_in1<br/>Positive1<br/>Negative1</td><td bgcolor='#EFF174'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOC</td><td bgcolor='#F7DCFF'>port7</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_rxd</td><td bgcolor='#90EE67'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>UART0<br/>SIM</td><td bgcolor='#FFFFFF'>uart_tx<br/>uart_tx0</td><td bgcolor='#FFFFFF'>Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sda</td><td bgcolor='#AFFF8E'>Input/Output</td>
			</tr>
			<tr>
				<td>41</td><td>PTD0/LLWU_P12/SPI0_PCS0/SS_b/UART0_CTS_b/FTM0_CH0/UART1_RX</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>GPIOD<br/>LLWU</td><td bgcolor='#FFFFFF'>port0<br/>wake_up12</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_cs0</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#5FE356'>UART0</td><td bgcolor='#5FE356'>uart_cts</td><td bgcolor='#5FE356'>Input</td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch0<br/>tmr0_ch0</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#5FE356'>UART1</td><td bgcolor='#5FE356'>uart_rx</td><td bgcolor='#5FE356'>Input</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>42</td><td>ADC0_SE2/PTD1/SPI0_SCK/UART0_RTS_b/FTM0_CH1/UART1_TX</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_se2</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOD</td><td bgcolor='#F7DCFF'>port1</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_sck</td><td bgcolor='#90EE67'>Input, Output</td>
				<td bgcolor='#5FE356'>UART0</td><td bgcolor='#5FE356'>uart_rts</td><td bgcolor='#5FE356'>Output</td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch1<br/>tmr0_ch1</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#FFFFFF'>UART1<br/>SIM</td><td bgcolor='#FFFFFF'>uart_tx<br/>uart_tx1</td><td bgcolor='#FFFFFF'>Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>43</td><td>PTD2/LLWU_P13/SPI0_SOUT/UART0_RX/FTM0_CH2/I2C0_SCL</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>GPIOD<br/>LLWU</td><td bgcolor='#FFFFFF'>port2<br/>wake_up13</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_txd</td><td bgcolor='#90EE67'>Output</td>
				<td bgcolor='#5FE356'>UART0</td><td bgcolor='#5FE356'>uart_rx</td><td bgcolor='#5FE356'>Input</td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch2<br/>tmr0_ch2</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sclk</td><td bgcolor='#AFFF8E'>Input/Output</td>
			</tr>
			<tr>
				<td>44</td><td>PTD3/SPI0_SIN/UART0_TX/FTM0_CH3/I2C0_SDA</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOD</td><td bgcolor='#F7DCFF'>port3</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_rxd</td><td bgcolor='#90EE67'>Input</td>
				<td bgcolor='#FFFFFF'>UART0<br/>SIM</td><td bgcolor='#FFFFFF'>uart_tx<br/>uart_tx0</td><td bgcolor='#FFFFFF'>Output</td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch3<br/>tmr0_ch3</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td></td><td></td><td></td>
				<td bgcolor='#AFFF8E'>I2C0</td><td bgcolor='#AFFF8E'>i2c_sda</td><td bgcolor='#AFFF8E'>Input/Output</td>
			</tr>
			<tr>
				<td>45</td><td>PTD4/LLWU_P14/SPI0_PCS1/UART0_RTS_b/FTM0_CH4/FTM2_CH0/EWM_IN</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>GPIOD<br/>LLWU</td><td bgcolor='#FFFFFF'>port4<br/>wake_up14</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_cs1</td><td bgcolor='#90EE67'>Output</td>
				<td bgcolor='#5FE356'>UART0</td><td bgcolor='#5FE356'>uart_rts</td><td bgcolor='#5FE356'>Output</td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch4<br/>tmr0_ch4</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#FFFFFF'>FTM2<br/>SIM<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch0<br/>tmr2_ch0<br/>tmr_xorFTM2_CH0</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#CEFFFF'>EWM</td><td bgcolor='#CEFFFF'>ewminput<br/>ewm_in</td><td bgcolor='#CEFFFF'>Input</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>46</td><td>ADC0_SE3/PTD5/SPI0_PCS2/UART0_CTS_b/FTM0_CH5/FTM2_CH1/EWM_OUT_b</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC0</td><td bgcolor='#F8FF9A'>adc_se3</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#F7DCFF'>GPIOD</td><td bgcolor='#F7DCFF'>port5</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_cs2</td><td bgcolor='#90EE67'>Output</td>
				<td bgcolor='#5FE356'>UART0</td><td bgcolor='#5FE356'>uart_cts</td><td bgcolor='#5FE356'>Input</td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch5<br/>tmr0_ch5</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#FFFFFF'>FTM2<br/>SIM<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch1<br/>tmr2_ch1<br/>tmr_xorFTM2_CH1</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#CEFFFF'>EWM</td><td bgcolor='#CEFFFF'>ewmoutput<br/>ewm_out</td><td bgcolor='#CEFFFF'>Output</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>47</td><td>ADC1_SE6/PTD6/LLWU_P15/SPI0_PCS3/UART0_RX/FTM0_CH0/FTM1_CH0/FTM0_FLT0</td><td><small><i>same</i></small></td>
				<td bgcolor='#F8FF9A'>ADC1</td><td bgcolor='#F8FF9A'>adc_sea6</td><td bgcolor='#F8FF9A'>Input</td>
				<td bgcolor='#FFFFFF'>GPIOD<br/>LLWU</td><td bgcolor='#FFFFFF'>port6<br/>wake_up15</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#90EE67'>SPI0</td><td bgcolor='#90EE67'>spi_cs3</td><td bgcolor='#90EE67'>Output</td>
				<td bgcolor='#5FE356'>UART0</td><td bgcolor='#5FE356'>uart_rx</td><td bgcolor='#5FE356'>Input</td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch0<br/>tmr0_ch0</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#B3EAFF'>FTM1</td><td bgcolor='#B3EAFF'>tmr_ch0</td><td bgcolor='#B3EAFF'>Input, Output</td>
				<td bgcolor='#B3EAFF'>FTM0</td><td bgcolor='#B3EAFF'>tmr_fault0</td><td bgcolor='#B3EAFF'>Input</td>
				<td></td><td></td><td></td>
			</tr>
			<tr>
				<td>48</td><td>PTD7/UART0_TX/FTM0_CH1/FTM1_CH1/FTM0_FLT1</td><td><small><i>same</i></small></td>
				<td></td><td></td><td></td>
				<td bgcolor='#F7DCFF'>GPIOD</td><td bgcolor='#F7DCFF'>port7</td><td bgcolor='#F7DCFF'>Input, Output</td>
				<td></td><td></td><td></td>
				<td bgcolor='#FFFFFF'>UART0<br/>SIM</td><td bgcolor='#FFFFFF'>uart_tx<br/>uart_tx0</td><td bgcolor='#FFFFFF'>Output</td>
				<td bgcolor='#FFFFFF'>FTM0<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch1<br/>tmr0_ch1</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#FFFFFF'>FTM1<br/>SIM</td><td bgcolor='#FFFFFF'>tmr_ch1<br/>tmr_xorFTM1_CH1</td><td bgcolor='#FFFFFF'>Input, Output</td>
				<td bgcolor='#B3EAFF'>FTM0</td><td bgcolor='#B3EAFF'>tmr_fault1</td><td bgcolor='#B3EAFF'>Input</td>
				<td></td><td></td><td></td>
			</tr>
		</table>

*/
