Near End High Speed Signal Quality Test
Results for dev_up_near_el_2_4_5_6_7

For details on test setup, methodology, and performance criteria, please consult the signal quality test description at the USB-IF Compliance Program web page.

Required Tests

- Overall result: pass!

- Signal eye:
  eye passes
- EOP width: 7.97 bits
  EOP width passes
- Measured signaling rate: 479.9438 MHz
  signal rate passes
- Rising Edge Rate: 1105.37 V/us (578.99 ps equivalent risetime)
  passes
- Falling Edge Rate: 1090.28 V/us (587.00 ps equivalent risetime)
  passes
- Edge Monotonicity: 0 mV
  Monotonic Edge passes

Additional Information

- Consecutive jitter range: -57.313 ps to 72.821 ps, RMS jitter 24.723 ps
  Paired JK jitter range: -59.154 ps to 55.015 ps, RMS jitter 24.430 ps
  Paired KJ jitter range: -55.923 ps to 59.462 ps, RMS jitter 25.716 ps

Signal Data and Eye

Tracking Information

- Analysis call: usbsigcheck('G:\LPC1800\el_2_4_5_6_7\dev_up_near_el_2_4_5_6_7.csv', 'hsne')
- Testing script version: 2.60.00
- Analysis performed: 28-Dec-2010 15:11:44