Chirp-Test Results for hs_001

For details on test setup, methodology, and performance criteria, please consult the power consumption requirements test description at the http://www.usb.org/developers/compliance/ USB-IF Compliance Program web page.

Required Tests

- Chirp Test Result: Pass
- Chirp K-Duration: 1.999609mS and USB Limits: 1.000000mS to 7.000000mS
- Chirp Reset Time: 903.4832uS and USB Limits: 2.500000uS to 6.000000mS

Additional Information

- Chirp-K Amplitude : 968.2200mV
- USB Specification Limits : Amplitude ~ 800.0000mV

TDSUSB2 software version: 3.5.0 Build 3