| Kinetis SDK v.2.0 API Reference Manual Rev. 0 Freescale Semiconductor, Inc.

- Main Page
- Related Pages
- API Reference

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Files | Data Structures
UART µCOS/III Driver
UART: Universal Asynchronous Receiver/Transmitter Driver

## Overview

## Files
file | fsl_uart_ucosiii.h

## Data Structures
struct | rtos_uart_config
| UART configuration structure. More...
struct | uart_rtos_handle_t
| UART FreeRTOS handle. More...

## Driver version
#define | FSL_UART_UCOSIII_DRIVER_VERSION (MAKE_VERSION(2, 0, 0))
| UART µCOS-III driver version 2.0.0. More...

## UART RTOS Operation
int | UART_RTOS_Init (uart_rtos_handle_t *handle, uart_handle_t *t_handle, const struct rtos_uart_config *cfg)
| Initializes a UART instance for operation in RTOS. More...
int | UART_RTOS_Deinit (uart_rtos_handle_t *handle)
| Deinitializes a UART instance for operation. More...

## UART transactional Operation
int | UART_RTOS_Send (uart_rtos_handle_t *handle, const uint8_t *buffer, uint32_t length)
| Sends data in the background. More...
int | UART_RTOS_Receive (uart_rtos_handle_t *handle, uint8_t *buffer, uint32_t length, size_t *received)
| Receives data. More...

## Data Structure Documentation

struct rtos_uart_config

### Data Fields
UART_Type * | base
| UART base address.
uint32_t | srcclk
| UART source clock in Hz.
uint32_t | baudrate
| Desired communication speed.
uart_parity_mode_t | parity
| Parity setting.
uart_stop_bit_count_t | stopbits
| Number of stop bits to use.
uint8_t * | buffer
| Buffer for background reception.
uint32_t | buffer_size
| Size of buffer for background reception.

struct uart_rtos_handle_t

### Data Fields
UART_Type * | base
| UART base address.
struct _uart_transfer | tx_xfer
| TX transfer structure.
struct _uart_transfer | rx_xfer
| RX transfer structure.
SemaphoreHandle_t | rx_sem
| RX semaphore for resource sharing.
SemaphoreHandle_t | tx_sem
| TX semaphore for resource sharing.
EventGroupHandle_t | rx_event
| RX completion event.
EventGroupHandle_t | tx_event
| TX completion event.
void * | t_state
| Transactional state of the underlying driver.
OS_EVENT * | rx_sem
| RX semaphore for resource sharing.
OS_EVENT * | tx_sem
| TX semaphore for resource sharing.
OS_FLAG_GRP * | rx_event
| RX completion event.
OS_FLAG_GRP * | tx_event
| TX completion event.
OS_SEM | rx_sem
| RX semaphore for resource sharing.
OS_SEM | tx_sem
| TX semaphore for resource sharing.
OS_FLAG_GRP | rx_event
| RX completion event.
OS_FLAG_GRP | tx_event
| TX completion event.

## Macro Definition Documentation

#define FSL_UART_UCOSIII_DRIVER_VERSION (MAKE_VERSION(2, 0, 0))

## Function Documentation

int UART_RTOS_Init | ( | uart_rtos_handle_t * | handle,
|  | uart_handle_t * | t_handle,
|  | const struct rtos_uart_config * | cfg
| ) |  |

Parameters

  handle | The RTOS UART handle, the pointer to allocated space for RTOS context.
  uart_t_handle | The pointer to an allocated space where to store transactional layer internal state.
  cfg | The pointer to the parameters required to configure the UART after initialization.

Returns
  0 Succeed, others fail.

int UART_RTOS_Deinit | ( | uart_rtos_handle_t * | handle | ) |

This function deinitializes the UART module, sets all register values to reset value, and releases the resources.

Parameters

  handle | The RTOS UART handle.

int UART_RTOS_Send | ( | uart_rtos_handle_t * | handle,
|  | const uint8_t * | buffer,
|  | uint32_t | length
| ) |  |

This function sends data. It is a synchronous API. If the hardware buffer is full, the task is in the blocked state.

Parameters

  handle | The RTOS UART handle.
  buffer | The pointer to buffer to send.
  length | The number of bytes to send.

int UART_RTOS_Receive | ( | uart_rtos_handle_t * | handle,
|  | uint8_t * | buffer,
|  | uint32_t | length,
|  | size_t * | received
| ) |  |

This function receives data from UART. It is a synchronous API. If any data is immediately available, it is returned immediately and the number of bytes received.

Parameters

  handle | The RTOS UART handle.
  buffer | The pointer to buffer where to write received data.
  length | The number of bytes to receive.
  received | The pointer to variable of a size_t where the number of received data is filled.