NXP NFC Reader Library v4.040.05.011646

Data Fields
phacDiscLoop_I18000p3m3_Info Struct Reference
Activity Layer » Discovery Loop » Component : Software

18000p3m3 parameter structure More...

## Data Fields
uint8_t | bTotalTagsFound
| Holds the number of tags detected.
uint8_t | bM
| Modulation; default PHPAL_I18000P3M3_M_MANCHESTER_4.
uint8_t | bDr
| Link frequency; default PHPAL_I18000P3M3_LF_847KHZ.

## Detailed Description

18000p3m3 parameter structure

The documentation for this struct was generated from the following file:

- phacDiscLoop.h