NXP NFC Reader Library v4.040.05.011646

Data Fields
phnpSnep_Sw_DataParams Struct Reference
Network Protocol Layer » NFCForum-SNEP » Component : Software

SNEP parameter structure. More...

## Data Fields
uint16_t | wId
| Layer ID for this component, NEVER MODIFY!. More...
void * | plnLlcpDataParams
| LLCP Data Parameters structure pointer. More...
void * | psSocket
| LLCP transport Socket structure pointer. More...
uint8_t | bSnepVersion
| SNEP protocol version supported by Implementation. More...
phnpSnep_Server_type_t | eServerType
| Initialized Server Type. More...

## Detailed Description

SNEP parameter structure.

## Field Documentation

## § wId

uint16_t phnpSnep_Sw_DataParams::wId

Layer ID for this component, NEVER MODIFY!.

## § plnLlcpDataParams

void* phnpSnep_Sw_DataParams::plnLlcpDataParams

LLCP Data Parameters structure pointer.

## § psSocket

void* phnpSnep_Sw_DataParams::psSocket

LLCP transport Socket structure pointer.

## § bSnepVersion

uint8_t phnpSnep_Sw_DataParams::bSnepVersion

SNEP protocol version supported by Implementation.

## § eServerType

phnpSnep_Server_type_t phnpSnep_Sw_DataParams::eServerType

Initialized Server Type.

The documentation for this struct was generated from the following file:

- phnpSnep.h