| eRPC API Reference Rev. 1.8.1 NXP Semiconductors

- Main Page
- API Reference
- Classes
- Files

- Class List
- Class Index
- Class Hierarchy
- Class Members

Class List
Here are the classes, structs, unions and interfaces with brief descriptions:
[detail level 1 2 3]

▼N erpc |
C ArbitratedClientManager | Client that can share a transport with a server
C BasicCodec | Simple binary serialization format
C BasicCodecFactory | Basic codec factory implements functions from codec factory
C ClientManager | Base client implementation
C ClientServerCommon | Common class inheritand by client and server class
C Codec | Abstract serialization encoder/decoder interface
C CodecFactory | Abstract interface for codec factory
C Crc16 | Class for compute crc16
C DspiMasterTransport | Very basic transport to send/receive messages via DSPI
C DspiSlaveTransport | Very basic transport to send/receive messages via DSPI
▼C FramedTransport | Base class for framed transport layers
C Header | Contents of the header that prefixes each message
C I2cSlaveTransport | Very basic transport to send/receive messages via I2C
▼C InterThreadBufferTransport | Very basic transport to send/receive messages between threads
C SharedState |
C ManuallyConstructed | Allocates static storage for an object
▼C MessageBuffer | Represents a memory buffer containing a message
C Cursor | Cursor within a MessageBuffer
C MessageBufferFactory | Abstract interface for message buffer factory
C MessageLogger | Logging messages objects used for logging sent/received messages
C MessageLoggers | Logging messages functionality
▼C Mutex | Mutex
C Guard |
C MUTransport | Transport that uses Messaging Unit (MU) for interprocessor messaging
C PrePostAction | Client and server may used cb functions before and after rpc call
C RequestContext | Encapsulates all information about a request
C RPMsgBaseTransport | Transport that other RPMsg transports inherits
C RPMsgLinuxTransport | RPMSG Linux transport to send/receive messages through RPMSG endpoints based on github.com/NXPmicro/rpmsg-sysfs/tree/0aa1817545a765c200b1b2f9b6680a420dcf9171 implementation
C RPMsgRTOSTransport | Transport that uses RPMsg zero copy RTOS API for interprocessor messaging
C RPMsgTransport | Transport that uses RPMsg zero copy API for interprocessor messaging
C RPMsgTTYRTOSTransport | Transport that uses RPMsg zero copy RTOS API for interprocessor messaging
C Semaphore | Simple semaphore class
C SerialTransport | Serial transport layer for host PC
C Server | Based server functionality
C Service | Abstract interface for service, which can be executed on server side
C SimpleServer | Based server implementation
C SpidevMasterTransport | Very basic transport to send/receive messages via SPIdev
C SpiMasterTransport | Very basic transport to send/receive messages via SPI
C SpiSlaveTransport | Very basic transport to send/receive messages via SPI
C StaticQueue | Template class which implements static queue as ring buffer
C TCPTransport | Client side of TCP/IP transport
C Thread | Simple thread class
C Transport | Abstract interface for transport layer
▼C TransportArbitrator | Interposer to share transport between client and server
C PendingClientInfo | Request info for a client trying to receive a response
C TransportFactory | Abstract interface for transport factory
C UartTransport | Very basic transport to send/receive messages via UART
C UsbCdcTransport | Very basic transport to send/receive messages via virtual USB CDC port
C DynamicMessageBufferFactory | Dynamic message buffer factory
C I2C_CLB_USER_DATA_PTR |
C RPMsgMessageBufferFactory | RPMsg zero copy message buffer factory
C RPMsgTTYMessageBufferFactory | RPMsg TTY message buffer factory
C StaticMessageBufferFactory | Static Message buffer factory