MCUX CLNS MCUX Crypto Library Normal Secure |

Data Structures | Macros | Typedefs | Functions
mcuxClPkc_Functions.h File Reference

APIs of mcuxClPkc component. More...

`#include <stdint.h>`
`#include <stdbool.h>`
`#include <mcuxCsslFlowProtection.h>`
`#include <mcuxClPkc_Types.h>`

Go to the source code of this file.

## Data Structures
struct | mcuxClPkc_State_t
| Structure of PKC state backup. More...

## Macros
#define | MCUXCLPKC_FP_INITIALIZE(pState)
| Helper macro to call mcuxClPkc_Initialize with flow protection. More...
#define | MCUXCLPKC_FP_DEINITIALIZE(pState)
| Helper macro to call mcuxClPkc_Deinitialize with flow protection. More...
#define | MCUXCLPKC_FP_GENERATEUPTRT(pUPTRT, pBaseBuffer, bufferSize, noOfBuffer)
| Helper macro to call mcuxClPkc_GenerateUPTRT with flow protection. More...
#define | MCUXCLPKC_FP_CALCFUP(pUPTR, ulen)
| Helper macro to call mcuxClPkc_CalcFup with flow protection. More...
#define | MCUXCLPKC_FP_CALCFUP_OFFSET(pUPTR, skipLen, ulen)
| Helper macro to call mcuxClPkc_CalcFup (skipping first skipLen calculation(s)) with flow protection. More...
#define | MCUXCLPKC_FP_WAITFORFINISH()
| Helper macro to call mcuxClPkc_WaitForFinish with flow protection. More...
#define | MCUXCLPKC_FP_WAITFORREADY()
| Helper macro to call mcuxClPkc_WaitForReady with flow protection. More...

## Typedefs
typedef const struct mcuxClPkc_FUPEntry * | mcuxClPkc_PtrFUPEntry_t
| type of FUP program address. More...

## Functions
mcuxClPkc_Status_Protected_t | mcuxClPkc_Initialize (mcuxClPkc_State_t *pState)
| initialize PKC hardware More...
mcuxClPkc_Status_Protected_t | mcuxClPkc_Deinitialize (const mcuxClPkc_State_t *pState)
| deinitialize PKC hardware More...
mcuxClPkc_Status_Protected_t | mcuxClPkc_GenerateUPTRT (uint16_t *pUPTRT, const uint8_t *pBaseBuffer, uint16_t bufferSize, uint8_t noOfBuffer)
| Initialize UPTR table. More...
mcuxClPkc_Status_Protected_t | mcuxClPkc_RandomizeUPTRT (uint16_t *pUPTRT, uint8_t noOfBuffer)
| Randomize UPTR table. More...
mcuxClPkc_Status_Protected_t | mcuxClPkc_ReRandomizeUPTRT (uint16_t *pUPTRT, uint16_t bufferSize, uint8_t noOfBuffer)
| Randomize UPTR table and operands in PKC workarea. More...
mcuxClPkc_Status_Protected_t | mcuxClPkc_Calc (uint16_t param_mode, uint32_t iR_iX_iY_iZ)
| Start a PKC calculation. More...
mcuxClPkc_Status_Protected_t | mcuxClPkc_CalcConst (uint16_t param_mode, uint32_t iR_iX_iY_C)
| Start a PKC calculation with one constant parameter. More...
mcuxClPkc_Status_Protected_t | mcuxClPkc_CalcFup (mcuxClPkc_PtrFUPEntry_t pUPTR, uint8_t ulen)
| Start a PKC FUP program calculation. More...
mcuxClPkc_Status_Protected_t | mcuxClPkc_WaitForFinish (void)
| Wait until PKC finishes calculations. More...
mcuxClPkc_Status_Protected_t | mcuxClPkc_WaitForReady (void)
| Wait until PKC is ready to accept new calculation. More...

## Detailed Description

APIs of mcuxClPkc component.