| RPMsg-Lite User's Guide Rev. 3.1.2 NXP Semiconductors

- Main Page
- API Reference

rpmsg_default_config.h
Go to the documentation of this file.
1 /*
2 * Copyright (c) 2014, Mentor Graphics Corporation
3 * Copyright (c) 2015 Xilinx, Inc.
4 * Copyright (c) 2016 Freescale Semiconductor, Inc.
5 * Copyright 2016-2021 NXP
6 * All rights reserved.
7 *
8 * Redistribution and use in source and binary forms, with or without
9 * modification, are permitted provided that the following conditions are met:
10 *
11 * 1. Redistributions of source code must retain the above copyright notice,
12 * this list of conditions and the following disclaimer.
13 * 2. Redistributions in binary form must reproduce the above copyright notice,
14 * this list of conditions and the following disclaimer in the documentation
15 * and/or other materials provided with the distribution.
16 * 3. Neither the name of the copyright holder nor the names of its
17 * contributors may be used to endorse or promote products derived from this
18 * software without specific prior written permission.
19 *
20 * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
21 * AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
22 * IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
23 * ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT HOLDER OR CONTRIBUTORS BE
24 * LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
25 * CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF
26 * SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
27 * INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
28 * CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
29 * ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
30 * POSSIBILITY OF SUCH DAMAGE.
31 */
32
33 #ifndef RPMSG_DEFAULT_CONFIG_H_
34 #define RPMSG_DEFAULT_CONFIG_H_
35
36 #define RL_USE_CUSTOM_CONFIG (1)
37
38 #if RL_USE_CUSTOM_CONFIG
39 #include "rpmsg_config.h"
40 #endif
41
48
50
55 #ifndef RL_MS_PER_INTERVAL
56 #define RL_MS_PER_INTERVAL (1)
57 #endif
58
64 #ifndef RL_BUFFER_PAYLOAD_SIZE
65 #define RL_BUFFER_PAYLOAD_SIZE (496U)
66 #endif
67
76 #ifndef RL_BUFFER_COUNT
77 #define RL_BUFFER_COUNT (2U)
78 #endif
79
84 #ifndef RL_API_HAS_ZEROCOPY
85 #define RL_API_HAS_ZEROCOPY (1)
86 #endif
87
92 #ifndef RL_USE_STATIC_API
93 #define RL_USE_STATIC_API (0)
94 #endif
95
101 #ifndef RL_CLEAR_USED_BUFFERS
102 #define RL_CLEAR_USED_BUFFERS (0)
103 #endif
104
111 #ifndef RL_USE_MCMGR_IPC_ISR_HANDLER
112 #define RL_USE_MCMGR_IPC_ISR_HANDLER (0)
113 #endif
114
120 #ifndef RL_USE_ENVIRONMENT_CONTEXT
121 #define RL_USE_ENVIRONMENT_CONTEXT (0)
122 #endif
123
127 #ifndef RL_DEBUG_CHECK_BUFFERS
128 #define RL_DEBUG_CHECK_BUFFERS (0)
129 #endif
130
138 #ifndef RL_ALLOW_CONSUMED_BUFFERS_NOTIFICATION
139 #define RL_ALLOW_CONSUMED_BUFFERS_NOTIFICATION (0)
140 #endif
141
145 static inline void RL_HANG(void)
146 {
147 for (;;)
148 {
149 }
150 }
151
155 #ifndef RL_ASSERT
156 #define RL_ASSERT_BOOL(b) \
157 do \
158 { \
159 if (!(b)) \
160 { \
161 RL_HANG(); \
162 } \
163 } while (0 == 1);
164 #define RL_ASSERT(x) RL_ASSERT_BOOL((int32_t)(x) != 0)
165
166 #endif
167
168
169 #endif /* RPMSG_DEFAULT_CONFIG_H_ */