=============================================================================
List of generated methods in project: PWM_Lab

THIS TEXT DESCRIPTION IS GENERATED BY THE TOOL. DO NOT MODIFY IT.
=============================================================================

Module "PWM1"      (bean PWM)
   - PWM1_SetRatio16 -This method sets a new duty-cycle ratio. Ratio is expressed as a 16-bit unsigned integer number. 0 - FFFF 
                value is proportional to ratio 0 - 100%.  Note: Calculated duty depends on the timer possibilities and on the 
                selected period.

Module "AD1"       (bean ADC)
   - AD1_Measure -This method performs one measurement on all channels that are set in the bean inspector. (Note: If the 
                <number of conversions> is more than one the conversion of A/D channels is performed specified number of times.)
   - AD1_GetValue16 -This method returns the last measured values of all channels justified to the left. Compared with 
                <GetValue> method this method returns more accurate result if the <number of conversions> is greater than 1 and 
                <AD resolution> is less than 16 bits. In addition, the user code dependency on <AD resolution> is eliminated.

Module "Cpu"       (bean MC9S08QE128_80)
   - Cpu_EnableInt -Enables maskable interrupts
   - Cpu_DisableInt -Disables maskable interrupts

===================================================================================
