/******************************************************************************/
/* 	Quick Start-up Guide for the NXP Cortex-M0 IEC60335 Class B Library   */
/*----------------------------------------------------------------------      */
/*	Clock test example						      */
/******************************************************************************/

---- WELCOME ------------------------------------------------------------
This example code will show how to implement the IEC60335 Class B 
Clock test.

!! Please note this example is only usable for LPC devices with RTC 
   clock. !!

This quick start guide explains how this example project is setup and 
how it can be configured and used best.


---- DIRECTORY STRUCTURE ------------------------------------------------
 Target			  -> 	Select your target, LPC1114 or LPC1227
	+ Config          ->	Folder with configuration source files
	|			(See description below)
	+ Core		  -> 	Core and device specific source files
        |
        + Device          ->    Folder containing the startup and 
        |                       system files for the various processors
        + Drivers         ->	Device specific peripheral drivers 
        |			used in this example
      	+ IEC60335_B_Lib  -> 	NXP Cortex-M0 IEC60335 Class B library
				Selected the corresponding test library

---- CONFIGURATION ------------------------------------------------------
A number of configurations is possible for this examples, please find 
here some more explanation. 
1. 	Select your target with the Target Select drop down box
		-> 	LPC1114 Flash (default)
		->	LPC1227 Flash
   	This will set some project definitions and select the corresponding 
   	source files.
2. 	Configuration files:
2.1	IEC60335_B_UserData.c/.h:
	This source file contains IEC60335 specific configurations
2.2	LPC1xxx_TargetConfig.c/.h:
	These source files contains target specific configurations 

---- ADDITIONAL INFORMATION ---------------------------------------------

	
---- INFORMATION --------------------------------------------------------
- 	Keep the NXP Cortex-M0 IEC60335 Class B application note
	nearby while developing your IEC60335 Class B application	

---- DISCLAIMER ---------------------------------------------------------	
/***********************************************************************
 * Software that is described herein is for illustrative purposes only
 * which provides customers with programming information regarding the
 * products. This software is supplied "AS IS" without any warranties.
 * NXP Semiconductors assumes no responsibility or liability for the
 * use of the software, conveys no license or title under any patent,
 * copyright, or mask work right to the product. NXP Semiconductors
 * reserves the right to make changes in the software without
 * notification. NXP Semiconductors also make no representation or
 * warranty that such application will be suitable for the specified
 * use without further testing or modification.
 **********************************************************************/