| USBD ROM Stack 2.0 ROM based USB device stack

Data Fields
WB_T Struct Reference
USB Core Layer

`#include <C:/Data/nxp/GIT/lpcopen_v3/lpcopen_version3/LPC11u6x/lpc11u6x/LPC_USBD_Lib/mw_usbd/mw_usbd.h>`

## Data Fields
uint8_t | L
uint8_t | H

## Detailed Description

Structure to pack lower and upper byte to form 16 bit word.

## Field Documentation

## ◆ L

uint8_t WB_T::L

lower byte

## ◆ H

uint8_t WB_T::H

upper byte

The documentation for this struct was generated from the following file:

- C:/Data/nxp/GIT/lpcopen_v3/lpcopen_version3/LPC11u6x/lpc11u6x/LPC_USBD_Lib/mw_usbd/mw_usbd.h