| USBD ROM Stack 2.0 ROM based USB device stack

Data Fields
WORD_BYTE Union Reference
USB Core Layer

`#include <C:/Data/nxp/GIT/lpcopen_v3/lpcopen_version3/LPC11u6x/lpc11u6x/LPC_USBD_Lib/mw_usbd/mw_usbd.h>`

## Data Fields
uint16_t | W
WB_T | WB

## Detailed Description

Union of _WB_T struct and 16 bit word.

## Field Documentation

## ◆ W

uint16_t WORD_BYTE::W

data member to do 16 bit access

## ◆ WB

WB_T WORD_BYTE::WB

data member to do 8 bit access

The documentation for this union was generated from the following file:

- C:/Data/nxp/GIT/lpcopen_v3/lpcopen_version3/LPC11u6x/lpc11u6x/LPC_USBD_Lib/mw_usbd/mw_usbd.h