| USBD ROM Stack 2.0 ROM based USB device stack

Data Fields
REQUEST_TYPE Union Reference
USB Core Layer

`#include <C:/Data/nxp/GIT/lpcopen_v3/lpcopen_version3/LPC11u6x/lpc11u6x/LPC_USBD_Lib/mw_usbd/mw_usbd.h>`

## Data Fields
uint8_t | B
BM_T | BM

## Detailed Description

Union of _BM_T struct and 8 bit byte.

## Field Documentation

## ◆ B

uint8_t REQUEST_TYPE::B

byte wide access memeber

## ◆ BM

BM_T REQUEST_TYPE::BM

bitfield structure access memeber

The documentation for this union was generated from the following file:

- C:/Data/nxp/GIT/lpcopen_v3/lpcopen_version3/LPC11u6x/lpc11u6x/LPC_USBD_Lib/mw_usbd/mw_usbd.h