| USBD ROM Stack 1.0 ROM based USB device stack

Data Fields
BM_T Struct Reference
USB Core Layer

`#include <mw_usbd/mw_usbd.h>`

## Data Fields
uint8_t | Recipient: 5
uint8_t | Type: 2
uint8_t | Dir: 1

## Detailed Description

Structure to define 8 bit USB request.

## Field Documentation

## ◆ Recipient

uint8_t BM_T::Recipient

Recipient type.

## ◆ Type

uint8_t BM_T::Type

Request type.

## ◆ Dir

uint8_t BM_T::Dir

Direction type.

The documentation for this struct was generated from the following file:

- mw_usbd/mw_usbd.h