| ISF 1.1 Intelligent Sensing Framework

- Main Page
- Data Structures
- Files
- Sensor Adapters

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines
Defines | Variables
User/Source/isf_sysconf_comms.c File Reference

System Communications channel configuration. More...

`#include <isf_user_config.h>`
`#include <isf_sysconf_types.h>`
`#include <isf_sysconf_comms.h>`

Go to the source code of this file.

## Defines
#define | I2C_MASTER_FXLC95000_BASE_ADDRESS (0xFFFF8040)
#define | FXLC95000_PINMUX_CTRL_REG (0xFFFF806B)
#define | FXLC95000_GPIO_EN_REG (0x00C00004)
#define | FXLC95000_PERIPHERAL_STOPFC (0xFFFF8065)
#define | FXLC95000_PERIPHERAL_RUN (0xFFFF8069)
#define | BUS1_NAME "B1"
#define | PMCR1_A2_LOWER_MASK 0x10
#define | PMCR1_A3_LOWER_MASK 0x40
#define | ONE_SECOND 1000
## Variables
const sys_channelDescriptor_t | gSys_ConfiguredChannelList []
const uint8 | gSys_NumChannels = sizeof(gSys_ConfiguredChannelList)/sizeof(sys_channelDescriptor_t)

## Detailed Description

System Communications channel configuration.

Version:
  0.0

Date:
  2012-08-01

Copyright (c) 2012, Freescale, Inc.

Definition in file isf_sysconf_comms.c.

## Define Documentation

#define BUS1_NAME "B1"

Definition at line 20 of file isf_sysconf_comms.c.

#define FXLC95000_GPIO_EN_REG (0x00C00004)

Definition at line 17 of file isf_sysconf_comms.c.

#define FXLC95000_PERIPHERAL_RUN (0xFFFF8069)

Definition at line 19 of file isf_sysconf_comms.c.

#define FXLC95000_PERIPHERAL_STOPFC (0xFFFF8065)

Definition at line 18 of file isf_sysconf_comms.c.

#define FXLC95000_PINMUX_CTRL_REG (0xFFFF806B)

Definition at line 16 of file isf_sysconf_comms.c.

#define I2C_MASTER_FXLC95000_BASE_ADDRESS (0xFFFF8040)

Definition at line 15 of file isf_sysconf_comms.c.

#define ONE_SECOND 1000

Definition at line 23 of file isf_sysconf_comms.c.

#define PMCR1_A2_LOWER_MASK 0x10

Definition at line 21 of file isf_sysconf_comms.c.

#define PMCR1_A3_LOWER_MASK 0x40

Definition at line 22 of file isf_sysconf_comms.c.

## Variable Documentation

const sys_channelDescriptor_t gSys_ConfiguredChannelList[]

Initial value:

    {
                    {

                     .protocolType       = PROTOCOL_TYPE_I2C,
                     .protocolInstanceId = I2C_BUS_ONE,
                     .pConfig            = &gSys_I2cBusConfig[I2C_BUS_ONE]
                    }
    }

Definition at line 72 of file isf_sysconf_comms.c.

const uint8 gSys_NumChannels = sizeof(gSys_ConfiguredChannelList)/sizeof(sys_channelDescriptor_t)

Definition at line 82 of file isf_sysconf_comms.c.