| ISF 1.1 Intelligent Sensing Framework

- Main Page
- Data Structures
- Files
- Sensor Adapters

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines
User/Include/isf_sysconf_comms.h
Go to the documentation of this file.

    00001 /*!
    00002 ********************************************************************************
    00003 * File: isf_sysconf_comms.h
    00004 *
    00005 * Copyright (c) 2012, Freescale Semiconductor, Inc.
    00006 *
    00007 *******************************************************************************/
    00008 /*!
    00009 * @file isf_sysconf_comms.h
    00010 * @brief  This file defines the system configuration for the communication channel.
    00011 */
    00012 #ifndef ISF_SYSCONF_COMMS_H
    00013 #define ISF_SYSCONF_COMMS_H
    00014
    00015
    00016 /******************************************************************************
    00017  * GENERAL CHANNEL INFORMATION FOR THE SYSTEM
    00018  ******************************************************************************/
    00019
    00020 /*! @brief Declaration of the actual channels available for a particular device.
    00021  *  These enums are indexes into the ::gSys_ConfiguredChannelList array and
    00022  *  facilitate accessing channel configuration data
    00023 */
    00024 enum {
    00025     INTERNAL_CHAN = 255, /*!< The channel ID for the on-board accelerometer channel. */
    00026     I2C_MASTER1 = 0,     /*!< The channel ID for the I2C Master.*/
    00027     SYS_NUM_CHANNEL_IDS  /*!< The number of channels in the system. */
    00028 };
    00029
    00030 #endif /* SYSCONF_COMMS_H */