| ISF 1.1 Intelligent Sensing Framework

- Main Page
- Data Structures
- Files
- Sensor Adapters

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines
Enumerations
User/Include/isf_sysconf_comms.h File Reference

This file defines the system configuration for the communication channel. More...

Go to the source code of this file.

## Enumerations
enum | { INTERNAL_CHAN = 255, I2C_MASTER1 = 0, SYS_NUM_CHANNEL_IDS }
| Declaration of the actual channels available for a particular device. These enums are indexes into the gSys_ConfiguredChannelList array and facilitate accessing channel configuration data. More...

## Detailed Description

This file defines the system configuration for the communication channel.

File: isf_sysconf_comms.h

Copyright (c) 2012, Freescale Semiconductor, Inc.

Definition in file isf_sysconf_comms.h.

## Enumeration Type Documentation

anonymous enum

Declaration of the actual channels available for a particular device. These enums are indexes into the gSys_ConfiguredChannelList array and facilitate accessing channel configuration data.

Enumerator:

  INTERNAL_CHAN | The channel ID for the on-board accelerometer channel.
  I2C_MASTER1 | The channel ID for the I2C Master.
  SYS_NUM_CHANNEL_IDS | The number of channels in the system.

Definition at line 24 of file isf_sysconf_comms.h.