| ISF 2.1 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Modules Pages
isf_sysconf_comms.h
Go to the documentation of this file.
1 /*!
2 ********************************************************************************
3 * File: isf_sysconf_comms.h
4 *
5 * Copyright (c) 2013, Freescale Semiconductor, Inc.
6 *
7 *******************************************************************************/
8 /*!
9 * @file isf_sysconf_comms.h
10 * @brief This file defines the system configuration for the communication channel.
11 */
12 #ifndef ISF_SYSCONF_COMMS_H
13 #define ISF_SYSCONF_COMMS_H
14 #include <isf_target.h>
15 uint32 get_ci_comm(void);
16 /******************************************************************************
17 * GENERAL CHANNEL INFORMATION FOR THE SYSTEM
18 ******************************************************************************/
19
20 /*! @brief Declaration of the actual channels available for a particular device.
21 * These enums are indexes into the ::gSys_ConfiguredChannelList array and
22 * facilitate accessing channel configuration data
23 */
24
25 // Number of communications channels: 3
26
27 // Defined buses
28 enum {
29 COMM_CHANNEL_INTERNAL = 255, /*!< The channel ID for the on-board accelerometer channel. */
30 COMM_CHANNEL_I2C_CH1 = 0, // <*!CommChannel0 */
31 COMM_CHANNEL_UART_CH1 = 1, // <*!CommChannel1 */
32 COMM_CHANNEL_SPI_CH1 = 2, // <*!CommChannel2 */
33 SYS_NUM_CHANNEL_IDS /*!< The number of channels in the system. */
34 };
35
36
37
38 #endif /* SYSCONF_COMMS_H */
39
isf_target.h
ISF board support header files.
COMM_CHANNEL_UART_CH1
Definition: isf_sysconf_comms.h:31
SYS_NUM_CHANNEL_IDS
Definition: isf_sysconf_comms.h:33
COMM_CHANNEL_INTERNAL
Definition: isf_sysconf_comms.h:29
uint32
unsigned long uint32
This defines uint32 as unsigned long.
Definition: isf_types.h:36
COMM_CHANNEL_SPI_CH1
Definition: isf_sysconf_comms.h:32
COMM_CHANNEL_I2C_CH1
Definition: isf_sysconf_comms.h:30
get_ci_comm
uint32 get_ci_comm(void)
Definition: isf_sysconf_comms.c:128
- © Freescale Semiconductor, Inc. 2015. All Rights Reserved.