| ISF 2.1 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Modules Pages
Data Fields
ci_stream_ctrl_reg1_t Struct Reference

Stream protocol control register 1 Structure. More...

`#include <ci_protocol_stream.h>`

Collaboration diagram for ci_stream_ctrl_reg1_t:

## Data Fields
uint8 | ctrl_reg1
struct {
uint8 enable_stream_data:1
uint8 enable_crc:1
uint8 reserved1:6
} | Bits

## Detailed Description

Stream protocol control register 1 Structure.

enable_stream_data : 0 - Stream data disabled, 1 - Stream data enabled enable_crc : 0 - CRC generation/checking disabled, 1 - CRC enabled reserved1 : Reserved Bits

Definition at line 186 of file ci_protocol_stream.h.

## Field Documentation

struct { ... } Bits

Referenced by ci_protocol_CB_stream(), isf_ci_stream_set_CRC(), and isf_ci_stream_update_data().

uint8 ctrl_reg1

Definition at line 187 of file ci_protocol_stream.h.

uint8 enable_crc

Definition at line 190 of file ci_protocol_stream.h.

Referenced by ci_protocol_CB_stream(), isf_ci_stream_set_CRC(), and isf_ci_stream_update_data().

uint8 enable_stream_data

Definition at line 189 of file ci_protocol_stream.h.

Referenced by ci_protocol_CB_stream(), and isf_ci_stream_update_data().

uint8 reserved1

Definition at line 191 of file ci_protocol_stream.h.

The documentation for this struct was generated from the following file:

- ISF/Command_Interpreter/Include/ci_protocol_stream.h

- © Freescale Semiconductor, Inc. 2015. All Rights Reserved.