| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

Data Fields
SysTick_t Struct Reference

Structure type to access the System Timer (SysTick). More...

`#include <isf_systick_defs.h>`

Collaboration diagram for SysTick_t:

## Data Fields
__IO uint32 | CTRL
__IO uint32 | LOAD
__IO uint32 | VAL
__I uint32 | CALIB

## Detailed Description

Structure type to access the System Timer (SysTick).

Definition at line 31 of file isf_systick_defs.h.

## Field Documentation

__I uint32 CALIB

Offset: 0x00C (R/ ) SysTick Calibration Register

Definition at line 36 of file isf_systick_defs.h.

__IO uint32 CTRL

Offset: 0x000 (R/W) SysTick Control and Status Register

Definition at line 33 of file isf_systick_defs.h.

__IO uint32 LOAD

Offset: 0x004 (R/W) SysTick Reload Value Register

Definition at line 34 of file isf_systick_defs.h.

__IO uint32 VAL

Offset: 0x008 (R/W) SysTick Current Value Register

Definition at line 35 of file isf_systick_defs.h.

The documentation for this struct was generated from the following file:

- ISF/Core/Include/isf_systick_defs.h

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.