| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

BMTIMER1.h
Go to the documentation of this file.
1 /* ###################################################################
2 ** This component module is generated by Processor Expert. Do not modify it.
3 ** Filename : BMTIMER1.h
4 ** Project : ISF2P2_K64F_MQX_PROJ
5 ** Processor : MK64FN1M0VLL12
6 ** Component : fsl_pit
7 ** Version : Component 1.2.0, Driver 01.00, CPU db: 3.00.000
8 ** Repository : KSDK 1.2.0
9 ** Compiler : GNU C Compiler
10 ** Date/Time : 2016-10-06, 13:38, # CodeGen: 0
11 ** Contents :
12 ** PIT_DRV_Init - pit_status_t PIT_DRV_Init(uint32_t instance,bool isRunInDebug);
13 ** PIT_DRV_Deinit - pit_status_t PIT_DRV_Deinit(uint32_t instance);
14 ** PIT_DRV_InitChannel - void PIT_DRV_InitChannel(uint32_t instance,uint32_t channel,const...
15 ** PIT_DRV_StartTimer - void PIT_DRV_StartTimer(uint32_t instance,uint32_t channel);
16 ** PIT_DRV_StopTimer - void PIT_DRV_StopTimer(uint32_t instance,uint32_t channel);
17 ** PIT_DRV_SetTimerPeriodByUs - void PIT_DRV_SetTimerPeriodByUs(uint32_t instance,uint32_t channel,uint32_t us);
18 ** PIT_DRV_GetTimerPeriodByUs - uint32_t PIT_DRV_GetTimerPeriodByUs(uint32_t instance,uint32_t channel);
19 ** PIT_DRV_ReadTimerUs - uint32_t PIT_DRV_ReadTimerUs(uint32_t instance,uint32_t channel);
20 ** PIT_DRV_SetTimerPeriodByCount - void PIT_DRV_SetTimerPeriodByCount(uint32_t instance,uint32_t...
21 ** PIT_DRV_GetTimerPeriodByCount - uint32_t PIT_DRV_GetTimerPeriodByCount(uint32_t instance,uint32_t channel);
22 ** PIT_DRV_ReadTimerCount - uint32_t PIT_DRV_ReadTimerCount(uint32_t instance,uint32_t channel);
23 ** PIT_DRV_InitUs - void PIT_DRV_InitUs(uint32_t instance,uint32_t channel);
24 ** PIT_DRV_GetUs - uint32_t PIT_DRV_GetUs(void);
25 ** PIT_DRV_DelayUs - void PIT_DRV_DelayUs(uint32_t us);
26 ** PIT_DRV_ClearIntFlag - void PIT_DRV_ClearIntFlag(uint32_t instance,uint32_t channel);
27 ** PIT_DRV_IsIntPending - bool PIT_DRV_IsIntPending(uint32_t instance,uint32_t channel);
28 **
29 ** Copyright : 1997 - 2015 Freescale Semiconductor, Inc.
30 ** All Rights Reserved.
31 **
32 ** Redistribution and use in source and binary forms, with or without modification,
33 ** are permitted provided that the following conditions are met:
34 **
35 ** o Redistributions of source code must retain the above copyright notice, this list
36 ** of conditions and the following disclaimer.
37 **
38 ** o Redistributions in binary form must reproduce the above copyright notice, this
39 ** list of conditions and the following disclaimer in the documentation and/or
40 ** other materials provided with the distribution.
41 **
42 ** o Neither the name of Freescale Semiconductor, Inc. nor the names of its
43 ** contributors may be used to endorse or promote products derived from this
44 ** software without specific prior written permission.
45 **
46 ** THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS" AND
47 ** ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED
48 ** WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE
49 ** DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT HOLDER OR CONTRIBUTORS BE LIABLE FOR
50 ** ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES
51 ** (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES;
52 ** LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON
53 ** ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
54 ** (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
55 ** SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
56 **
57 ** http: www.freescale.com
58 ** mail: support@freescale.com
59 ** ###################################################################*/
60 /*!
61 ** @file BMTIMER1.h
62 ** @version 01.00
63 */
64 /*!
65 ** @addtogroup BMTIMER1_module BMTIMER1 module documentation
66 ** @{
67 */
68 #ifndef __BMTIMER1_H
69 #define __BMTIMER1_H
70 /* MODULE BMTIMER1. */
71
72 /* Include inherited beans */
73 #include "clockMan1.h"
74 #include "Cpu.h"
75
76 /*! @brief Device instance number */
77 #define FSL_BMTIMER1 0
78 /*! @brief PIT timer channel */
79 #define FSL_BMTIMER1_CHANNEL 0
80
81 /*! @brief PIT configuration declaration */
82 extern const pit_user_config_t BMTIMER1_InitConfig0;
83
84
85 #endif
86 /* ifndef __BMTIMER1_H */
87 /*!
88 ** @}
89 */
90 /*
91 ** ###################################################################
92 **
93 ** This file was created by Processor Expert 10.5 [05.21]
94 ** for the Freescale Kinetis series of microcontrollers.
95 **
96 ** ###################################################################
97 */
Cpu.h
clockMan1.h
BMTIMER1_InitConfig0
const pit_user_config_t BMTIMER1_InitConfig0
PIT configuration declaration.
Definition: BMTIMER1.c:57
- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.