| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

isf_user_config.h
Go to the documentation of this file.
1 /**
2 * @file isf_user_config.h
3 * @brief The \b isf_user_config.h file contains the user configurable settings to either include or
4 * exclude an ISF component.
5 *
6 * @copyright Copyright (c) 2015, Freescale Semiconductor, Inc.
7 */
8
9 #ifndef ISF_USER_CONFIG_H_
10 #define ISF_USER_CONFIG_H_
11
12 /*!
13 * @brief When ISF_COMPONENT_SM is defined as 1, the Sensor Manager component
14 * is linked to the user application.
15 */
16
17 /*!
18 * @brief When ISF_COMPONENT_CI is defined as 1, the Command Interpreter component
19 * is linked to the user application.
20 */
21 #ifndef ISF_COMPONENT_CI
22 #define ISF_COMPONENT_CI (1)
23 #endif
24
25
26
27 /*!
28 * @brief When ISF_COMPONENT_BM is defined as 1, the Bus Mangement component
29 * code is compiled.
30 * <br>\b Note: The component must be recompiled when this setting is changed.
31 */
32 #ifndef ISF_COMPONENT_BM
33 #define ISF_COMPONENT_BM (1)
34 #endif
35
36
37
38 /*!
39 * @brief When defined as 1, the Power Management component\n
40 * code will compiled. The component must be recompiled when
41 * this setting is changed.
42 */
43 #ifndef ISF_COMPONENT_PM
44 #define ISF_COMPONENT_PM (0)
45 #endif
46
47
48
49 #endif /* ISF_USER_CONFIG_H_ */
50
- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.