| ISF 2.2 rev 5 Intelligent Sensing Framework for Kinetis with Processor Expert

- Main Page
- Modules
- Data Structures
- Files

- File List
- Globals

Data Structures | Typedefs
isf_temperature_types.h File Reference

The isf_temperature_fixed_t.h file contains the ISF data type definitions for use with the ISF generic temperature fixed and floating point interface. More...

`#include <isf_sensor_base_types.h>`
Include dependency graph for isf_temperature_types.h:
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Data Structures
struct | isf_DegreesCelsius1D_EngFixed_t
| Standard fixed type for single axis pressure sensor. More...
struct | isf_DegreesCelsius1D_float_t
| Standard floating point type for single axis temperature sensor. More...

## Typedefs
typedef int32 | isf_temperature_degC_fixed_32s1i16_t
| ISF sensors standard fixed point temperature in degrees Celsius using AC_Fixed(32,16,1) notation This means of 32 total bits, 16 are used to represent the fractional portion and the MSB is used as a sign bit. the LSB is therefore ~1.5259E-05 degC. The type can contain pressures in the +/- 32768 degC range. More...
typedef float | isf_temperature_degC_float_t
| ISF sensors standard floating point temperature in degC. More...

## Detailed Description

The isf_temperature_fixed_t.h file contains the ISF data type definitions for use with the ISF generic temperature fixed and floating point interface.

Copyright
  Copyright (c) 2015, Freescale Semiconductor, Inc.

Definition in file isf_temperature_types.h.

## Typedef Documentation

typedef int32 isf_temperature_degC_fixed_32s1i16_t

ISF sensors standard fixed point temperature in degrees Celsius using AC_Fixed(32,16,1) notation This means of 32 total bits, 16 are used to represent the fractional portion and the MSB is used as a sign bit. the LSB is therefore ~1.5259E-05 degC. The type can contain pressures in the +/- 32768 degC range.

Definition at line 22 of file isf_temperature_types.h.

typedef float isf_temperature_degC_float_t

ISF sensors standard floating point temperature in degC.

Definition at line 32 of file isf_temperature_types.h.

- © Freescale Semiconductor, Inc. 2016. All Rights Reserved.