         ________________________________________________________  
        |                                                        | 
        |  =====            PHILIPS SEMICONDUCTEURS              | 
        | | P   |                                                | 
        | |  S  |             2 Rue de la Girafe                 | 
        | |   C |                  BP 5120                       | 
        |  =====             14079 CAEN CEDEX 5                  | 
        |                                                        | 
        |________________________________________________________| 
 
 
        BOARD       : PCB1648   IND : 1.0      STUDY : PN531_USB                 
 
        PROJECT     : TAMA                     DATE  : 21/10/2005           
 
        DESIGNED BY : ducastel                                
 
 
                   ***  COMPONENTS APPROVISIONNING  ***
    
    



  COUNT        GEOMETRY                              VALUE_SPECIFICATION                                      

    1                        Printed_Circuit_Board_PCB1648-1                                                     
    3        tpboucle1.0     5001, KEYSTONE:Black,Testpoint,Type1                                                
    1      5108_2x14s_0.8md  5108_1_02810_00, WP-PRODUCTS:5108,Serie,SMT,Connector,Straight,Male,2x14pins,0.8mm  
    1           bar2sp       Empr_CAVAL_2.54, Pattern,Single,Row,2,pin                                           
    6           bar2sp       CAVAL_2.54, Pattern,Single,Row,2,pin,+,ANTELEC,CCM1D                                
    7           c0402        0.1uF, Capacitor,CER2,0402,X7R,16V,-10+10%,PDC                                      
    2           c0402        18pF, Capacitor,CER2,0402,C0G,50V,5%                                                
    1           c0402        1nF, Capacitor,CER2,0402,X7R,50V,10%                                                
    2           c0402        220pF_C0G, Capacitor,CER2,0402,C0G,50V,GPR15_5C_1H_221                              
    2           c0402        22pF, Capacitor,CER2,0402,C0G,50V,5%                                                
    2           c0402        27pF, Capacitor,CER2,0402,C0G,50V,5%                                                
    2           c0402        56pF, Capacitor,CER2,0402,C0G,50V,5%                                                
    4           c0402        N.C., Capacitor,CER2,0402,***NOT,CONNECTED***                                       
    1           c0603        10uF, Capacitor,CER2,0603,X5R,4V,10%                                                
    1           c0603        1uF, Capacitor,CER2,0603,X5R,16V,10%                                                
    1           c0603        4.7uF, Capacitor,CER2,0603,X5R,6.3V,10%                                             
    3         chevron_a      CHEVRON, ***NOT,CONNECTED***                                                        
    2        self_mlf2012    0.56uH, TDK:MLF2012DR56K,Chip,Inductor,SMD,0.15A,10%                                
    6          plage.75      PLAGE.75, ***NOT,CONNECTED***                                                       
    2           r0402        0, Resistor,Package:0402,5%,1/16W                                                   
    1           r0402        1.5K, Resistor,Package:0402,5%,1/16W                                                
    1           r0402        100K, Resistor,Package:0402,5%,1/16W                                                
    1           r0402        1K, Resistor,Package:0402,5%,1/16W                                                  
    1           r0402        2.7K, Resistor,Package:0402,5%,1/16W                                                
    2           r0402        3.3_1%, Resistor,Package:0402,1%,1/16W                                              
    1           r0402        47K, Resistor,Package:0402,5%,1/16W                                                 
    1        mlf6x40_0.5     TAMA                                                                                
    1          tas3225       27.12MHZ, TOKYO-DENPA:TAS-3225A,Type,Quartz,Crystal,SMD                             
    5           tp0.9        CAVAL_2.54, Pattern,Single,Row,1,pin,+,ANTELEC,CCM1D                                
    4           tp0.9        Empr_CAVAL_2.54, Pattern,Single,Row,1,pin                                           
    1           usb_b        67068_0000, MOLEX:USB,Type,B,Receptacle                                             
    1             xe         4MHZ, TAITIEN:XE,Type,Quartz,Crystal,SMD                                            
