
         ________________________________________________________
        |                                                        |
        |  =====           PHILIPS SEMICONDUCTEURS               |
        | | P   |                                                |
        | |  S  |             2 Rue de la Girafe                 |
        | |   C |                  BP 5120                       |
        |  =====             14079 CAEN CEDEX 5                  |
        |                                                        |
        |________________________________________________________|


        BOARD       : PCB1648   IND : 1.0     STUDY : PN531_USB

        PROJECT     : TAMA           DATE  : 21 Octobre 2005

        DESIGNED BY : ducastel

                                                                          
                       ***  COMPONENTS LISTE  ***                         


REFERENCE    GEOMETRY          VALUE                       SPECIFICATION          
---------    --------          -----                       -------------   


  C1         c0402           N.C.                 Capacitor,CER2,0402,***NOT,CONNECTED***
  C2         c0402           18pF                 Capacitor,CER2,0402,C0G,50V,5%
  C3         c0402           N.C.                 Capacitor,CER2,0402,***NOT,CONNECTED***
  C4         c0402           56pF                 Capacitor,CER2,0402,C0G,50V,5%
  C5         c0402           220pF_C0G            Capacitor,CER2,0402,C0G,50V,GPR15_5C_1H_221
  C6         c0402           N.C.                 Capacitor,CER2,0402,***NOT,CONNECTED***
  C7         c0402           56pF                 Capacitor,CER2,0402,C0G,50V,5%
  C8         c0402           220pF_C0G            Capacitor,CER2,0402,C0G,50V,GPR15_5C_1H_221
  C9         c0402           18pF                 Capacitor,CER2,0402,C0G,50V,5%
  C10        c0402           N.C.                 Capacitor,CER2,0402,***NOT,CONNECTED***
  C11        c0402           1nF                  Capacitor,CER2,0402,X7R,50V,10%
  C12        c0402           22pF                 Capacitor,CER2,0402,C0G,50V,5%
  C13        c0402           22pF                 Capacitor,CER2,0402,C0G,50V,5%
  C14        c0402           27pF                 Capacitor,CER2,0402,C0G,50V,5%
  C15        c0402           27pF                 Capacitor,CER2,0402,C0G,50V,5%
  C16        c0603           1uF                  Capacitor,CER2,0603,X5R,16V,10%
  C17        c0402           0.1uF                Capacitor,CER2,0402,X7R,16V,-10+10%,PDC
  C18        c0603           10uF                 Capacitor,CER2,0603,X5R,4V,10%
  C19        c0402           0.1uF                Capacitor,CER2,0402,X7R,16V,-10+10%,PDC
  C20        c0603           4.7uF                Capacitor,CER2,0603,X5R,6.3V,10%
  C21        c0402           0.1uF                Capacitor,CER2,0402,X7R,16V,-10+10%,PDC
  C22        c0402           0.1uF                Capacitor,CER2,0402,X7R,16V,-10+10%,PDC
  C23        c0402           0.1uF                Capacitor,CER2,0402,X7R,16V,-10+10%,PDC
  C24        c0402           0.1uF                Capacitor,CER2,0402,X7R,16V,-10+10%,PDC
  C25        c0402           0.1uF                Capacitor,CER2,0402,X7R,16V,-10+10%,PDC
  IC1        mlf6x40_0.5     TAMA                 tama
  J1         5108_2x14s_0.8md 5108_1_02810_00      WP-PRODUCTS:5108,Serie,SMT,Connector,Straight,Male,2x14pins,0.8mm
  J2         usb_b           67068_0000           MOLEX:USB,Type,B,Receptacle
  L1         self_mlf2012    0.56uH               TDK:MLF2012DR56K,Chip,Inductor,SMD,0.15A,10%
  L2         self_mlf2012    0.56uH               TDK:MLF2012DR56K,Chip,Inductor,SMD,0.15A,10%
  R1         r0402           3.3_1%               Resistor,Package:0402,1%,1/16W
  R2         r0402           3.3_1%               Resistor,Package:0402,1%,1/16W
  R3         r0402           100K                 Resistor,Package:0402,5%,1/16W
  R4         r0402           2.7K                 Resistor,Package:0402,5%,1/16W
  R5         r0402           1.5K                 Resistor,Package:0402,5%,1/16W
  R6         r0402           47K                  Resistor,Package:0402,5%,1/16W
  R7         r0402           0                    Resistor,Package:0402,5%,1/16W
  R8         r0402           0                    Resistor,Package:0402,5%,1/16W
  R9         r0402           1K                   Resistor,Package:0402,5%,1/16W
  ST2        chevron_a       CHEVRON              ***NOT,CONNECTED***
  ST4        chevron_a       CHEVRON              ***NOT,CONNECTED***
  ST10       chevron_a       CHEVRON              ***NOT,CONNECTED***
  TB1        bar2sp          CAVAL_2.54           Pattern,Single,Row,2,pin,+,ANTELEC,CCM1D
  TB2        bar2sp          Empr_CAVAL_2.54      Pattern,Single,Row,2,pin
  TB3        bar2sp          CAVAL_2.54           Pattern,Single,Row,2,pin,+,ANTELEC,CCM1D
  TB4        bar2sp          CAVAL_2.54           Pattern,Single,Row,2,pin,+,ANTELEC,CCM1D
  TB5        bar2sp          CAVAL_2.54           Pattern,Single,Row,2,pin,+,ANTELEC,CCM1D
  TB6        bar2sp          CAVAL_2.54           Pattern,Single,Row,2,pin,+,ANTELEC,CCM1D
  TB7        bar2sp          CAVAL_2.54           Pattern,Single,Row,2,pin,+,ANTELEC,CCM1D
  TB8        tp0.9           CAVAL_2.54           Pattern,Single,Row,1,pin,+,ANTELEC,CCM1D
  TB9        tp0.9           CAVAL_2.54           Pattern,Single,Row,1,pin,+,ANTELEC,CCM1D
  TB10       tp0.9           CAVAL_2.54           Pattern,Single,Row,1,pin,+,ANTELEC,CCM1D
  TB11       tp0.9           CAVAL_2.54           Pattern,Single,Row,1,pin,+,ANTELEC,CCM1D
  TB12       tp0.9           CAVAL_2.54           Pattern,Single,Row,1,pin,+,ANTELEC,CCM1D
  TB13       tp0.9           Empr_CAVAL_2.54      Pattern,Single,Row,1,pin
  TB14       tp0.9           Empr_CAVAL_2.54      Pattern,Single,Row,1,pin
  TB15       tp0.9           Empr_CAVAL_2.54      Pattern,Single,Row,1,pin
  TB16       tp0.9           Empr_CAVAL_2.54      Pattern,Single,Row,1,pin
  TP1        plage.75        PLAGE.75             ***NOT,CONNECTED***
  TP2        plage.75        PLAGE.75             ***NOT,CONNECTED***
  TP3        plage.75        PLAGE.75             ***NOT,CONNECTED***
  TP4        plage.75        PLAGE.75             ***NOT,CONNECTED***
  TP5        plage.75        PLAGE.75             ***NOT,CONNECTED***
  TP6        plage.75        PLAGE.75             ***NOT,CONNECTED***
  TP7        tpboucle1.0     5001                 KEYSTONE:Black,Testpoint,Type1
  TP8        tpboucle1.0     5001                 KEYSTONE:Black,Testpoint,Type1
  TP9        tpboucle1.0     5001                 KEYSTONE:Black,Testpoint,Type1
  Y1         tas3225         27.12MHZ             TOKYO-DENPA:TAS-3225A,Type,Quartz,Crystal,SMD
  Y2         xe              4MHZ                 TAITIEN:XE,Type,Quartz,Crystal,SMD
